Quick Navigation
| Background
| System Summary
| Motherboard
| Processor
| BIOS
| PCI/AGP Devices
| Memory Modules
| Memory (SMBIOS)
| HDD
| ATAPI
| Storage (ASPI)
| Logical Drives
| USB Devices
| Printers
| Slots (SMBIOS)
| Ports (SMBIOS)
| Network
| Monitor
| Video
| Hardware Monitoring
| Diagnostics
| Software
Background
| Background
| Version | ASTRA32 v.3.30
| URL | www.astra32.com
| Network Name | A2KKV
| User Name | kkv1
| Report Date | April 28, 2015
| Report Time | 21:59:40
| OS Version | MS Windows 7 Ultimate x64 Edition (6.1.7601 Service Pack 1)
| Registered To | Sysinfo Lab
| License Type | Professional for 1 computer
System Summary
| Processor
| Processor | Intel Core i3-4160 3600 MHz
| CPU Clock | 3591.7 MHz (36.0 x 99.8 MHz)
| Level 1 Cache | 2 x 32 kB + 2 x 32 kB (data+instr.)
| Level 2 Cache | 2 x 256 kB
| Level 3 Cache | 1 x 3 MB
| Motherboard
| System Name | Gigabyte Technology Co., Ltd. H81M-S2PV
| Board Model | Gigabyte Technology Co., Ltd. H81M-S2PV
| BIOS Version | AMI BIOS 08.00.10
| Chipset Name | Intel H81 (Lynx Point)
| Chipset Vendor | Intel Corporation
| Chipset | 4th Gen Core Processor DRAM Controller
| Southbridge Vendor | Intel Corporation
| Southbridge | H81 Chipset LPC Controller
| DMI/SMBIOS Version | 2.7
| Memory
| Memory Size | 3.9 GB
| System Memory | 4042 MB
| Memory Module | 2048MB DDR3-1333 (PC3-10600) SDRAM (Kingston)
| Memory Module | 2048MB DDR3-1333 (PC3-10600) SDRAM (Kingston)
| Storage
| HDD Model | SSD Smartbuy 60GB
| HDD Size | 57241 MB (55.90 GB)
| HDD Model | WDC WD1001FALS-00J7B0
| HDD Size | 953869 MB (931.51 GB)
| Video
| Monitor Vendor | LG Electronics Inc.
| Monitor Model | LG FLATRON F920P
| Video Chip Vendor | ATI Technologies Inc
| Video Chip | Pitcairn PRO [Radeon HD 7800 Series]
| Video Memory Size | 2 GB
| Sound
| Sound Chip Vendor | Intel Corporation
| Sound Chip | 8 Series/C220 Series Chipset Family HD Audio Controller
| Sound Chip Vendor | ATI Technologies Inc
| Sound Chip | Cape Verde/Pitcairn HDMI Audio [Radeon HD 7700/7800 Series]
| AC'97/HDA Codec Name | ATI R6xx HDMI
| Sound Chip Vendor | Creative Labs
| Sound Chip | EMU10K2 Audio Chipset (SB Audigy Series)
| Operating System
| Operating System | MS Windows 7 Ultimate x64 Edition (6.1.7601 Service Pack 1)
| Windows Folder | G:\Windows
| Modem
| Modem Vendor | Intel Corporation
| Modem Model | 8 Series/C220 Series Chipset Family MEI Controller #1
| Network
| Network Name | A2KKV
| Interface Description | TAP-Windows Adapter V9
| MAC Address | 00-FF-CA-D1-AF-0D
| Adapter Vendor | Realtek Semiconductor
| Adapter Name | RTL8111/8168/8411 PCI Express Gigabit Ethernet Controller
| Interface Description | Realtek PCIe GBE Family Controller
| MAC Address | 74-D4-35-CD-93-A8
| Ports
| LPT Ports | None
| COM Ports | None
Motherboard
| System
| System Vendor | Gigabyte Technology Co., Ltd.
| Product Name | H81M-S2PV
| Version | To be filled by O.E.M.
| Serial Number | To be filled by O.E.M.
| UUID | 7402D4033504CD059306A80700080009
| Wake-up Type | Power Switch
| SKU Number | To be filled by O.E.M.
| Family | To be filled by O.E.M.
| Motherboard
| Motherboard Vendor | Unknown (0001)
| Vendor URL | Unknown
| Board Model | Gigabyte Technology Co., Ltd. H81M-S2PV
| Version | x.x
| Serial Number | To be filled by O.E.M.
| BIOS Version | AMI BIOS 08.00.10
| BIOS Date | 04/13/12
| Chipset Name | Intel H81 (Lynx Point)
| Chipset Vendor | Intel Corporation
| Chipset | 4th Gen Core Processor DRAM Controller
| Southbridge Vendor | Intel Corporation
| Southbridge | H81 Chipset LPC Controller
| Onboard Device 1
| Description | To Be Filled By O.E.M.
| Device Type | Video
| Status | Enabled
| Configuration Options
| To Be Filled By O.E.M.
| System Enclosure
| Manufacturer | Gigabyte Technology Co., Ltd.
| Type | Desktop
| Version | To Be Filled By O.E.M.
| Serial Number | To Be Filled By O.E.M.
| Asset Tag | To Be Filled By O.E.M.
| Boot-up State | Safe
| Power Supply State | Safe
| Thermal State | Safe
| Security Status | None
| OEM-defined | 00000000h
| Height | 0.0 sm
| Power Cords | 1
| Contained Element | 0
CPU
| CPU
| Processor | Intel Core i3-4160 3600 MHz
| Coprocessor | Internal
| CPU Clock | 3591.7 MHz
| Level 1 Cache | 2 x 32 kB + 2 x 32 kB (data+instr.)
| Level 2 Cache | 2 x 256 kB
| Level 3 Cache | 1 x 3 MB
| Code Name | Haswell-DT
| Manufacturing Process | 22 nm
| FSB Clock | 99.8 MHz
| Multiplier | 36.0
| Expected Clock | 3600 MHz
| Socket Type | Socket 1150 FCLGA
| Package Temperature | 38 °C (100 °F)
| Temperature Core 1 | 36 °C (97 °F)
| Temperature Core 2 | 38 °C (100 °F)
| Tjmax Temperature | 100 °C (212 °F)
| Core Voltage | 1.175 V
| Vendor | GenuineIntel
| Processor Name | Intel(R) Core(TM) i3-4160 CPU @ 3.60GHz
| Processor Type | Original OEM Processor
| CPUID | Family: 6, Model: 12, Stepping: 3
| Ext. Family/Model | Family: -, Model: 3
| CPU Signature | 000306C3h
| Brand ID | Not Supported
| Number of Cores | 2
| Logical CPU Count | 4
| Core Stepping | C-0
| Max TDP | 54 Wattes
| Transistor Count | 1400 million
| Die Size | 177 mm2
| Family Frequency Range | 3.4-3.7 GHz
| Family Release Date | September, 2013
| Max CPUID Level | 13
| Max ExtCPUID Level | 80000008h
| Instruction Set
| Floating-Point Unit On-Chip | Supported
| IA MMX Technology | Supported
| SSE Instruction Set | Supported
| SSE2 Instruction Set | Supported
| SSE3 Instruction Set | Supported
| Supplemental SSE3 Instruction Set | Supported
| SSE4.1 Instruction Set | Supported
| SSE4.2 Instruction Set | Supported
| Advanced Vector Extensions (AVX) | Supported
| Advanced Vector Extensions 2 (AVX2) | Supported
| AVX-512 Foundation Instructions | Not Supported
| AVX-512 Prefetch Instructions | Not Supported
| AVX-512 Exponential and Reciprocal | Not Supported
| AVX-512 Conflict Detection | Not Supported
| AVX-512 Byte and Word Instructions | Not Supported
| AVX-512 Doubleword and Quadword | Not Supported
| AVX-512 Vector Length Extensions | Not Supported
| AVX-512 Integer Fused Multiply-Add | Not Supported
| AVX-512 Vector Bit Manipulation | Not Supported
| PCOMMIT Instruction | Not Supported
| CLWB Instruction | Not Supported
| PREFETCHWT1 Instruction | Not Supported
| Software Guard Extensions (SGX) | Not Supported
| FMA Instructions Set | Supported
| AES Instructions Set | Supported
| Intel Extended Memory 64 Tech. | Supported
| Intel Architecture - 64 (IA-64) | Not Supported
| AMD MMX Instruction Extensions | Not Supported
| AMD 3DNow! Instructions | Not Supported
| AMD 3DNow! Extensions | Not Supported
| AMD 3DNow! Prefetch | Not Supported
| AMD SSE4A Extensions | Not Supported
| AMD eXtended OPeration (XOP) | Not Supported
| AMD Misaligned SSE | Not Supported
| AMD64 Architecture | Not Supported
| Cyrix Extended MMX | Not Supported
| CMPXCHG8 Instruction Supported | Supported
| CMPXCHG16 Instruction Supported | Supported
| Fast System Call | Supported
| Conditional Move Instruction | Supported
| CLFLUSH Insruction Supported | Supported
| Fast Save and Restore | Supported
| Monitor/MWAIT Instructions | Supported
| SYSCALL/SYSRET Instructions | Not Supported
| LAHF/SAHF Instructions | Supported
| POPCNT Insruction Supported | Supported
| XSAVE Insructions Supported | Supported
| OS Supports XSAVE Instructions | Supported
| PCLMULQDQ Instruction Supported | Supported
| MOVBE Insruction Supported | Supported
| F16C Insruction Supported | Supported
| RDTSCP Insruction Supported | Supported
| RDRAND Insruction Supported | Supported
| (RD/WR)(FS/GS) BASE Instructions | Supported
| Bit Manipulation 1 Instructions | Supported
| Bit Manipulation 1 Instructions | Supported
| Enhanced REP MOVSB/STOSB | Supported
| INVPCID Instruction | Supported
| XSAVEOPT Instruction | Supported
| RDSEED Instruction | Not Supported
| ADCX/ADOX Instructions | Not Supported
| CLAC/STAC Instructions | Not Supported
| SCLFLUSHOPT Instruction | Not Supported
| AMD Fast Save and Restore | Not Supported
| AMD SKINIT, STGI, DEV Supported | Not Supported
| AMD Light Weight Profiling (LWP) | Not Supported
| AMD FMA4 Insruction Supported | Not Supported
| AMD TBM Insruction Supported | Not Supported
| Processor Features
| Virtual Mode Extension | Supported
| Debugging Extension | Supported
| Page Size Extension | Supported
| Time Stamp Counter | Supported
| Model Specific Registers | Supported
| Physical Address Extension | Supported
| Machine Check Exception | Supported
| On-chip APIC Hardware Supported | Supported
| Memory Type Range Registers | Supported
| Page Global Enable | Supported
| Machine Check Architecture | Supported
| Page Attribute Table | Supported
| 36-bit Page Size Extension | Supported
| Processor Serial Number | Not Supported
| Debug Store | Supported
| 64-bit Debug Store | Supported
| Self-Snoop | Supported
| Hyper-Threading Technology | Supported
| Pending Break Enable | Supported
| CPL-Qualified Debug Store | Supported
| L1 Context ID | Not Supported
| Send Task Priority Messages | Supported
| Direct Cache Access | Not Supported
| Performance Capabilities MSR | Supported
| x2APIC Architecture | Not Supported
| Advanced Bit Manipulation | Supported
| OS Visible Workaround | Not Supported
| Instruction Based Sampling | Not Supported
| 1-GB Large Page | Supported
| Process Context Identifiers | Supported
| Time Stamp Counter Deadline | Supported
| Time Stamp Counter Adjust | Supported
| Intel Virtualization Technology | Supported
| Intel Trusted Execution Technology | Not Supported
| Supervisor Mode Execution Protection | Supported
| Hardware Lock Elision | Not Supported
| Restricted Transactional Memory | Not Supported
| Quality of Service Monitoring | Not Supported
| Quality of Service Enforcement | Not Supported
| Deprecated FPU CS and FPU DS | Supported
| Memory Protection Extensions (MPX) | Not Supported
| Processor Trace (PT) | Not Supported
| Secure Hash Algorithm Ext. (SHA) | Not Supported
| Debug Interface MSR | Supported
| Intel Turbo Boost Technology | Not Supported
| Intel Execute Disable Bit | Supported
| AMD Secure Virtual Machine | Not Supported
| AMD Model-Specific Registers | Not Supported
| AMD Multiprocessing Capable | Not Supported
| AMD CMP Legacy Mode | Not Supported
| AMD CR8 in Legacy Mode | Not Supported
| AMD Ext. APIC Register Space | Not Supported
| AMD Watchdog Timer | Not Supported
| AMD Translation Cache Extension | Not Supported
| AMD Topology Extensions | Not Supported
| AMD Core Performance Counter Ext. | Not Supported
| AMD NB Performance Counter Ext. | Not Supported
| AMD Streaming Performance Monitor | Not Supported
| AMD Data Breakpoint Extension | Not Supported
| AMD Performance TSC | Not Supported
| AMD L2I Performance Counter Ext. | Not Supported
| Power Management
| ACPI Supported | Supported
| Thermal Monitor Supported | Supported
| Thermal Monitor 2 | Supported
| Enhanced SpeedStep Technology | Supported
| Digital Thermal Sensor | Supported
| Always Running APIC Timer | Supported
| Invariant TSC | Supported
| Power Limit Notification | Supported
| Extended Clock Modulation Duty | Supported
| Package Thermal Management | Supported
| Hardware Coordination Feedback | Supported
| ACNT2 Capability | Not Supported
| Performance-Energy Bias | Not Supported
| AMD Temperature Sensor | Not Supported
| AMD Frequency ID Control | Not Supported
| AMD Voltage ID Control | Not Supported
| AMD Thermal Trip | Not Supported
| AMD Thermal Monitoring | Not Supported
| AMD Software Thermal Control | Not Supported
| AMD 100MHz Multiplier Steps | Not Supported
| AMD Hardware P-State Control | Not Supported
| AMD Effective Frequency Interface | Not Supported
| AMD Processor Feedback Interface | Not Supported
| AMD Processor Accumulator | Not Supported
CPU Cache
| Level 1 Instruction Cache
| Size | 2 x 32 kB
| Associativity | 8-way
| Line Size | 64 byte
| TLB 4K Pages |
| Number of Entries | 64
| Associativity | 8-way
| TLB 2/4M Pages |
| Number of Entries | 8
| Associativity | full
| Level 1 Data Cache
| Size | 2 x 32 kB
| Associativity | 8-way
| Line Size | 64 byte
| TLB 4K Pages |
| Number of Entries | 64
| Associativity | 4-way
| TLB 2/4M Pages |
| Number of Entries | 4
| Associativity | 4-way
| Level 2 Cache
| Size | 2 x 256 kB
| Associativity | 8-way
| Line Size | 64 byte
| Level 3 Cache
| Size | 1 x 3 MB
| Associativity | 12-way
| Line Size | 64 byte
CPU (SMBIOS)
| Processor
| Processor Vendor | Intel
| Processor Version | Intel(R) Core(TM) i3-4160 CPU @ 3.60GHz
| Current Speed | 3600 MHz
| External Clock | 100 MHz
| Voltage | 1.1 V
| Processor Upgrade | Other
| Processor Status | CPU Enabled
| Socket Designation | SOCKET 0
| Processor Type | Central Processor
| Processor Family | Intel Core i7
| Processor ID1 | 000306C3h
| Processor ID2 | BFEBFBFFh
| Max Speed | 7000 MHz
| Socket Status | CPU Socket Populated
| Serial Number |
| Asset Tag | Fill By OEM
| Part Number | Fill By OEM
| CPU Core Count | 2 (Enabled: 1)
| CPU Thread Count | 2
| Structure Length | 2Ah
CPU (SMBIOS) Cache
| Level 1 Cache
| Installed Size | 128 kB
| Operational Mode | Write Back
| Current SRAM Type | Unknown
| Status | Enabled
| Socket Designation | CPU Internal L1
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 128 kB
| Supported SRAM Type | Unknown
| Cache Speed | Unknown
| Error Correction | Single-bit ECC
| System Cache Type | Other
| Associativity | 8-way Set-Associative
| Structure Length | 13h
| Level 2 Cache
| Installed Size | 512 kB
| Operational Mode | Write Back
| Current SRAM Type | Unknown
| Status | Enabled
| Socket Designation | CPU Internal L2
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 512 kB
| Supported SRAM Type | Unknown
| Cache Speed | Unknown
| Error Correction | Single-bit ECC
| System Cache Type | Unified
| Associativity | 8-way Set-Associative
| Structure Length | 13h
| Level 3 Cache
| Installed Size | 3072 kB
| Operational Mode | Write Back
| Current SRAM Type | Unknown
| Status | Enabled
| Socket Designation | CPU Internal L3
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 3072 kB
| Supported SRAM Type | Unknown
| Cache Speed | Unknown
| Error Correction | Single-bit ECC
| System Cache Type | Unified
| Associativity | 12-way Set-Associative
| Structure Length | 13h
BIOS
| BIOS
| Motherboard Vendor | Unknown (0001)
| Vendor URL | Unknown
| BIOS Version | AMI BIOS 08.00.10
| BIOS Date | 04/13/12
| BIOS Copyright | 04/13/12(C)2010 American Megatrends, Inc. All Rights Reserved
| Motherboard ID | BIOS Date: 06/19/14 23:14:41 Ver: 04.06.05
| BIOS ID | 63-0100-000001-00101111-041312-Chipset
| BIOS Size | 512 kB
| Processor | 686
| Chipset ID | Chipset
| BIOS Revision | 0100
| MP Specification Ver. | 1.4
| MP Table Address | 000Fh:D450h
| Number of CPU/Cores | 2
| DMI/SMBIOS Version | 2.7
| DMI/SMBIOS Structures | 76
| DMI/SMBIOS Address | 000Eh:C070h
| SMBIOS
| BIOS Vendor | American Megatrends Inc.
| BIOS Version | F8
| BIOS Date | 06/19/2014
| BIOS ROM Size | 8192 kB
| System BIOS Version | 4.6
| Starting Segment | F000h
| Current Language | en|US|iso8859-1
| Number of Languages | 7
| Structure Length | 18h
| Bus Supported
| PCI is Supported | Supported
| AGP is Supported | Not Supported
| USB is Supported | Supported
| ISA is Supported | Not Supported
| VLBus is Supported | Not Supported
| MCA is Supported | Not Supported
| EISA is Supported | Not Supported
| PC Card is Supported | Not Supported
| Boot Options
| Selectable Boot | Supported
| Boot From CD | Supported
| ATAPI ZIP Drive Boot | Not Supported
| LS-120 Boot | Not Supported
| BIOS Boot Specification | Supported
| Boot From PC Card | Not Supported
| Network Service Boot Supported | Not Supported
| I2O Boot | Not Supported
| 1394 Boot | Not Supported
| BIOS Features
| BIOS Characteristics | Supported
| ACPI Supported | Supported
| PnP is Supported | Not Supported
| APM is Supported | Not Supported
| ESCD Support | Not Supported
| Enhanced Disk Drive (EDD) | Supported
| BIOS is Upgradeable (Flash) | Supported
| BIOS ROM is Socketed | Supported
| BIOS Shadowing is Allowed | Supported
| Smart Battery Supported | Not Supported
| Targeted Content Distribution | Supported
| UEFI Specification is Supported | Supported
| Virtual Machine | Not Supported
| Int 13h - 5.25"/360kB Floppy | Not Supported
| Int 13h - 5.25"/1.2MB Floppy | Supported
| Int 13h - 3.5"/720kB Floppy | Supported
| Int 13h - 3.5"/2.88MB Floppy | Supported
| Int 5h, Print Screen Service | Supported
| Int 9h, 8042 Keyboard Services | Supported
| Int 14h, Serial Services | Supported
| Int 17h, Printer Services | Supported
| Int 10h, CGA/Mono Video Services | Not Supported
| Int 13h - Floppy for NEC 9800 | Not Supported
| Int 13h - Floppy for Toshiba | Not Supported
| NEC PC-98 | Not Supported
| OEM SMBIOS Strings
| To Be Filled By O.E.M.
| To Be Filled By O.E.M.
| To Be Filled By O.E.M.
| To Be Filled By O.E.M.
| To Be Filled By O.E.M.
| Other SMBIOS Structures
| System Boot Information (32)
| Management Device (34)
| Voltage Probe (26)
| Management Device Threshold Data (36)
| Management Device Component (35)
| Temperature Probe (28)
| Management Device Threshold Data (36)
| Management Device Component (35)
| Cooling Device (27)
| Management Device Threshold Data (36)
| Management Device Component (35)
| Cooling Device (27)
| Management Device Threshold Data (36)
| Management Device Component (35)
| Electrical Current Probe (29)
| Management Device Threshold Data (36)
| Management Device Component (35)
| Voltage Probe (26)
| Temperature Probe (28)
| Cooling Device (27)
| Electrical Current Probe (29)
| System Power Supply (39)
| Unknown (41)
| Memory Device Mapped Address (20)
| Memory Device Mapped Address (20)
| Memory Array Mapped Address (19)
| Unknown (136)
| Unknown (131)
PCI/AGP Devices
| Bus: 00h, Device: 00h, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (0C00h) | 4th Gen Core Processor DRAM Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5000h) | Unknown
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 06h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | Intel(R) 4th Gen Core processor DRAM Controller - 0C00
| Device Class | System
| Device Location | PCI bus 0, device 0, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Hardware ID | PCI\VEN_8086&DEV_0C00&SUBSYS_50001458&REV_06
| Compatible ID | PCI\VEN_8086&DEV_0C00&REV_06
| Bus: 00h, Device: 01h, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (0C01h) | 4th Gen Core/Xeon E3-1200 v3 Processor PCI Express x16 Controller
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | 06h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | E000h - EFFFh
| Memory Address | F7E00000h - F7EFFFFFh
| Memory Address | E0000000h - EFFFFFFFh
| System IRQ | 16
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 5.0 GB/s (Current: 2.5 GB/s)
| Link Width | x16 (Current: x16)
| Link Port Number | 2
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | PCI standard PCI-to-PCI bridge
| Device Class | System
| Device Location | PCI bus 0, device 1, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | pci
| Hardware ID | PCI\VEN_8086&DEV_0C01&SUBSYS_50001458&REV_06
| Compatible ID | PCI\VEN_8086&DEV_0C01&REV_06
| Bus: 00h, Device: 14h, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (8C31h) | 8 Series/C220 Series Chipset Family USB xHCI Host Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5007h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 05h
| Interface | 30h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | F7F00000h - F7F0FFFFh
| Driver
| Driver Status | The device is working properly
| Manufacturer | Intel(R) Corporation
| Device Description | Ðàñøèðÿåìûé õîñò-êîíòðîëëåð Intel(R) USB 3.0
| Device Class | USB
| Device Location | PCI bus 0, device 20, function 0
| Driver Provider | Intel(R) Corporation
| Driver Version | 3.0.2.54
| Driver Date | 10-30-2014
| Inf File | oem8.inf
| Service Name | iusb3xhc
| Hardware ID | PCI\VEN_8086&DEV_8C31&SUBSYS_50071458&REV_05
| Compatible ID | PCI\VEN_8086&DEV_8C31&REV_05
| Bus: 00h, Device: 16h, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (8C3Ah) | 8 Series/C220 Series Chipset Family MEI Controller #1
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (1C3Ah) | Unknown
| Class (07h) | Communication
| SubClass (80h) | Other
| Revision | 04h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | F7F1A000h - F7F1A00Fh
| System IRQ | 11
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is working properly
| Manufacturer | Intel
| Device Description | Intel(R) 8 Series/C220 Series Management Engine Interface - 8C3A
| Device Class | System
| Device Location | PCI bus 0, device 22, function 0
| Driver Provider | Intel
| Driver Version | 1.2.3.2005
| Driver Date | 1-2-2014
| Inf File | oem14.inf
| Hardware ID | PCI\VEN_8086&DEV_8C3A&SUBSYS_1C3A1458&REV_04
| Compatible ID | PCI\VEN_8086&DEV_8C3A&REV_04
| Bus: 00h, Device: 1Ah, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (8C2Dh) | 8 Series/C220 Series Chipset Family USB Enhanced Host Controller #2
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5006h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 05h
| Interface | 20h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | F7F18000h - F7F183FFh
| System IRQ | 16
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | Intel(R) 8 Series/C220 Series USB EHCI #2 - 8C2D
| Device Class | USB
| Device Location | PCI bus 0, device 26, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.18328
| Driver Date | 6-21-2006
| Inf File | usbport.inf
| Service Name | usbehci
| Hardware ID | PCI\VEN_8086&DEV_8C2D&SUBSYS_50061458&REV_05
| Compatible ID | PCI\VEN_8086&DEV_8C2D&REV_05
| Bus: 00h, Device: 1Bh, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (8C20h) | 8 Series/C220 Series Chipset Family HD Audio Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (A002h) | Unknown
| Class (04h) | Multimedia
| SubClass (03h) | Hi-definition Audio
| Revision | 05h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | F7F10000h - F7F13FFFh
| System IRQ | 22
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 1.0
| Device/Port Type | Root Complex Integrated Endpoint
| Link Speed | Unknown (0) (Current: Unknown (0))
| Link Width | x0 (Current: x0)
| Link Port Number | 0
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Microsoft
| Device Description | High Definition Audio Controller
| Device Class | System
| Device Location | PCI bus 0, device 27, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 11-19-2010
| Inf File | hdaudbus.inf
| Service Name | HDAudBus
| Hardware ID | PCI\VEN_8086&DEV_8C20&SUBSYS_A0021458&REV_05
| Compatible ID | PCI\VEN_8086&DEV_8C20&REV_05
| Bus: 00h, Device: 1Ch, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (8C10h) | 8 Series/C220 Series Chipset Family PCI Express Root Port 1
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | D5h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FFF00000h - 000FFFFFh
| System IRQ | 16
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 5.0 GB/s (Current: 2.5 GB/s)
| Link Width | x1 (Current: x0)
| Link Port Number | 1
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | Intel(R) 8 Series/C220 Series PCI Express Root Port #1 - 8C10
| Device Class | System
| Device Location | PCI bus 0, device 28, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | pci
| Hardware ID | PCI\VEN_8086&DEV_8C10&SUBSYS_50011458&REV_D5
| Compatible ID | PCI\VEN_8086&DEV_8C10&REV_D5
| Bus: 00h, Device: 1Ch, Function: 02h
| Vendor (8086h) | Intel Corporation
| Device (8C14h) | 8 Series/C220 Series Chipset Family PCI Express Root Port 3
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | D5h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | D000h - DFFFh
| Memory Address | F7D00000h - F7DFFFFFh
| Memory Address | F0000000h - F00FFFFFh
| System IRQ | 18
| Interrupt Pin | INTC#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 5.0 GB/s (Current: 2.5 GB/s)
| Link Width | x1 (Current: x1)
| Link Port Number | 3
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | Intel(R) 8 Series/C220 Series PCI Express Root Port #3 - 8C14
| Device Class | System
| Device Location | PCI bus 0, device 28, function 2
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | pci
| Hardware ID | PCI\VEN_8086&DEV_8C14&SUBSYS_50011458&REV_D5
| Compatible ID | PCI\VEN_8086&DEV_8C14&REV_D5
| Bus: 00h, Device: 1Ch, Function: 03h
| Vendor (8086h) | Intel Corporation
| Device (244Eh) | 82801FB Hub Interface to PCI Bridge (ICH6 C0 step)
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | D5h
| Interface | 01h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | C000h - CFFFh
| Memory Address | FFF00000h - 000FFFFFh
| System IRQ | 19
| Interrupt Pin | INTD#
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Root Port of PCI-E Root Complex
| Link Speed | 5.0 GB/s (Current: 2.5 GB/s)
| Link Width | x1 (Current: x1)
| Link Port Number | 4
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Intel
| Device Description | Intel(R) 82801 PCI Bridge - 244E
| Device Class | System
| Device Location | PCI bus 0, device 28, function 3
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | pci
| Hardware ID | PCI\VEN_8086&DEV_244E&SUBSYS_50011458&REV_D5
| Compatible ID | PCI\VEN_8086&DEV_244E&REV_D5
| Bus: 00h, Device: 1Dh, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (8C26h) | 8 Series/C220 Series Chipset Family USB Enhanced Host Controller #1
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5006h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 05h
| Interface | 20h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | F7F17000h - F7F173FFh
| System IRQ | 23
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | Intel(R) 8 Series/C220 Series USB EHCI #1 - 8C26
| Device Class | USB
| Device Location | PCI bus 0, device 29, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.18328
| Driver Date | 6-21-2006
| Inf File | usbport.inf
| Service Name | usbehci
| Hardware ID | PCI\VEN_8086&DEV_8C26&SUBSYS_50061458&REV_05
| Compatible ID | PCI\VEN_8086&DEV_8C26&REV_05
| Bus: 00h, Device: 1Fh, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (8C5Ch) | H81 Chipset LPC Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5001h) | Unknown
| Class (06h) | Bridge
| SubClass (01h) | PCI/ISA
| Revision | 05h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | Intel(R) H81 LPC Controller - 8C5C
| Device Class | System
| Device Location | PCI bus 0, device 31, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | msisadrv
| Hardware ID | PCI\VEN_8086&DEV_8C5C&SUBSYS_50011458&REV_05
| Compatible ID | PCI\VEN_8086&DEV_8C5C&REV_05
| Bus: 00h, Device: 1Fh, Function: 02h
| Vendor (8086h) | Intel Corporation
| Device (8C02h) | 8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (B005h) | Unknown
| Class (01h) | Storage
| SubClass (06h) | Serial ATA
| Revision | 05h
| Interface | 01h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Base I/O Port | 0000F070h - 0000F077h
| Base I/O Port | 0000F060h - 0000F063h
| Base I/O Port | 0000F050h - 0000F057h
| Base I/O Port | 0000F040h - 0000F043h
| Base I/O Port | 0000F020h - 0000F03Fh
| Memory Address | F7F16000h - F7F167FFh
| System IRQ | 19
| Interrupt Pin | INTB#
| Driver
| Driver Status | The device is working properly
| Manufacturer | Standard AHCI 1.0 Serial ATA Controller
| Device Description | Intel(R) 8 Series/C220 Series SATA AHCI Controller - 8C02
| Device Class | hdc
| Device Location | PCI bus 0, device 31, function 2
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.18231
| Driver Date | 6-21-2006
| Inf File | mshdc.inf
| Service Name | msahci
| Hardware ID | PCI\VEN_8086&DEV_8C02&SUBSYS_B0051458&REV_05
| Compatible ID | PCI\VEN_8086&DEV_8C02&REV_05
| Bus: 00h, Device: 1Fh, Function: 03h
| Vendor (8086h) | Intel Corporation
| Device (8C22h) | 8 Series/C220 Series Chipset Family SMBus Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5001h) | Unknown
| Class (0Ch) | Serial
| SubClass (05h) | SMBus Controller
| Revision | 05h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Not Supported
| I/O Access | Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| SMBus Port | F000h
| Memory Address | F7F15000h - F7F150FFh
| Base I/O Port | 0000F000h - 0000F01Fh
| System IRQ | 4
| Interrupt Pin | INTC#
| Driver
| Driver Status | The device is working properly
| Manufacturer | Intel
| Device Description | Intel(R) 8 Series/C220 Series SMBus Controller - 8C22
| Device Class | System
| Device Location | PCI bus 0, device 31, function 3
| Driver Provider | Intel
| Driver Version | 10.0.13.0
| Driver Date | 2-25-2014
| Inf File | oem2.inf
| Hardware ID | PCI\VEN_8086&DEV_8C22&SUBSYS_50011458&REV_05
| Compatible ID | PCI\VEN_8086&DEV_8C22&REV_05
| Bus: 01h, Device: 00h, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (6819h) | Pitcairn PRO [Radeon HD 7800 Series]
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (2553h) | Unknown
| Class (03h) | Display
| SubClass (00h) | VGA
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | E0000000h - EFFFFFFFh
| Memory Address | F7E00000h - F7E3FFFFh
| Base I/O Port | 0000E000h - 0000E0FFh
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 8.0 GB/s (Current: 2.5 GB/s)
| Link Width | x16 (Current: x16)
| Link Port Number | 0
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Advanced Micro Devices, Inc.
| Device Description | AMD Radeon HD 7800 Series
| Device Class | Display
| Device Location | PCI bus 1, device 0, function 0
| Driver Provider | Advanced Micro Devices, Inc.
| Driver Version | 14.501.1003.0
| Driver Date | 11-20-2014
| Inf File | oem15.inf
| Service Name | amdkmdap
| Hardware ID | PCI\VEN_1002&DEV_6819&SUBSYS_25531458&REV_00
| Compatible ID | PCI\VEN_1002&DEV_6819&REV_00
| Bus: 01h, Device: 00h, Function: 01h
| Vendor (1002h) | ATI Technologies Inc
| Device (AAB0h) | Cape Verde/Pitcairn HDMI Audio [Radeon HD 7700/7800 Series]
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (AAB0h) | Unknown
| Class (04h) | Multimedia
| SubClass (03h) | Hi-definition Audio
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | F7E60000h - F7E63FFFh
| System IRQ | 17
| Interrupt Pin | INTB#
| AC'97/HDA Capabilities
| AC'97/HDA Codec Name | ATI R6xx HDMI
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 8.0 GB/s (Current: 2.5 GB/s)
| Link Width | x16 (Current: x16)
| Link Port Number | 0
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Microsoft
| Device Description | High Definition Audio Controller
| Device Class | System
| Device Location | PCI bus 1, device 0, function 1
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 11-19-2010
| Inf File | hdaudbus.inf
| Service Name | HDAudBus
| Hardware ID | PCI\VEN_1002&DEV_AAB0&SUBSYS_AAB01458&REV_00
| Compatible ID | PCI\VEN_1002&DEV_AAB0&REV_00
| Bus: 03h, Device: 00h, Function: 00h
| Vendor (10ECh) | Realtek Semiconductor
| Device (8168h) | RTL8111/8168/8411 PCI Express Gigabit Ethernet Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (E000h) | GA-EP45-DS5 Motherboard
| Class (02h) | Network
| SubClass (00h) | Ethernet
| Revision | 06h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | 0000D000h - 0000D0FFh
| Memory Address | F7D00000h - F7D00FFFh
| Memory Address | F0000000h - F0003FFFh
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | PCI-E Endpoint
| Link Speed | 2.5 GB/s (Current: 2.5 GB/s)
| Link Width | x1 (Current: x1)
| Link Port Number | 0
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Realtek
| Device Description | Realtek PCIe GBE Family Controller
| Device Class | Net
| Device Location | PCI bus 3, device 0, function 0
| Driver Provider | Realtek
| Driver Version | 7.90.826.2014
| Driver Date | 8-26-2014
| Inf File | oem9.inf
| Service Name | RTL8167
| Hardware ID | PCI\VEN_10EC&DEV_8168&SUBSYS_E0001458&REV_06
| Compatible ID | PCI\VEN_10EC&DEV_8168&REV_06
| Bus: 04h, Device: 00h, Function: 00h
| Vendor (8086h) | Intel Corporation
| Device (244Eh) | 82801 Family (ICH2/3/4/5/6/7/8/9,63xxESB) Hub Interface to PCI Bridge
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | 41h
| Interface | 01h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | C000h - CFFFh
| Memory Address | FFF00000h - 000FFFFFh
| System IRQ | 19
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is working properly
| Manufacturer | Intel
| Device Description | Intel(R) 82801 PCI Bridge - 244E
| Device Class | System
| Device Location | PCI bus 4, device 0, function 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.17514
| Driver Date | 6-21-2006
| Inf File | machine.inf
| Service Name | pci
| Hardware ID | PCI\VEN_8086&DEV_244E&SUBSYS_88921458&REV_41
| Compatible ID | PCI\VEN_8086&DEV_244E&REV_41
| Bus: 05h, Device: 01h, Function: 00h
| Vendor (1102h) | Creative Labs
| Device (0004h) | EMU10K2 Audio Chipset (SB Audigy Series)
| Subsys Vendor (1102h) | Creative Labs
| Subsystem ID (2005h) | Unknown
| Class (04h) | Multimedia
| SubClass (01h) | Audio
| Revision | 04h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Not Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | 0000C000h - 0000C03Fh
| System IRQ | 16
| Interrupt Pin | INTA#
| Driver
| Driver Status | The device is working properly
| Manufacturer | Creative Technology, Ltd.
| Device Description | Creative Audigy Audio Processor (WDM)
| Friendly Name | Creative SB Audigy 2 ZS (WDM)
| Device Class | MEDIA
| Device Location | PCI bus 5, device 1, function 0
| Driver Provider | Creative
| Driver Version | 6.0.301.39
| Driver Date | 3-13-2014
| Inf File | oem11.inf
| Service Name | ctaud2k
| Hardware ID | PCI\VEN_1102&DEV_0004&SUBSYS_20051102&REV_04
| Compatible ID | PCI\VEN_1102&DEV_0004&REV_04
Memory Modules
| Memory Slot 1
| Memory Type | 2048MB DDR3-1333 (PC3-10600) SDRAM
| Manufacturer | Kingston
| Module Type | Unbuffered DIMM
| Number of Ranks/Banks | 1 Ranks, 8 Banks
| Module Attributes | Unbuffered
| Error Checking | None
| CAS# Latency | 9.0 (Cycle Time: 1.500ns/686MHz)
| CAS# Latency | 8.0 (Cycle Time: 1.371ns/610MHz)
| CAS# Latency | 7.0 (Cycle Time: 1.200ns/533MHz)
| CAS# Latency | 6.0 (Cycle Time: 1.029ns/457MHz)
| Refresh Rate | 7.8 us (2X 85-95 C)
| Data Width | 64 bits
| SDRAM Width | x8
| Voltage Interface | 1.5 V
| Max Case Temperature | 95 °C (203 °F)
| SPD Revision | 1.0
| Part Number | 99U5474-010.A00LF
| Manufacturing Location | 5
| Manufacture Date | June 2012 (1238h)
| Serial Number | 92275739h
| Revision Code | None
| EPP Support | Not Supported
| XMP Support | Not Supported
| Memory Slot 3
| Memory Type | 2048MB DDR3-1333 (PC3-10600) SDRAM
| Manufacturer | Kingston
| Module Type | Unbuffered DIMM
| Number of Ranks/Banks | 1 Ranks, 8 Banks
| Module Attributes | Unbuffered
| Error Checking | None
| CAS# Latency | 9.0 (Cycle Time: 1.500ns/686MHz)
| CAS# Latency | 8.0 (Cycle Time: 1.371ns/610MHz)
| CAS# Latency | 7.0 (Cycle Time: 1.200ns/533MHz)
| CAS# Latency | 6.0 (Cycle Time: 1.029ns/457MHz)
| Refresh Rate | 7.8 us (2X 85-95 C)
| Data Width | 64 bits
| SDRAM Width | x8
| Voltage Interface | 1.5 V
| Max Case Temperature | 95 °C (203 °F)
| SPD Revision | 1.0
| Part Number | 99U5474-010.A00LF
| Manufacturing Location | 5
| Manufacture Date | June 2012 (1238h)
| Serial Number | 8D276A39h
| Revision Code | None
| EPP Support | Not Supported
| XMP Support | Not Supported
Memory (SMBIOS)
| Physical Memory Array 1
| Maximum Capacity | 32768 MB
| Location | System Board or Motherboard
| Use | System Memory
| Memory Error Correct. | None
| Memory Devices | 2
| Structure Length | 17h
| Memory Device 1
| Size | 2048 MB
| Form Factor | DIMM
| Memory Type | DDR3
| Speed | 1333 MHz
| Configured Speed | 1333 MHz
| Device Locator | ChannelA-DIMM0
| Bank Locator | BANK 0
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | Synchronous
| Manufacturer | Kingston
| Serial Number | 92275739
| Asset Tag | 9876543210
| Part Number | 99U5474-010.A00LF
| Structure Length | 22h
| Memory Device 2
| Size | Not Installed
| Form Factor | DIMM
| Memory Type | Unknown
| Speed | Unknown
| Device Locator | ChannelA-DIMM1
| Bank Locator | BANK 1
| Total Width | 0 bits
| Data Width | 0 bits
| Device Set | 00h
| Type Detail | None
| Manufacturer | [Empty]
| Serial Number | [Empty]
| Asset Tag | 9876543210
| Part Number | [Empty]
| Structure Length | 22h
| Memory Device 3
| Size | 2048 MB
| Form Factor | DIMM
| Memory Type | DDR3
| Speed | 1333 MHz
| Configured Speed | 1333 MHz
| Device Locator | ChannelB-DIMM0
| Bank Locator | BANK 2
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | Synchronous
| Manufacturer | Kingston
| Serial Number | 8D276A39
| Asset Tag | 9876543210
| Part Number | 99U5474-010.A00LF
| Structure Length | 22h
| Memory Device 4
| Size | Not Installed
| Form Factor | DIMM
| Memory Type | Unknown
| Speed | Unknown
| Device Locator | ChannelB-DIMM1
| Bank Locator | BANK 3
| Total Width | 0 bits
| Data Width | 0 bits
| Device Set | 00h
| Type Detail | None
| Manufacturer | [Empty]
| Serial Number | [Empty]
| Asset Tag | 9876543210
| Part Number | [Empty]
| Structure Length | 22h
HDD
| Primary/Master HDD
| HDD Model | SSD Smartbuy 60GB
| HDD Size | 57241 MB (55.90 GB)
| Interface Type | Serial ATA III (SATA/600)
| Form Factor | 2.5"
| Rotation Rate | SSD
| Geometry | Heads: 16, Sectors: 63, Tracks: 16383
| Compatibility | ATA8-ACS
| Serial Number | DA5A07471EEE00690280
| Controller Revision | S8FM07.7
| HDD Marketing Size | 60022 MB (60.02 GB)
| Buffer Size | Unknown
| Buffer Type | Not Specified
| Reallocated Sectors | 0
| HDD Health Status | Good
| SSD Remaining Life | 100 %
| Total Host Writes | 1520.0 GB
| ECC bytes | None
| Security Erase Time | 60 min
| Enh. Security Erase | 60 min
| Current APM Value | None
| Acoustic Management | None
| Device Location | Primary/Master
| Transfer Modes
| SATA Speed | 600 MB/s, Active: 600 MB/s
| PIO Mode Support | 4
| SW DMA Mode Support | Not Supported
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 6 (UltraDMA/133), Active: 5 (UltraDMA/100)
| Sectors per Interrupt | 16, Active: 16
| HDD Features
| SATA NCQ Command | Supported
| SSD TRIM Command | Supported
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Supported
| Double Word I/O | Supported
| Standard Standby Timer | Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Supported
| S.M.A.R.T. | Supported, Enabled
| S.M.A.R.T. Self-test | Supported, Enabled
| S.M.A.R.T. Error Logging | Supported, Enabled
| Security Mode Feature Set | Supported, Disabled
| Removable Media | Not Supported
| Power Management | Supported, Enabled
| PACKET Command | Not Supported
| Write Cache | Supported, Enabled
| Look-ahead | Supported, Enabled
| Release Interrupt | Not Supported
| Service Interrupt | Not Supported
| Device Reset Command | Not Supported
| Host Protected Area | Supported, Enabled
| Write Verify Command | Not Supported
| Write Buffer Command | Supported, Enabled
| Read Buffer Command | Supported, Enabled
| NOP Command | Not Supported
| Identify Device DMA Command | Not Supported
| Download Microcode Command | Supported, Enabled
| Read/Write DMA Queued | Not Supported
| CFA Feature Set | Not Supported
| Advanced Power Management | Supported, Disabled
| Removable Media Status | Not Supported
| Power-up in Standby | Not Supported
| Set Features Req. to Spinup | Not Supported
| Set Max Security Extension | Supported, Disabled
| Automatic Acoustic Management | Not Supported
| 48-bit Address | Supported, Enabled
| Device Configuration Overlay | Supported, Enabled
| Flush Cache Command | Supported, Enabled
| Flush Cache Ext Command | Supported, Enabled
| Media Serial Number | Not Supported
| Media Card Pass Through | Not Supported
| Streaming Feature Set | Not Supported
| General Purpose Logging | Supported, Enabled
| Write DMA/Multiple FUA EXT | Supported, Enabled
| Write DMA Queued FUA EXT | Not Supported
| World Wide Name | Not Supported
| S.M.A.R.T.
| ID | Attribute Name | Threshold | Worst | Value | Raw Value
| 1 | Raw Read Error Rate | 50 | 100 | 100 | 0
| 9 | Power On Hours Count | 0 | 100 | 100 | 1107
| 12 | Drive Power Cycle Count | 0 | 100 | 100 | 793
| 168 | SATA PHY Error Count | 0 | 100 | 100 | 1210307
| 170 | Available Reserved Space | 10 | 100 | 100 | 193
| 173 | Average Erase Count | 0 | 100 | 100 | 3539092
| 192 | Unsafe Shutdown Count | 0 | 100 | 100 | 27
| 218 | Vendor Specific | 50 | 100 | 100 | 1301
| 241 | Total Host Writes | 0 | 100 | 100 | 1520
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard disk drives)
| Device Description | Disk drive
| Friendly Name | SSD Smartbuy 60GB ATA Device
| Device Class | DiskDrive
| Device Location | Channel 0, Target 0, Lun 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7600.16385
| Driver Date | 6-21-2006
| Inf File | disk.inf
| Service Name | disk
| Hardware ID | IDE\DiskSSD_Smartbuy_60GB_______________________S8FM07.7
| Compatible ID | GenDisk
| Secondary/Master HDD
| HDD Model | WDC WD1001FALS-00J7B0
| HDD Size | 953869 MB (931.51 GB)
| Interface Type | Serial ATA II (SATA/300)
| Geometry | Heads: 16, Sectors: 63, Tracks: 16383
| Compatibility | ATA8-ACS
| Serial Number | WD-WMATV0357962
| Controller Revision | 05.00K05
| HDD Marketing Size | 1000204 MB (1000.20 GB)
| Buffer Size | 32 MB
| Buffer Type | Not Specified
| HDD Temperature | 43 °C (109 °F)
| Reallocated Sectors | 0
| HDD Health Status | Good
| ECC bytes | 50
| Security Erase Time | 194 min
| Enh. Security Erase | 194 min
| Current APM Value | None
| Acoustic Management | 80h (80h Recommended) - Enabled
| Device Location | Secondary/Master
| Transfer Modes
| SATA Speed | 300 MB/s
| PIO Mode Support | 4
| SW DMA Mode Support | Not Supported
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 6 (UltraDMA/133), Active: 5 (UltraDMA/100)
| Sectors per Interrupt | 16, Active: 16
| HDD Features
| SATA NCQ Command | Supported
| SSD TRIM Command | Not Supported
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Supported
| Double Word I/O | Not Supported
| Standard Standby Timer | Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Supported
| S.M.A.R.T. | Supported, Enabled
| S.M.A.R.T. Self-test | Supported, Enabled
| S.M.A.R.T. Error Logging | Supported, Enabled
| Security Mode Feature Set | Supported, Disabled
| Removable Media | Not Supported
| Power Management | Supported, Enabled
| PACKET Command | Not Supported
| Write Cache | Supported, Enabled
| Look-ahead | Supported, Enabled
| Release Interrupt | Not Supported
| Service Interrupt | Not Supported
| Device Reset Command | Not Supported
| Host Protected Area | Supported, Enabled
| Write Verify Command | Not Supported
| Write Buffer Command | Supported, Enabled
| Read Buffer Command | Supported, Enabled
| NOP Command | Supported, Enabled
| Identify Device DMA Command | Not Supported
| Download Microcode Command | Supported, Enabled
| Read/Write DMA Queued | Not Supported
| CFA Feature Set | Not Supported
| Advanced Power Management | Not Supported
| Removable Media Status | Not Supported
| Power-up in Standby | Supported, Disabled
| Set Features Req. to Spinup | Supported, Enabled
| Set Max Security Extension | Supported, Disabled
| Automatic Acoustic Management | Supported, Enabled
| 48-bit Address | Supported, Enabled
| Device Configuration Overlay | Supported, Enabled
| Flush Cache Command | Supported, Enabled
| Flush Cache Ext Command | Supported, Enabled
| Media Serial Number | Not Supported
| Media Card Pass Through | Not Supported
| Streaming Feature Set | Not Supported
| General Purpose Logging | Supported, Enabled
| Write DMA/Multiple FUA EXT | Not Supported
| Write DMA Queued FUA EXT | Not Supported
| World Wide Name | Supported, Enabled
| S.M.A.R.T.
| ID | Attribute Name | Threshold | Worst | Value | Raw Value
| 1 | Raw Read Error Rate | 51 | 200 | 200 | 0
| 3 | Spin-up Time | 21 | 253 | 253 | 5483
| 4 | Start/Stop Count | 0 | 90 | 90 | 10384
| 5 | Reallocated Sectors Count | 140 | 200 | 200 | 0
| 7 | Seek Error Rate | 51 | 200 | 200 | 0
| 9 | Power On Hours Count | 0 | 73 | 73 | 19809
| 10 | Spin-up Retry Count | 51 | 100 | 100 | 0
| 11 | Recalibration Retries | 51 | 100 | 100 | 0
| 12 | Drive Power Cycle Count | 0 | 90 | 90 | 10100
| 192 | Power-Off Retract Count | 0 | 198 | 198 | 1714
| 193 | Load/Unload Cycle Count | 0 | 197 | 197 | 10382
| 194 | Drive Temperature | 0 | 89 | 107 | 43
| 196 | Reallocation Event Count | 0 | 200 | 200 | 0
| 197 | Current Pending Sectors | 0 | 200 | 200 | 0
| 198 | Uncorrectable Sectors | 0 | 200 | 200 | 0
| 199 | UltraDMA CRC Error Rate | 0 | 200 | 200 | 312
| 200 | Write Error Rate | 51 | 200 | 200 | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard disk drives)
| Device Description | Disk drive
| Friendly Name | WDC WD1001FALS-00J7B0 ATA Device
| Device Class | DiskDrive
| Device Location | Channel 1, Target 0, Lun 0
| Driver Provider | Microsoft
| Driver Version | 6.1.7600.16385
| Driver Date | 6-21-2006
| Inf File | disk.inf
| Service Name | disk
| Hardware ID | IDE\DiskWDC_WD1001FALS-00J7B0___________________05.00K05
| Compatible ID | GenDisk
Storage (ASPI)
| ASPI devices not found
Logical Drives
| Local Drives
| C:[SYSTEM]
| Drive Letter | C:
| Drive Type | Fixed Disk
| Volume Label | SYSTEM
| File System | FAT
| Volume Serial Number | 2255-1BEA
| Total Size | 2047.0 MB
| Free Space | 402.1 MB (19.6%)
| D:[UTILITIES]
| Drive Letter | D:
| Drive Type | Fixed Disk
| Volume Label | UTILITIES
| File System | FAT
| Volume Serial Number | 2E4A-1BEB
| Total Size | 2047.1 MB
| Free Space | 113.5 MB (5.5%)
| E:[INSTALL]
| Drive Letter | E:
| Drive Type | Fixed Disk
| Volume Label | INSTALL
| File System | NTFS
| Volume Serial Number | 08B6-AD4A
| Total Size | 53.0 GB
| Free Space | 146.5 MB (0.3%)
| F:[WIN10]
| Drive Letter | F:
| Drive Type | Fixed Disk
| Volume Label | WIN10
| File System | NTFS
| Volume Serial Number | E804-72DE
| Total Size | 30.0 GB
| Free Space | 8.5 GB (28.3%)
| G:[WIN7]
| Drive Letter | G:
| Drive Type | Fixed Disk
| Volume Label | WIN7
| File System | NTFS
| Volume Serial Number | 48B9-FCDB
| Total Size | 55.9 GB
| Free Space | 2.7 GB (4.8%)
| H:[MUSIC]
| Drive Letter | H:
| Drive Type | Fixed Disk
| Volume Label | MUSIC
| File System | NTFS
| Volume Serial Number | 38D2-852D
| Total Size | 834.5 GB
| Free Space | 36.4 GB (4.4%)
| I:[WINXP]
| Drive Letter | I:
| Drive Type | Fixed Disk
| Volume Label | WINXP
| File System | NTFS
| Volume Serial Number | A297-0D56
| Total Size | 10.0 GB
| Free Space | 5.9 GB (58.6%)
USB Devices
| USB Device 1
| Vendor (8087h) | Intel Corp.
| Device (8000h) | Integrated Rate Matching Hub
| Manufacturer |
| Product |
| Serial Number |
| Device Version | 0.05
| Class (09h) | Hub
| SubClass (00h) | Unused
| Protocol (01h) | Single TT
| Configuration |
| USB Version | 2.00
| Speed | 480 Mb/s
| Transfer Type | Interrupt
| Data Packet Size | 64 bytes
| Max Power | Remote Wakeup
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Generic USB Hub)
| Device Description | Generic USB Hub
| Device Class | USB
| Device Location | Port_#0001.Hub_#0002
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.18328
| Driver Date | 6-21-2006
| Inf File | usb.inf
| Service Name | usbhub
| Hardware ID | USB\VID_8087&PID_8000&REV_0005
| Compatible ID | USB\Class_09&SubClass_00&Prot_00
| Interface 1
| Class (09h) | Hub
| SubClass (00h) | Unused
| Protocol (00h) | Full Speed (or Root) Hub
| Interface |
| USB Device 2
| Vendor (8087h) | Intel Corp.
| Device (8008h) | Integrated Rate Matching Hub
| Manufacturer |
| Product |
| Serial Number |
| Device Version | 0.05
| Class (09h) | Hub
| SubClass (00h) | Unused
| Protocol (01h) | Single TT
| Configuration |
| USB Version | 2.00
| Speed | 480 Mb/s
| Transfer Type | Interrupt
| Data Packet Size | 64 bytes
| Max Power | Remote Wakeup
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Generic USB Hub)
| Device Description | Generic USB Hub
| Device Class | USB
| Device Location | Port_#0001.Hub_#0001
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.18328
| Driver Date | 6-21-2006
| Inf File | usb.inf
| Service Name | usbhub
| Hardware ID | USB\VID_8087&PID_8008&REV_0005
| Compatible ID | USB\Class_09&SubClass_00&Prot_00
| Interface 1
| Class (09h) | Hub
| SubClass (00h) | Unused
| Protocol (00h) | Full Speed (or Root) Hub
| Interface |
| USB Device 3
| Vendor (0458h) | KYE Systems Corp. (Genius)
| Device (002Ch) | Wireless TwinTouch Optical Office
| Manufacturer | KYE SYSTEMS CORP.
| Product | Wireless TwinTouch Optical Office
| Serial Number |
| Device Version | 1.13
| Class (00h) | Unknown
| SubClass (00h) | Unknown
| Protocol (00h) | Unknown
| Configuration | HID Keyboard / Mouse
| USB Version | 1.10
| Speed | Low (1.5 Mb/s)
| Transfer Type | Interrupt
| Data Packet Size | 8 bytes
| Max Power | 100 mA Remote Wakeup
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard USB Host Controller)
| Device Description | USB Composite Device
| Device Class | USB
| Device Location | Port_#0004.Hub_#0001
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.18328
| Driver Date | 6-21-2006
| Inf File | usb.inf
| Service Name | usbccgp
| Hardware ID | USB\VID_0458&PID_002C&REV_010D
| Compatible ID | IUSB3\DevClass_00&SubClass_00&Prot_00
| Interface 1
| Class (03h) | Human Interface Devices
| SubClass (01h) | Boot Interface Subclass
| Protocol (01h) | Keyboard
| Interface | EP1 Interrupt
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | USB Input Device
| Device Class | HIDClass
| Device Location | 0000.0014.0000.004.000.000.000.000.000
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.18199
| Driver Date | 6-21-2006
| Inf File | input.inf
| Service Name | HidUsb
| Hardware ID | USB\VID_0458&PID_002C&REV_010D&MI_00
| Compatible ID | USB\Class_03&SubClass_01&Prot_01
| Interface 2
| Class (03h) | Human Interface Devices
| SubClass (01h) | Boot Interface Subclass
| Protocol (02h) | Mouse
| Interface | EP2 Interrupt
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | USB Input Device
| Device Class | HIDClass
| Device Location | 0000.0014.0000.004.000.000.000.000.000
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.18199
| Driver Date | 6-21-2006
| Inf File | input.inf
| Service Name | HidUsb
| Hardware ID | USB\VID_0458&PID_002C&REV_010D&MI_01
| Compatible ID | USB\Class_03&SubClass_01&Prot_02
| USB Device 4
| Vendor (0458h) | KYE Systems Corp. (Genius)
| Device (003Ah) | Scroll Mouse
| Manufacturer | Genius
| Product | USB Optical Mouse
| Serial Number |
| Device Version | 1.00
| Class (00h) | Unknown
| SubClass (00h) | Unknown
| Protocol (00h) | Unknown
| Configuration |
| USB Version | 2.00
| Speed | 480 Mb/s
| Transfer Type | Interrupt
| Data Packet Size | 8 bytes
| Max Power | 100 mA Remote Wakeup
| Driver
| Driver Status | The device is working properly
| Manufacturer | (Standard system devices)
| Device Description | USB Input Device
| Device Class | HIDClass
| Device Location | Port_#0006.Hub_#0001
| Driver Provider | Microsoft
| Driver Version | 6.1.7601.18199
| Driver Date | 6-21-2006
| Inf File | input.inf
| Service Name | HidUsb
| Hardware ID | USB\VID_0458&PID_003A&REV_0100
| Compatible ID | USB\Class_03&SubClass_01&Prot_02
| Interface 1
| Class (03h) | Human Interface Devices
| SubClass (01h) | Boot Interface Subclass
| Protocol (02h) | Mouse
| Interface |
Physical Printers
| LPT/PnP or USB printer not found
Installed Printers
| Local Printers
| Installed Printer 1
| Printer Name | Microsoft XPS Document Writer
| Printer Port | XPSPort:
| Default Printer | Yes
| Printer Type | Local
| Print Processor | winprint
| Data Type | RAW
| Installed Printer 2
| Printer Name | Fax
| Printer Port | SHRFAX:
| Default Printer | No
| Printer Type | Local
| Print Processor | winprint
| Data Type | RAW
Slots (SMBIOS)
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 16x or x16
| Slot Designation | J6B2
| Slot Length | Long Length
| Slot ID | 0
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 1x or x1
| Slot Designation | J6B1
| Slot Length | Short Length
| Slot ID | 1
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 8x or x8
| Slot Designation | J6D1
| Slot Length | Short Length
| Slot ID | 2
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 16x or x16
| Slot Designation | J7B1
| Slot Length | Short Length
| Slot ID | 3
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | In Use
| Data Bus Width | 1x or x1
| Slot Designation | J8B4
| Slot Length | Short Length
| Slot ID | 4
| Slot PCI
| Slot Type | PCI
| Current Usage | In Use
| Data Bus Width | 32 bit
| Slot Designation | J8B3
| Slot Length | Short Length
| Slot ID | 6
Ports (SMBIOS)
| Port 1 Mouse Port
| Int. Connector Type | None
| Ext. Connector Type | PS/2
| Port Type | Mouse Port
| Int. Designator | J1A1
| Ext. Designator | PS2Mouse
| Port 2 Keyboard Port
| Int. Connector Type | None
| Ext. Connector Type | PS/2
| Port Type | Keyboard Port
| Int. Designator | J1A1
| Ext. Designator | Keyboard
| Port 3 Other
| Int. Connector Type | None
| Ext. Connector Type | Mini-Centronics Type-14
| Port Type | Other
| Int. Designator | J2A1
| Ext. Designator | TV Out
| Port 4 Serial Port 16550A Compatible
| Int. Connector Type | None
| Ext. Connector Type | DB-9 pin male
| Port Type | Serial Port 16550A Compatible
| Int. Designator | J2A2A
| Ext. Designator | COM A
| Port 5 Video Port
| Int. Connector Type | None
| Ext. Connector Type | DB-15 pin female
| Port Type | Video Port
| Int. Designator | J2A2B
| Ext. Designator | Video
| Port 6 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | J3A1
| Ext. Designator | USB1
| Port 7 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | J3A1
| Ext. Designator | USB2
| Port 8 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | J3A1
| Ext. Designator | USB3
| Port 9 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J9A1 - TPM HDR
| Ext. Designator |
| Port 10 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J9C1 - PCIE DOCKING CONN
| Ext. Designator |
| Port 11 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J2B3 - CPU FAN
| Ext. Designator |
| Port 12 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J6C2 - EXT HDMI
| Ext. Designator |
| Port 13 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J3C1 - GMCH FAN
| Ext. Designator |
| Port 14 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J1D1 - ITP
| Ext. Designator |
| Port 15 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J9E2 - MDC INTPSR
| Ext. Designator |
| Port 16 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J9E4 - MDC INTPSR
| Ext. Designator |
| Port 17 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J9E3 - LPC HOT DOCKING
| Ext. Designator |
| Port 18 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J9E1 - SCAN MATRIX
| Ext. Designator |
| Port 19 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J9G1 - LPC SIDE BAND
| Ext. Designator |
| Port 20 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J8F1 - UNIFIED
| Ext. Designator |
| Port 21 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J6F1 - LVDS
| Ext. Designator |
| Port 22 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J2F1 - LAI FAN
| Ext. Designator |
| Port 23 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J2G1 - GFX VID
| Ext. Designator |
| Port 24 Other
| Int. Connector Type | Other
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | J1G6 - AC JACK
| Ext. Designator |
Network
| Network
| Network Name | A2KKV
| User Name | kkv1
| User Role | Administrator
| Logon Domain | A2KKV
| Interface 1
| Description | TAP-Windows Adapter V9
| MAC Address | 00-FF-CA-D1-AF-0D
| Adapter Type | Ethernet
| Link Speed | 100.0 Mbps
| MTU Size | 1500 byte
| Adapter Status | Enabled
| Operational Status | Non Operational
| DHCP Server | Unknown
| Gateway | 0.0.0.0
| Interface 2
| Adapter Vendor | Realtek Semiconductor
| Adapter Name | RTL8111/8168/8411 PCI Express Gigabit Ethernet Controller
| Subsys Vendor | Giga-Byte Technology
| Subsystem ID | GA-EP45-DS5 Motherboard
| Bus Type | PCI-E
| Description | Realtek PCIe GBE Family Controller
| MAC Address | 74-D4-35-CD-93-A8
| Adapter Type | Ethernet
| Link Speed | 100.0 Mbps
| MTU Size | 1500 byte
| Adapter Status | Enabled
| Operational Status | Operational
| DHCP Server | 192.168.1.1
| IP Address | 192.168.1.141
| IP Address Subnet Mask | 255.255.255.0
| Gateway | 192.168.1.1
| DNS Server | 192.168.1.1
Monitor
| Monitor
| Monitor Vendor | LG Electronics Inc.
| Monitor Model | LG FLATRON F920P
| Viewable Size | 17.7" (45.0 sm)
| Serial Number | 319823
| Manufacture Date | March 2005
| EDID Version | 1.3
| Monitor ID | GSM4A88
| Aspect Ratio | 4:3
| Horizontal Size | 36 sm
| Vertical Size | 27 sm
| Gamma Factor | 2.910
| Display Type | RGB Color
| Input Signal | Analog
| Internal Model | F920P
| Vertical Frequency | 50-160 Hz
| Horizontal Frequency | 30-111 kHz
| DPMS Features
| Active Off | Supported
| Suspend | Supported
| Standby | Supported
| Supported Modes
| Mode 1 | 720x400 @ 70 Hz (VGA)
| Mode 2 | 720x400 @ 88 Hz (XGA2)
| Mode 3 | 640x480 @ 60 Hz (VGA)
| Mode 4 | 640x480 @ 67 Hz (Mac II)
| Mode 5 | 640x480 @ 72 Hz (VESA)
| Mode 6 | 640x480 @ 75 Hz (VESA)
| Mode 7 | 800x600 @ 56 Hz (VESA)
| Mode 8 | 800x600 @ 60 Hz (VESA)
| Mode 9 | 800x600 @ 72 Hz (VESA)
| Mode 10 | 800x600 @ 75 Hz (VESA)
| Mode 11 | 832x624 @ 75 Hz (Mac II)
| Mode 12 | 1024x768 @ 87 Hz (interlaced)
| Mode 13 | 1024x768 @ 60 Hz (VESA)
| Mode 14 | 1024x768 @ 70 Hz (VESA)
| Mode 15 | 1024x768 @ 75 Hz (VESA)
| Mode 16 | 1280x1024 @ 75 Hz (VESA)
| Mode 17 | 1920x1440 @ 70 Hz
| Mode 18 | 2048x1536 @ 60 Hz
| Mode 19 | 1024x768 @ 120 Hz
| Mode 20 | 1280x1024 @ 100 Hz
| Mode 21 | 1280x1024 @ 85 Hz
| Mode 22 | 1600x1200 @ 75 Hz
| Mode 23 | 1600x1200 @ 85 Hz
| Mode 24 | 1152x864 @ 120 Hz
| Driver
| Driver Status | The device is working properly
| Manufacturer | LGE
| Device Description | LGE F920P (GSM4A88 EDID Override)
| Device Class | Monitor
| Driver Provider | EnTech Taiwan
| Driver Version | 1.0.0.0
| Inf File | oem4.inf
| Service Name | monitor
| Hardware ID | MONITOR\GSM4A88
| Compatible ID | *PNP09FF
Video
| Video
| Video Chip Vendor | ATI Technologies Inc
| Video Chip | Pitcairn PRO [Radeon HD 7800 Series]
| Subsystem Vendor | Giga-Byte Technology
| Video Memory Size | 2 GB
| Video BIOS Version | 015.021.000.003
| Video BIOS Date | 2012/08/05 21:33
| Part Number | 113-xxx-xxx
| Core Temperature | 35 °C (95 °F)
| Current Core Clock | 300 MHz
| Current Memory Clock | 150 MHz
| Core Voltage | 0.825 V
| Core Usage | 0 %
| Performance Level | 0
| Bus Type | PCI-E
| PCI-E Capabilities
| PCI Express Version | 2.0
| Device/Port Type | Legacy PCI-E Endpoint
| Link Speed | 8.0 GB/s (Current: 2.5 GB/s)
| Link Width | x16 (Current: x16)
| Link Port Number | 0
| Physical Slot Number | 0
| Driver
| Driver Status | The device is working properly
| Manufacturer | Advanced Micro Devices, Inc.
| Device Description | AMD Radeon HD 7800 Series
| Device Class | Display
| Device Location | PCI bus 1, device 0, function 0
| Driver Provider | Advanced Micro Devices, Inc.
| Driver Version | 14.501.1003.0
| Driver Date | 11-20-2014
| Inf File | oem15.inf
| Service Name | amdkmdap
| Hardware ID | PCI\VEN_1002&DEV_6819&SUBSYS_25531458&REV_00
| Compatible ID | PCI\VEN_1002&DEV_6819&REV_00
Hardware Monitoring
| Processor
| Processor | Intel Core i3-4160 3600 MHz
| Core Voltage | 0.925 V
| Package Temperature | 38 °C (100 °F)
| Core 1
| Temperature Core | 36 °C (97 °F)
| Core Clock | 1696.1 MHz (Original: 3600 MHz)
| FSB Clock | 99.8 MHz
| Multiplier | 17.0
| Core 2
| Temperature Core | 38 °C (100 °F)
| Core Clock | 3591.7 MHz (Original: 3600 MHz)
| FSB Clock | 99.8 MHz
| Multiplier | 36.0
| Video Card
| Video Chip | Pitcairn PRO [Radeon HD 7800 Series]
| Core Temperature | 35 °C (95 °F)
| Current Core Clock | 300 MHz
| Current Memory Clock | 150 MHz
| Core Voltage | 0.825 V
| Core Usage | 0 %
| Performance Level | 0
| Disk Drive 1
| HDD Model | SSD Smartbuy 60GB
| Total Host Writes | 1520.0 GB
| Disk Drive 2
| HDD Model | WDC WD1001FALS-00J7B0
| HDD Temperature | 43 °C (109 °F)
Drivers Troubleshooter
| List of Problem Devices
| All devices are working properly
HDD Diagnostics
| HDD 1 Status
| HDD Model | SSD Smartbuy 60GB
| HDD Size | 57241 MB (55.90 GB)
| Interface Type | Serial ATA III (SATA/600)
| Serial Number | DA5A07471EEE00690280
| Controller Revision | S8FM07.7
| HDD Marketing Size | 60022 MB (60.02 GB)
| Buffer Size | Unknown
| Device Location | Primary/Master
| Reallocated Sectors | 0
| HDD Health Status | Good
| SSD Remaining Life | 100 %
| Total Host Writes | 1520.0 GB
| HDD 2 Status
| HDD Model | WDC WD1001FALS-00J7B0
| HDD Size | 953869 MB (931.51 GB)
| Interface Type | Serial ATA II (SATA/300)
| Serial Number | WD-WMATV0357962
| Controller Revision | 05.00K05
| HDD Marketing Size | 1000204 MB (1000.20 GB)
| Buffer Size | 32767.5 kB
| Device Location | Secondary/Master
| HDD Temperature | 43 °C (109 °F)
| Reallocated Sectors | 0
| HDD Health Status | Good
Windows
| Windows
| Operating System | MS Windows 7 Ultimate x64 Edition (6.1.7601 Service Pack 1)
| OS Language | Russian (Russia)
| Windows Folder | G:\Windows
| Installation Date | December 18, 2014
| Kernel Type | Multiprocessor Free
| Registered Owner | kkv1
| Registered Organization | Microsoft
| Product ID | 00426-OEM-8992662-00400
| Product Key | XXXXX-XXXXX-XXXXX-XXXXX-XXXXX
| System UpTime | 0 Hour(s) 5 Minutes 16 Seconds
| IE Version | 9.11.9600.17691
| DirectX Version | DirectX 11
| Regional Settings
| Country | Russia
| Language | Russian
| Time Zone | Russia TZ 2 Standard Time (GMT+3)
| Currency Name | Russian Ruble
| Measurment System | Metric
| ANSI Code Page | 1251
| OEM Code Page | 866
Installed Programs
| Installed Programs
| Program Name | Version | Publisher | Date | Size |
| ASTRA32 - Advanced System Information Tool | 3.23 | Sysinfo Lab |  |  |
| Mozilla Firefox (x86 ru) | 37.0.2 | Mozilla |  | 84.7 MB |
| OpenOffice 4.1.1 | 4.11.9775 | Apache Software Foundation | 22.01.2015 | 332.4 MB |
| OpenVPN | 2.3.6-I601 |  |  |  |
| Realtek Ethernet Controller Driver | 7.90.826.2014 | Realtek | 18.12.2014 |  |
| Realtek High Definition Audio Driver | 6.0.1.7246 | Realtek Semiconductor Corp. | 22.01.2015 |  |
| Sound Blaster Audigy 2 ZS | 1.0 | Creative Technology Limited |  |  |
| TAP-Windows | 9.21.1 |  |  |  |
| WinCDEmu | 4.0 | Sysprogs |  |  |
| foobar2000 | 1.3.7 | Peter Pawlowski |  | 18 MB |
Installed Hotfixes
| Installed Hotfixes
| Hotfix for Microsoft Windows (KB2534111) | 18.12.2014
| Hotfix for Microsoft Windows (KB2847077) | 18.12.2014
| Hotfix for Microsoft Windows (KB2977728) |
| Hotfix for Microsoft Windows (KB3006137) |
| Hotfix for Microsoft Windows (KB3009736) |