  +------------------------------------------------------------------------+
  |    This report is created by ASTRA32 v.3.30  .  Apr-28-2015 21:59:40   |
  +------------------------------------------------------------------------+
                               A2KKV
                               
     Registered To:            Sysinfo Lab
     License Type:             Professional for 1 computer
                               
                  +-----------------------------------------+
                  |              System Summary             |
                  +-----------------------------------------+
  Processor 
     Processor:                Intel Core i3-4160 3600 MHz
     CPU Clock:                3591.7 MHz (36.0 x 99.8 MHz)
     Level 1 Cache:            2 x 32 kB + 2 x 32 kB (data+instr.)
     Level 2 Cache:            2 x 256 kB
     Level 3 Cache:            1 x 3 MB
  Motherboard
     System Name:              Gigabyte Technology Co., Ltd. H81M-S2PV
     Board Model:              Gigabyte Technology Co., Ltd. H81M-S2PV
     BIOS Version:             AMI BIOS 08.00.10
     Chipset Name:             Intel H81 (Lynx Point)
     Chipset Vendor:           Intel Corporation
     Chipset:                  4th Gen Core Processor DRAM Controller
     Southbridge Vendor:       Intel Corporation
     Southbridge:              H81 Chipset LPC Controller
     DMI/SMBIOS Version:       2.7
  Memory
     Memory Size:              3.9 GB
     System Memory:            4042 MB
     Memory Module:            2048MB DDR3-1333 (PC3-10600) SDRAM (Kingston)
     Memory Module:            2048MB DDR3-1333 (PC3-10600) SDRAM (Kingston)
  Storage
     HDD Model:                SSD Smartbuy 60GB
     HDD Size:                 57241 MB (55.90 GB)
     HDD Model:                WDC WD1001FALS-00J7B0
     HDD Size:                 953869 MB (931.51 GB)
  Video
     Monitor Vendor:           LG Electronics Inc.
     Monitor Model:            LG FLATRON F920P
     Video Chip Vendor:        ATI Technologies Inc
     Video Chip:               Pitcairn PRO [Radeon HD 7800 Series]
     Video Memory Size:        2 GB
  Sound
     Sound Chip Vendor:        Intel Corporation
     Sound Chip:               8 Series/C220 Series Chipset Family HD Audio Controller
     Sound Chip Vendor:        ATI Technologies Inc
     Sound Chip:               Cape Verde/Pitcairn HDMI Audio [Radeon HD 7700/7800 Series]
     AC'97/HDA Codec Name:     ATI R6xx HDMI
     Sound Chip Vendor:        Creative Labs
     Sound Chip:               EMU10K2 Audio Chipset (SB Audigy Series)
  Operating System
     Operating System:         MS Windows 7 Ultimate x64 Edition (6.1.7601 Service Pack 1)
     Windows Folder:           G:\Windows
  Modem
     Modem Vendor:             Intel Corporation
     Modem Model:              8 Series/C220 Series Chipset Family MEI Controller #1
  Network
     Network Name:             A2KKV
     Interface Description:    TAP-Windows Adapter V9
     MAC Address:              00-FF-CA-D1-AF-0D
     Adapter Vendor:           Realtek Semiconductor
     Adapter Name:             RTL8111/8168/8411 PCI Express Gigabit Ethernet Controller
     Interface Description:    Realtek PCIe GBE Family Controller
     MAC Address:              74-D4-35-CD-93-A8
  Ports
     LPT Ports:                None
     COM Ports:                None
                               
                  +-----------------------------------------+
                  |               Motherboard               |
                  +-----------------------------------------+
  System
     System Vendor:            Gigabyte Technology Co., Ltd.
     Product Name:             H81M-S2PV
     Version:                  To be filled by O.E.M.
     Serial Number:            To be filled by O.E.M.
     UUID:                     7402D4033504CD059306A80700080009
     Wake-up Type:             Power Switch
     SKU Number:               To be filled by O.E.M.
     Family:                   To be filled by O.E.M.
  Motherboard
     Motherboard Vendor:       Unknown (0001)
     Vendor URL:               Unknown
     Board Model:              Gigabyte Technology Co., Ltd. H81M-S2PV
     Version:                  x.x
     Serial Number:            To be filled by O.E.M.
     BIOS Version:             AMI BIOS 08.00.10
     BIOS Date:                04/13/12
     Chipset Name:             Intel H81 (Lynx Point)
     Chipset Vendor:           Intel Corporation
     Chipset:                  4th Gen Core Processor DRAM Controller
     Southbridge Vendor:       Intel Corporation
     Southbridge:              H81 Chipset LPC Controller
  Onboard Device 1
     Description:              To Be Filled By O.E.M.
     Device Type:              Video
     Status:                   Enabled
  Configuration Options
     To Be Filled By O.E.M.
  System Enclosure
     Manufacturer:             Gigabyte Technology Co., Ltd.
     Type:                     Desktop
     Version:                  To Be Filled By O.E.M.
     Serial Number:            To Be Filled By O.E.M.
     Asset Tag:                To Be Filled By O.E.M.
     Boot-up State:            Safe
     Power Supply State:       Safe
     Thermal State:            Safe
     Security Status:          None
     OEM-defined:              00000000h
     Height:                   0.0 sm
     Power Cords:              1
     Contained Element:        0
                               
                  +-----------------------------------------+
                  |                  CPU                    |
                  +-----------------------------------------+
  CPU 
     Processor:                Intel Core i3-4160 3600 MHz
     Coprocessor:              Internal
     CPU Clock:                3591.7 MHz
     Level 1 Cache:            2 x 32 kB + 2 x 32 kB (data+instr.)
     Level 2 Cache:            2 x 256 kB
     Level 3 Cache:            1 x 3 MB
     Code Name:                Haswell-DT
     Manufacturing Process:    22 nm
     FSB Clock:                99.8 MHz
     Multiplier:               36.0
     Expected Clock:           3600 MHz
     Socket Type:              Socket 1150 FCLGA
     Package Temperature:      38 °C (100 °F)
     Temperature Core 1:       36 °C (97 °F)
     Temperature Core 2:       38 °C (100 °F)
     Tjmax Temperature:        100 °C (212 °F)
     Core Voltage:             1.175 V
     Vendor:                   GenuineIntel
     Processor Name:           Intel(R) Core(TM) i3-4160 CPU @ 3.60GHz
     Processor Type:           Original OEM Processor
     CPUID:                    Family: 6, Model: 12, Stepping: 3
     Ext. Family/Model:        Family: -, Model: 3
     CPU Signature:            000306C3h
     Brand ID:                 Not Supported
     Number of Cores:          2
     Logical CPU Count:        4
     Core Stepping:            C-0
     Max TDP:                  54 Wattes
     Transistor Count:         1400 million
     Die Size:                 177 mm2
     Family Frequency Range:   3.4-3.7 GHz
     Family Release Date:      September, 2013
     Max CPUID Level:          13
     Max ExtCPUID Level:       80000008h
  Instruction Set
     Floating-Point Unit On-Chip:         [X]
     IA MMX Technology:                   [X]
     SSE Instruction Set:                 [X]
     SSE2 Instruction Set:                [X]
     SSE3 Instruction Set:                [X]
     Supplemental SSE3 Instruction Set:   [X]
     SSE4.1 Instruction Set:              [X]
     SSE4.2 Instruction Set:              [X]
     Advanced Vector Extensions (AVX):    [X]
     Advanced Vector Extensions 2 (AVX2): [X]
     AVX-512 Foundation Instructions:     [ ]
     AVX-512 Prefetch Instructions:       [ ]
     AVX-512 Exponential and Reciprocal:  [ ]
     AVX-512 Conflict Detection:          [ ]
     AVX-512 Byte and Word Instructions:  [ ]
     AVX-512 Doubleword and Quadword:     [ ]
     AVX-512 Vector Length Extensions:    [ ]
     AVX-512 Integer Fused Multiply-Add:  [ ]
     AVX-512 Vector Bit Manipulation:     [ ]
     PCOMMIT Instruction:                 [ ]
     CLWB Instruction:                    [ ]
     PREFETCHWT1 Instruction:             [ ]
     Software Guard Extensions (SGX):     [ ]
     FMA Instructions Set:                [X]
     AES Instructions Set:                [X]
     Intel Extended Memory 64 Tech.:      [X]
     Intel Architecture - 64 (IA-64):     [ ]
     AMD MMX Instruction Extensions:      [ ]
     AMD 3DNow! Instructions:             [ ]
     AMD 3DNow! Extensions:               [ ]
     AMD 3DNow! Prefetch:                 [ ]
     AMD SSE4A Extensions:                [ ]
     AMD eXtended OPeration (XOP):        [ ]
     AMD Misaligned SSE:                  [ ]
     AMD64 Architecture:                  [ ]
     Cyrix Extended MMX:                  [ ]
     CMPXCHG8 Instruction Supported:      [X]
     CMPXCHG16 Instruction Supported:     [X]
     Fast System Call:                    [X]
     Conditional Move Instruction:        [X]
     CLFLUSH Insruction Supported:        [X]
     Fast Save and Restore:               [X]
     Monitor/MWAIT Instructions:          [X]
     SYSCALL/SYSRET Instructions:         [ ]
     LAHF/SAHF Instructions:              [X]
     POPCNT Insruction Supported:         [X]
     XSAVE Insructions Supported:         [X]
     OS Supports XSAVE Instructions:      [X]
     PCLMULQDQ Instruction Supported:     [X]
     MOVBE Insruction Supported:          [X]
     F16C Insruction Supported:           [X]
     RDTSCP Insruction Supported:         [X]
     RDRAND Insruction Supported:         [X]
     (RD/WR)(FS/GS) BASE Instructions:    [X]
     Bit Manipulation 1 Instructions:     [X]
     Bit Manipulation 1 Instructions:     [X]
     Enhanced REP MOVSB/STOSB:            [X]
     INVPCID Instruction:                 [X]
     XSAVEOPT Instruction:                [X]
     RDSEED Instruction:                  [ ]
     ADCX/ADOX Instructions:              [ ]
     CLAC/STAC Instructions:              [ ]
     SCLFLUSHOPT Instruction:             [ ]
     AMD Fast Save and Restore:           [ ]
     AMD SKINIT, STGI, DEV Supported:     [ ]
     AMD Light Weight Profiling (LWP):    [ ]
     AMD FMA4 Insruction Supported:       [ ]
     AMD TBM Insruction Supported:        [ ]
  Processor Features
     Virtual Mode Extension:              [X]
     Debugging Extension:                 [X]
     Page Size Extension:                 [X]
     Time Stamp Counter:                  [X]
     Model Specific Registers:            [X]
     Physical Address Extension:          [X]
     Machine Check Exception:             [X]
     On-chip APIC Hardware Supported:     [X]
     Memory Type Range Registers:         [X]
     Page Global Enable:                  [X]
     Machine Check Architecture:          [X]
     Page Attribute Table:                [X]
     36-bit Page Size Extension:          [X]
     Processor Serial Number:             [ ]
     Debug Store:                         [X]
     64-bit Debug Store:                  [X]
     Self-Snoop:                          [X]
     Hyper-Threading Technology:          [X]
     Pending Break Enable:                [X]
     CPL-Qualified Debug Store:           [X]
     L1 Context ID:                       [ ]
     Send Task Priority Messages:         [X]
     Direct Cache Access:                 [ ]
     Performance Capabilities MSR:        [X]
     x2APIC Architecture:                 [ ]
     Advanced Bit Manipulation:           [X]
     OS Visible Workaround:               [ ]
     Instruction Based Sampling:          [ ]
     1-GB Large Page:                     [X]
     Process Context Identifiers:         [X]
     Time Stamp Counter Deadline:         [X]
     Time Stamp Counter Adjust:           [X]
     Intel Virtualization Technology:     [X]
     Intel Trusted Execution Technology:  [ ]
     Supervisor Mode Execution Protection:[X]
     Hardware Lock Elision:               [ ]
     Restricted Transactional Memory:     [ ]
     Quality of Service Monitoring:       [ ]
     Quality of Service Enforcement:      [ ]
     Deprecated FPU CS and FPU DS:        [X]
     Memory Protection Extensions (MPX):  [ ]
     Processor Trace (PT):                [ ]
     Secure Hash Algorithm Ext. (SHA):    [ ]
     Debug Interface MSR:                 [X]
     Intel Turbo Boost Technology:        [ ]
     Intel Execute Disable Bit:           [X]
     AMD Secure Virtual Machine:          [ ]
     AMD Model-Specific Registers:        [ ]
     AMD Multiprocessing Capable:         [ ]
     AMD CMP Legacy Mode:                 [ ]
     AMD CR8 in Legacy Mode:              [ ]
     AMD Ext. APIC Register Space:        [ ]
     AMD Watchdog Timer:                  [ ]
     AMD Translation Cache Extension:     [ ]
     AMD Topology Extensions:             [ ]
     AMD Core Performance Counter Ext.:   [ ]
     AMD NB Performance Counter Ext.:     [ ]
     AMD Streaming Performance Monitor:   [ ]
     AMD Data Breakpoint Extension:       [ ]
     AMD Performance TSC:                 [ ]
     AMD L2I Performance Counter Ext.:    [ ]
  Power Management
     ACPI Supported:                      [X]
     Thermal Monitor Supported:           [X]
     Thermal Monitor 2:                   [X]
     Enhanced SpeedStep Technology:       [X]
     Digital Thermal Sensor:              [X]
     Always Running APIC Timer:           [X]
     Invariant TSC:                       [X]
     Power Limit Notification:            [X]
     Extended Clock Modulation Duty:      [X]
     Package Thermal Management:          [X]
     Hardware Coordination Feedback:      [X]
     ACNT2 Capability:                    [ ]
     Performance-Energy Bias:             [ ]
     AMD Temperature Sensor:              [ ]
     AMD Frequency ID Control:            [ ]
     AMD Voltage ID Control:              [ ]
     AMD Thermal Trip:                    [ ]
     AMD Thermal Monitoring:              [ ]
     AMD Software Thermal Control:        [ ]
     AMD 100MHz Multiplier Steps:         [ ]
     AMD Hardware P-State Control:        [ ]
     AMD Effective Frequency Interface:   [ ]
     AMD Processor Feedback Interface:    [ ]
     AMD Processor Accumulator:           [ ]
                               
                  +-----------------------------------------+
                  |                CPU Cache                |
                  +-----------------------------------------+
  Level 1 Instruction Cache
     Size:                     2 x 32 kB
     Associativity:            8-way
     Line Size:                64 byte
     TLB 4K Pages:             
       Number of Entries:      64
       Associativity:          8-way
     TLB 2/4M Pages:           
       Number of Entries:      8
       Associativity:          full
  Level 1 Data Cache
     Size:                     2 x 32 kB
     Associativity:            8-way
     Line Size:                64 byte
     TLB 4K Pages:             
       Number of Entries:      64
       Associativity:          4-way
     TLB 2/4M Pages:           
       Number of Entries:      4
       Associativity:          4-way
  Level 2 Cache
     Size:                     2 x 256 kB
     Associativity:            8-way
     Line Size:                64 byte
  Level 3 Cache
     Size:                     1 x 3 MB
     Associativity:            12-way
     Line Size:                64 byte
                               
                  +-----------------------------------------+
                  |              CPU (SMBIOS)               |
                  +-----------------------------------------+
  Processor 
     Processor Vendor:         Intel
     Processor Version:        Intel(R) Core(TM) i3-4160 CPU @ 3.60GHz
     Current Speed:            3600 MHz
     External Clock:           100 MHz
     Voltage:                  1.1 V
     Processor Upgrade:        Other
     Processor Status:         CPU Enabled
     Socket Designation:       SOCKET 0
     Processor Type:           Central Processor
     Processor Family:         Intel Core i7
     Processor ID1:            000306C3h
     Processor ID2:            BFEBFBFFh
     Max Speed:                7000 MHz
     Socket Status:            CPU Socket Populated
     Serial Number:            
     Asset Tag:                Fill By OEM
     Part Number:              Fill By OEM
     CPU Core Count:           2 (Enabled: 1)
     CPU Thread Count:         2
     Structure Length:         2Ah
                               
                  +-----------------------------------------+
                  |            CPU (SMBIOS) Cache           |
                  +-----------------------------------------+
  Level 1 Cache
     Installed Size:           128 kB
     Operational Mode:         Write Back
     Current SRAM Type:        Unknown
     Status:                   Enabled
     Socket Designation:       CPU Internal L1
     Cache Socketed:           Not Socketed
     Location:                 Internal
     Maximum Cache Size:       128 kB
     Supported SRAM Type:      Unknown
     Cache Speed:              Unknown
     Error Correction:         Single-bit ECC
     System Cache Type:        Other
     Associativity:            8-way Set-Associative
     Structure Length:         13h
  Level 2 Cache
     Installed Size:           512 kB
     Operational Mode:         Write Back
     Current SRAM Type:        Unknown
     Status:                   Enabled
     Socket Designation:       CPU Internal L2
     Cache Socketed:           Not Socketed
     Location:                 Internal
     Maximum Cache Size:       512 kB
     Supported SRAM Type:      Unknown
     Cache Speed:              Unknown
     Error Correction:         Single-bit ECC
     System Cache Type:        Unified
     Associativity:            8-way Set-Associative
     Structure Length:         13h
  Level 3 Cache
     Installed Size:           3072 kB
     Operational Mode:         Write Back
     Current SRAM Type:        Unknown
     Status:                   Enabled
     Socket Designation:       CPU Internal L3
     Cache Socketed:           Not Socketed
     Location:                 Internal
     Maximum Cache Size:       3072 kB
     Supported SRAM Type:      Unknown
     Cache Speed:              Unknown
     Error Correction:         Single-bit ECC
     System Cache Type:        Unified
     Associativity:            12-way Set-Associative
     Structure Length:         13h
                               
                  +-----------------------------------------+
                  |                  BIOS                   |
                  +-----------------------------------------+
  BIOS
     Motherboard Vendor:       Unknown (0001)
     Vendor URL:               Unknown
     BIOS Version:             AMI BIOS 08.00.10
     BIOS Date:                04/13/12
     BIOS Copyright:           04/13/12(C)2010 American Megatrends, Inc. All Rights Reserved
     Motherboard ID:           BIOS Date: 06/19/14 23:14:41 Ver: 04.06.05
     BIOS ID:                  63-0100-000001-00101111-041312-Chipset
     BIOS Size:                512 kB
     Processor:                686
     Chipset ID:               Chipset
     BIOS Revision:            0100
     MP Specification Ver.:    1.4
     MP Table Address:         000Fh:D450h
     Number of CPU/Cores:      2
     DMI/SMBIOS Version:       2.7
     DMI/SMBIOS Structures:    76
     DMI/SMBIOS Address:       000Eh:C070h
  SMBIOS
     BIOS Vendor:              American Megatrends Inc.
     BIOS Version:             F8
     BIOS Date:                06/19/2014
     BIOS ROM Size:            8192 kB
     System BIOS Version:      4.6
     Starting Segment:         F000h
     Current Language:         en|US|iso8859-1
     Number of Languages:      7
     Structure Length:         18h
  Bus Supported
     PCI is Supported:                    [X]
     AGP is Supported:                    [ ]
     USB is Supported:                    [X]
     ISA is Supported:                    [ ]
     VLBus is Supported:                  [ ]
     MCA is Supported:                    [ ]
     EISA is Supported:                   [ ]
     PC Card is Supported:                [ ]
  Boot Options
     Selectable Boot:                     [X]
     Boot From CD:                        [X]
     ATAPI ZIP Drive Boot:                [ ]
     LS-120 Boot:                         [ ]
     BIOS Boot Specification:             [X]
     Boot From PC Card:                   [ ]
     Network Service Boot Supported:      [ ]
     I2O Boot:                            [ ]
     1394 Boot:                           [ ]
  BIOS Features
     BIOS Characteristics:                [X]
     ACPI Supported:                      [X]
     PnP is Supported:                    [ ]
     APM is Supported:                    [ ]
     ESCD Support:                        [ ]
     Enhanced Disk Drive (EDD):           [X]
     BIOS is Upgradeable (Flash):         [X]
     BIOS ROM is Socketed:                [X]
     BIOS Shadowing is Allowed:           [X]
     Smart Battery Supported:             [ ]
     Targeted Content Distribution:       [X]
     UEFI Specification is Supported:     [X]
     Virtual Machine:                     [ ]
     Int 13h - 5.25"/360kB Floppy:        [ ]
     Int 13h - 5.25"/1.2MB Floppy:        [X]
     Int 13h - 3.5"/720kB Floppy:         [X]
     Int 13h - 3.5"/2.88MB Floppy:        [X]
     Int 5h, Print Screen Service:        [X]
     Int 9h, 8042 Keyboard Services:      [X]
     Int 14h, Serial Services:            [X]
     Int 17h, Printer Services:           [X]
     Int 10h, CGA/Mono Video Services:    [ ]
     Int 13h - Floppy for NEC 9800:       [ ]
     Int 13h - Floppy for Toshiba:        [ ]
     NEC PC-98:                           [ ]
  OEM SMBIOS Strings
     To Be Filled By O.E.M.
     To Be Filled By O.E.M.
     To Be Filled By O.E.M.
     To Be Filled By O.E.M.
     To Be Filled By O.E.M.
  Other SMBIOS Structures
     System Boot Information (32)
     Management Device (34)
     Voltage Probe (26)
     Management Device Threshold Data (36)
     Management Device Component (35)
     Temperature Probe (28)
     Management Device Threshold Data (36)
     Management Device Component (35)
     Cooling Device (27)
     Management Device Threshold Data (36)
     Management Device Component (35)
     Cooling Device (27)
     Management Device Threshold Data (36)
     Management Device Component (35)
     Electrical Current Probe (29)
     Management Device Threshold Data (36)
     Management Device Component (35)
     Voltage Probe (26)
     Temperature Probe (28)
     Cooling Device (27)
     Electrical Current Probe (29)
     System Power Supply (39)
     Unknown (41)
     Memory Device Mapped Address (20)
     Memory Device Mapped Address (20)
     Memory Array Mapped Address (19)
     Unknown (136)
     Unknown (131)
                               
                  +-----------------------------------------+
                  |             PCI/AGP Devices             |
                  +-----------------------------------------+
  Bus: 00h, Device: 00h, Function: 00h         
     Vendor (8086h):           Intel Corporation
     Device (0C00h):           4th Gen Core Processor DRAM Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5000h):     Unknown
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 06h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       Intel(R) 4th Gen Core processor DRAM Controller - 0C00
     Device Class:             System
     Device Location:          PCI bus 0, device 0, function 0
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.17514
     Driver Date:              6-21-2006
     Inf File:                 machine.inf
     Hardware ID:              PCI\VEN_8086&DEV_0C00&SUBSYS_50001458&REV_06
     Compatible ID:            PCI\VEN_8086&DEV_0C00&REV_06
                               
  Bus: 00h, Device: 01h, Function: 00h         
     Vendor (8086h):           Intel Corporation
     Device (0C01h):           4th Gen Core/Xeon E3-1200 v3 Processor PCI Express x16 Controller
     Class (06h):              Bridge
     SubClass (04h):           PCI/PCI
     Revision:                 06h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Base I/O Port:            E000h - EFFFh
     Memory Address:           F7E00000h - F7EFFFFFh
     Memory Address:           E0000000h - EFFFFFFFh
     System IRQ:               16
     Interrupt Pin:            INTA#
  PCI-E Capabilities
     PCI Express Version:      2.0
     Device/Port Type:         Root Port of PCI-E Root Complex
     Link Speed:               5.0 GB/s (Current: 2.5 GB/s)
     Link Width:               x16 (Current: x16)
     Link Port Number:         2
     Physical Slot Number:     0
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       PCI standard PCI-to-PCI bridge
     Device Class:             System
     Device Location:          PCI bus 0, device 1, function 0
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.17514
     Driver Date:              6-21-2006
     Inf File:                 machine.inf
     Service Name:             pci
     Hardware ID:              PCI\VEN_8086&DEV_0C01&SUBSYS_50001458&REV_06
     Compatible ID:            PCI\VEN_8086&DEV_0C01&REV_06
                               
  Bus: 00h, Device: 14h, Function: 00h         
     Vendor (8086h):           Intel Corporation
     Device (8C31h):           8 Series/C220 Series Chipset Family USB xHCI Host Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5007h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 05h
     Interface:                30h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Memory Address:           F7F00000h - F7F0FFFFh
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Intel(R) Corporation
     Device Description:       Ðàñøèðÿåìûé õîñò-êîíòðîëëåð Intel(R) USB 3.0
     Device Class:             USB
     Device Location:          PCI bus 0, device 20, function 0
     Driver Provider:          Intel(R) Corporation
     Driver Version:           3.0.2.54
     Driver Date:              10-30-2014
     Inf File:                 oem8.inf
     Service Name:             iusb3xhc
     Hardware ID:              PCI\VEN_8086&DEV_8C31&SUBSYS_50071458&REV_05
     Compatible ID:            PCI\VEN_8086&DEV_8C31&REV_05
                               
  Bus: 00h, Device: 16h, Function: 00h         
     Vendor (8086h):           Intel Corporation
     Device (8C3Ah):           8 Series/C220 Series Chipset Family MEI Controller #1
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (1C3Ah):     Unknown
     Class (07h):              Communication
     SubClass (80h):           Other
     Revision:                 04h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Memory Address:           F7F1A000h - F7F1A00Fh
     System IRQ:               11
     Interrupt Pin:            INTA#
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Intel
     Device Description:       Intel(R) 8 Series/C220 Series Management Engine Interface - 8C3A
     Device Class:             System
     Device Location:          PCI bus 0, device 22, function 0
     Driver Provider:          Intel
     Driver Version:           1.2.3.2005
     Driver Date:              1-2-2014
     Inf File:                 oem14.inf
     Hardware ID:              PCI\VEN_8086&DEV_8C3A&SUBSYS_1C3A1458&REV_04
     Compatible ID:            PCI\VEN_8086&DEV_8C3A&REV_04
                               
  Bus: 00h, Device: 1Ah, Function: 00h         
     Vendor (8086h):           Intel Corporation
     Device (8C2Dh):           8 Series/C220 Series Chipset Family USB Enhanced Host Controller #2
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5006h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 05h
     Interface:                20h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Memory Address:           F7F18000h - F7F183FFh
     System IRQ:               16
     Interrupt Pin:            INTA#
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard USB Host Controller)
     Device Description:       Intel(R) 8 Series/C220 Series  USB EHCI #2 - 8C2D
     Device Class:             USB
     Device Location:          PCI bus 0, device 26, function 0
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.18328
     Driver Date:              6-21-2006
     Inf File:                 usbport.inf
     Service Name:             usbehci
     Hardware ID:              PCI\VEN_8086&DEV_8C2D&SUBSYS_50061458&REV_05
     Compatible ID:            PCI\VEN_8086&DEV_8C2D&REV_05
                               
  Bus: 00h, Device: 1Bh, Function: 00h         
     Vendor (8086h):           Intel Corporation
     Device (8C20h):           8 Series/C220 Series Chipset Family HD Audio Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (A002h):     Unknown
     Class (04h):              Multimedia
     SubClass (03h):           Hi-definition Audio
     Revision:                 05h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Memory Address:           F7F10000h - F7F13FFFh
     System IRQ:               22
     Interrupt Pin:            INTA#
  PCI-E Capabilities
     PCI Express Version:      1.0
     Device/Port Type:         Root Complex Integrated Endpoint
     Link Speed:               Unknown (0) (Current: Unknown (0))
     Link Width:               x0 (Current: x0)
     Link Port Number:         0
     Physical Slot Number:     0
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Microsoft
     Device Description:       High Definition Audio Controller
     Device Class:             System
     Device Location:          PCI bus 0, device 27, function 0
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.17514
     Driver Date:              11-19-2010
     Inf File:                 hdaudbus.inf
     Service Name:             HDAudBus
     Hardware ID:              PCI\VEN_8086&DEV_8C20&SUBSYS_A0021458&REV_05
     Compatible ID:            PCI\VEN_8086&DEV_8C20&REV_05
                               
  Bus: 00h, Device: 1Ch, Function: 00h         
     Vendor (8086h):           Intel Corporation
     Device (8C10h):           8 Series/C220 Series Chipset Family PCI Express Root Port 1
     Class (06h):              Bridge
     SubClass (04h):           PCI/PCI
     Revision:                 D5h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Memory Address:           FFF00000h - 000FFFFFh
     System IRQ:               16
     Interrupt Pin:            INTA#
  PCI-E Capabilities
     PCI Express Version:      2.0
     Device/Port Type:         Root Port of PCI-E Root Complex
     Link Speed:               5.0 GB/s (Current: 2.5 GB/s)
     Link Width:               x1 (Current: x0)
     Link Port Number:         1
     Physical Slot Number:     0
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       Intel(R) 8 Series/C220 Series  PCI Express Root Port #1 - 8C10
     Device Class:             System
     Device Location:          PCI bus 0, device 28, function 0
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.17514
     Driver Date:              6-21-2006
     Inf File:                 machine.inf
     Service Name:             pci
     Hardware ID:              PCI\VEN_8086&DEV_8C10&SUBSYS_50011458&REV_D5
     Compatible ID:            PCI\VEN_8086&DEV_8C10&REV_D5
                               
  Bus: 00h, Device: 1Ch, Function: 02h         
     Vendor (8086h):           Intel Corporation
     Device (8C14h):           8 Series/C220 Series Chipset Family PCI Express Root Port 3
     Class (06h):              Bridge
     SubClass (04h):           PCI/PCI
     Revision:                 D5h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Base I/O Port:            D000h - DFFFh
     Memory Address:           F7D00000h - F7DFFFFFh
     Memory Address:           F0000000h - F00FFFFFh
     System IRQ:               18
     Interrupt Pin:            INTC#
  PCI-E Capabilities
     PCI Express Version:      2.0
     Device/Port Type:         Root Port of PCI-E Root Complex
     Link Speed:               5.0 GB/s (Current: 2.5 GB/s)
     Link Width:               x1 (Current: x1)
     Link Port Number:         3
     Physical Slot Number:     0
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       Intel(R) 8 Series/C220 Series  PCI Express Root Port #3 - 8C14
     Device Class:             System
     Device Location:          PCI bus 0, device 28, function 2
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.17514
     Driver Date:              6-21-2006
     Inf File:                 machine.inf
     Service Name:             pci
     Hardware ID:              PCI\VEN_8086&DEV_8C14&SUBSYS_50011458&REV_D5
     Compatible ID:            PCI\VEN_8086&DEV_8C14&REV_D5
                               
  Bus: 00h, Device: 1Ch, Function: 03h         
     Vendor (8086h):           Intel Corporation
     Device (244Eh):           82801FB Hub Interface to PCI Bridge (ICH6 C0 step)
     Class (06h):              Bridge
     SubClass (04h):           PCI/PCI
     Revision:                 D5h
     Interface:                01h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Base I/O Port:            C000h - CFFFh
     Memory Address:           FFF00000h - 000FFFFFh
     System IRQ:               19
     Interrupt Pin:            INTD#
  PCI-E Capabilities
     PCI Express Version:      2.0
     Device/Port Type:         Root Port of PCI-E Root Complex
     Link Speed:               5.0 GB/s (Current: 2.5 GB/s)
     Link Width:               x1 (Current: x1)
     Link Port Number:         4
     Physical Slot Number:     0
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Intel
     Device Description:       Intel(R) 82801 PCI Bridge - 244E
     Device Class:             System
     Device Location:          PCI bus 0, device 28, function 3
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.17514
     Driver Date:              6-21-2006
     Inf File:                 machine.inf
     Service Name:             pci
     Hardware ID:              PCI\VEN_8086&DEV_244E&SUBSYS_50011458&REV_D5
     Compatible ID:            PCI\VEN_8086&DEV_244E&REV_D5
                               
  Bus: 00h, Device: 1Dh, Function: 00h         
     Vendor (8086h):           Intel Corporation
     Device (8C26h):           8 Series/C220 Series Chipset Family USB Enhanced Host Controller #1
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5006h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 05h
     Interface:                20h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Memory Address:           F7F17000h - F7F173FFh
     System IRQ:               23
     Interrupt Pin:            INTA#
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard USB Host Controller)
     Device Description:       Intel(R) 8 Series/C220 Series  USB EHCI #1 - 8C26
     Device Class:             USB
     Device Location:          PCI bus 0, device 29, function 0
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.18328
     Driver Date:              6-21-2006
     Inf File:                 usbport.inf
     Service Name:             usbehci
     Hardware ID:              PCI\VEN_8086&DEV_8C26&SUBSYS_50061458&REV_05
     Compatible ID:            PCI\VEN_8086&DEV_8C26&REV_05
                               
  Bus: 00h, Device: 1Fh, Function: 00h         
     Vendor (8086h):           Intel Corporation
     Device (8C5Ch):           H81 Chipset LPC Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5001h):     Unknown
     Class (06h):              Bridge
     SubClass (01h):           PCI/ISA
     Revision:                 05h
     Interface:                00h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       Intel(R) H81 LPC Controller - 8C5C
     Device Class:             System
     Device Location:          PCI bus 0, device 31, function 0
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.17514
     Driver Date:              6-21-2006
     Inf File:                 machine.inf
     Service Name:             msisadrv
     Hardware ID:              PCI\VEN_8086&DEV_8C5C&SUBSYS_50011458&REV_05
     Compatible ID:            PCI\VEN_8086&DEV_8C5C&REV_05
                               
  Bus: 00h, Device: 1Fh, Function: 02h         
     Vendor (8086h):           Intel Corporation
     Device (8C02h):           8 Series/C220 Series Chipset Family 6-Port SATA AHCI Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (B005h):     Unknown
     Class (01h):              Storage
     SubClass (06h):           Serial ATA
     Revision:                 05h
     Interface:                01h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Base I/O Port:            0000F070h - 0000F077h
     Base I/O Port:            0000F060h - 0000F063h
     Base I/O Port:            0000F050h - 0000F057h
     Base I/O Port:            0000F040h - 0000F043h
     Base I/O Port:            0000F020h - 0000F03Fh
     Memory Address:           F7F16000h - F7F167FFh
     System IRQ:               19
     Interrupt Pin:            INTB#
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Standard AHCI 1.0 Serial ATA Controller
     Device Description:       Intel(R) 8 Series/C220 Series  SATA AHCI Controller - 8C02
     Device Class:             hdc
     Device Location:          PCI bus 0, device 31, function 2
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.18231
     Driver Date:              6-21-2006
     Inf File:                 mshdc.inf
     Service Name:             msahci
     Hardware ID:              PCI\VEN_8086&DEV_8C02&SUBSYS_B0051458&REV_05
     Compatible ID:            PCI\VEN_8086&DEV_8C02&REV_05
                               
  Bus: 00h, Device: 1Fh, Function: 03h         
     Vendor (8086h):           Intel Corporation
     Device (8C22h):           8 Series/C220 Series Chipset Family SMBus Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5001h):     Unknown
     Class (0Ch):              Serial
     SubClass (05h):           SMBus Controller
     Revision:                 05h
     Interface:                00h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [ ]
     I/O Access:               [X]
     Bus Master:               [ ]
     66 MHz Speed Support:     [ ]
  Device Resources
     SMBus Port:               F000h
     Memory Address:           F7F15000h - F7F150FFh
     Base I/O Port:            0000F000h - 0000F01Fh
     System IRQ:               4
     Interrupt Pin:            INTC#
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Intel
     Device Description:       Intel(R) 8 Series/C220 Series  SMBus Controller - 8C22
     Device Class:             System
     Device Location:          PCI bus 0, device 31, function 3
     Driver Provider:          Intel
     Driver Version:           10.0.13.0
     Driver Date:              2-25-2014
     Inf File:                 oem2.inf
     Hardware ID:              PCI\VEN_8086&DEV_8C22&SUBSYS_50011458&REV_05
     Compatible ID:            PCI\VEN_8086&DEV_8C22&REV_05
                               
  Bus: 01h, Device: 00h, Function: 00h         
     Vendor (1002h):           ATI Technologies Inc
     Device (6819h):           Pitcairn PRO [Radeon HD 7800 Series]
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (2553h):     Unknown
     Class (03h):              Display
     SubClass (00h):           VGA
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Memory Address:           E0000000h - EFFFFFFFh
     Memory Address:           F7E00000h - F7E3FFFFh
     Base I/O Port:            0000E000h - 0000E0FFh
  PCI-E Capabilities
     PCI Express Version:      2.0
     Device/Port Type:         Legacy PCI-E Endpoint
     Link Speed:               8.0 GB/s (Current: 2.5 GB/s)
     Link Width:               x16 (Current: x16)
     Link Port Number:         0
     Physical Slot Number:     0
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Advanced Micro Devices, Inc.
     Device Description:       AMD Radeon HD 7800 Series
     Device Class:             Display
     Device Location:          PCI bus 1, device 0, function 0
     Driver Provider:          Advanced Micro Devices, Inc.
     Driver Version:           14.501.1003.0
     Driver Date:              11-20-2014
     Inf File:                 oem15.inf
     Service Name:             amdkmdap
     Hardware ID:              PCI\VEN_1002&DEV_6819&SUBSYS_25531458&REV_00
     Compatible ID:            PCI\VEN_1002&DEV_6819&REV_00
                               
  Bus: 01h, Device: 00h, Function: 01h         
     Vendor (1002h):           ATI Technologies Inc
     Device (AAB0h):           Cape Verde/Pitcairn HDMI Audio [Radeon HD 7700/7800 Series]
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (AAB0h):     Unknown
     Class (04h):              Multimedia
     SubClass (03h):           Hi-definition Audio
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Memory Address:           F7E60000h - F7E63FFFh
     System IRQ:               17
     Interrupt Pin:            INTB#
  AC'97/HDA Capabilities
     AC'97/HDA Codec Name:     ATI R6xx HDMI
  PCI-E Capabilities
     PCI Express Version:      2.0
     Device/Port Type:         Legacy PCI-E Endpoint
     Link Speed:               8.0 GB/s (Current: 2.5 GB/s)
     Link Width:               x16 (Current: x16)
     Link Port Number:         0
     Physical Slot Number:     0
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Microsoft
     Device Description:       High Definition Audio Controller
     Device Class:             System
     Device Location:          PCI bus 1, device 0, function 1
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.17514
     Driver Date:              11-19-2010
     Inf File:                 hdaudbus.inf
     Service Name:             HDAudBus
     Hardware ID:              PCI\VEN_1002&DEV_AAB0&SUBSYS_AAB01458&REV_00
     Compatible ID:            PCI\VEN_1002&DEV_AAB0&REV_00
                               
  Bus: 03h, Device: 00h, Function: 00h         
     Vendor (10ECh):           Realtek Semiconductor
     Device (8168h):           RTL8111/8168/8411 PCI Express Gigabit Ethernet Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (E000h):     GA-EP45-DS5 Motherboard
     Class (02h):              Network
     SubClass (00h):           Ethernet
     Revision:                 06h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Base I/O Port:            0000D000h - 0000D0FFh
     Memory Address:           F7D00000h - F7D00FFFh
     Memory Address:           F0000000h - F0003FFFh
  PCI-E Capabilities
     PCI Express Version:      2.0
     Device/Port Type:         PCI-E Endpoint
     Link Speed:               2.5 GB/s (Current: 2.5 GB/s)
     Link Width:               x1 (Current: x1)
     Link Port Number:         0
     Physical Slot Number:     0
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Realtek
     Device Description:       Realtek PCIe GBE Family Controller
     Device Class:             Net
     Device Location:          PCI bus 3, device 0, function 0
     Driver Provider:          Realtek
     Driver Version:           7.90.826.2014
     Driver Date:              8-26-2014
     Inf File:                 oem9.inf
     Service Name:             RTL8167
     Hardware ID:              PCI\VEN_10EC&DEV_8168&SUBSYS_E0001458&REV_06
     Compatible ID:            PCI\VEN_10EC&DEV_8168&REV_06
                               
  Bus: 04h, Device: 00h, Function: 00h         
     Vendor (8086h):           Intel Corporation
     Device (244Eh):           82801 Family (ICH2/3/4/5/6/7/8/9,63xxESB) Hub Interface to PCI Bridge
     Class (06h):              Bridge
     SubClass (04h):           PCI/PCI
     Revision:                 41h
     Interface:                01h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Base I/O Port:            C000h - CFFFh
     Memory Address:           FFF00000h - 000FFFFFh
     System IRQ:               19
     Interrupt Pin:            INTA#
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Intel
     Device Description:       Intel(R) 82801 PCI Bridge - 244E
     Device Class:             System
     Device Location:          PCI bus 4, device 0, function 0
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.17514
     Driver Date:              6-21-2006
     Inf File:                 machine.inf
     Service Name:             pci
     Hardware ID:              PCI\VEN_8086&DEV_244E&SUBSYS_88921458&REV_41
     Compatible ID:            PCI\VEN_8086&DEV_244E&REV_41
                               
  Bus: 05h, Device: 01h, Function: 00h         
     Vendor (1102h):           Creative Labs
     Device (0004h):           EMU10K2 Audio Chipset (SB Audigy Series)
     Subsys Vendor (1102h):    Creative Labs
     Subsystem ID (2005h):     Unknown
     Class (04h):              Multimedia
     SubClass (01h):           Audio
     Revision:                 04h
     Interface:                00h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [ ]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Base I/O Port:            0000C000h - 0000C03Fh
     System IRQ:               16
     Interrupt Pin:            INTA#
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Creative Technology, Ltd.
     Device Description:       Creative Audigy Audio Processor (WDM)
     Friendly Name:            Creative SB Audigy 2 ZS (WDM)
     Device Class:             MEDIA
     Device Location:          PCI bus 5, device 1, function 0
     Driver Provider:          Creative
     Driver Version:           6.0.301.39
     Driver Date:              3-13-2014
     Inf File:                 oem11.inf
     Service Name:             ctaud2k
     Hardware ID:              PCI\VEN_1102&DEV_0004&SUBSYS_20051102&REV_04
     Compatible ID:            PCI\VEN_1102&DEV_0004&REV_04
                               
                  +-----------------------------------------+
                  |              Memory Modules             |
                  +-----------------------------------------+
  Memory Slot 1
     Memory Type:              2048MB DDR3-1333 (PC3-10600) SDRAM
     Manufacturer:             Kingston
     Module Type:              Unbuffered DIMM
     Number of Ranks/Banks:    1 Ranks, 8 Banks
     Module Attributes:        Unbuffered
     Error Checking:           None
     CAS# Latency:             9.0 (Cycle Time: 1.500ns/686MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 9.0-9-9-24)
                               (tWR-tRC: 10-33)
     CAS# Latency:             8.0 (Cycle Time: 1.371ns/610MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 8.0-8-8-22)
                               (tWR-tRC: 10-30)
     CAS# Latency:             7.0 (Cycle Time: 1.200ns/533MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 7.0-7-7-20)
                               (tWR-tRC: 8-27)
     CAS# Latency:             6.0 (Cycle Time: 1.029ns/457MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 6.0-6-6-17)
                               (tWR-tRC: 7-23)
     Refresh Rate:             7.8 us (2X 85-95 C)
     Data Width:               64 bits
     SDRAM Width:              x8
     Voltage Interface:        1.5 V
     Max Case Temperature:     95 °C (203 °F)
     SPD Revision:             1.0
     Part Number:              99U5474-010.A00LF 
     Manufacturing Location:   5
     Manufacture Date:         June 2012 (1238h)
     Serial Number:            92275739h
     Revision Code:            None
     EPP Support:              [ ]
     XMP Support:              [ ]
                               
  Memory Slot 3
     Memory Type:              2048MB DDR3-1333 (PC3-10600) SDRAM
     Manufacturer:             Kingston
     Module Type:              Unbuffered DIMM
     Number of Ranks/Banks:    1 Ranks, 8 Banks
     Module Attributes:        Unbuffered
     Error Checking:           None
     CAS# Latency:             9.0 (Cycle Time: 1.500ns/686MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 9.0-9-9-24)
                               (tWR-tRC: 10-33)
     CAS# Latency:             8.0 (Cycle Time: 1.371ns/610MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 8.0-8-8-22)
                               (tWR-tRC: 10-30)
     CAS# Latency:             7.0 (Cycle Time: 1.200ns/533MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 7.0-7-7-20)
                               (tWR-tRC: 8-27)
     CAS# Latency:             6.0 (Cycle Time: 1.029ns/457MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 6.0-6-6-17)
                               (tWR-tRC: 7-23)
     Refresh Rate:             7.8 us (2X 85-95 C)
     Data Width:               64 bits
     SDRAM Width:              x8
     Voltage Interface:        1.5 V
     Max Case Temperature:     95 °C (203 °F)
     SPD Revision:             1.0
     Part Number:              99U5474-010.A00LF 
     Manufacturing Location:   5
     Manufacture Date:         June 2012 (1238h)
     Serial Number:            8D276A39h
     Revision Code:            None
     EPP Support:              [ ]
     XMP Support:              [ ]
                               
                  +-----------------------------------------+
                  |             Memory (SMBIOS)             |
                  +-----------------------------------------+
  Physical Memory Array 1
     Maximum Capacity:         32768 MB
     Location:                 System Board or Motherboard
     Use:                      System Memory
     Memory Error Correct.:    None
     Memory Devices:           2
     Structure Length:         17h
  Memory Device 1
     Size:                     2048 MB
     Form Factor:              DIMM
     Memory Type:              DDR3
     Speed:                    1333 MHz
     Configured Speed:         1333 MHz
     Device Locator:           ChannelA-DIMM0
     Bank Locator:             BANK 0
     Total Width:              64 bits
     Data Width:               64 bits
     Device Set:               00h
     Type Detail:              Synchronous
     Manufacturer:             Kingston
     Serial Number:            92275739
     Asset Tag:                9876543210
     Part Number:              99U5474-010.A00LF
     Structure Length:         22h
  Memory Device 2
     Size:                     Not Installed
     Form Factor:              DIMM
     Memory Type:              Unknown
     Speed:                    Unknown
     Device Locator:           ChannelA-DIMM1
     Bank Locator:             BANK 1
     Total Width:              0 bits
     Data Width:               0 bits
     Device Set:               00h
     Type Detail:              None
     Manufacturer:             [Empty]
     Serial Number:            [Empty]
     Asset Tag:                9876543210
     Part Number:              [Empty]
     Structure Length:         22h
  Memory Device 3
     Size:                     2048 MB
     Form Factor:              DIMM
     Memory Type:              DDR3
     Speed:                    1333 MHz
     Configured Speed:         1333 MHz
     Device Locator:           ChannelB-DIMM0
     Bank Locator:             BANK 2
     Total Width:              64 bits
     Data Width:               64 bits
     Device Set:               00h
     Type Detail:              Synchronous
     Manufacturer:             Kingston
     Serial Number:            8D276A39
     Asset Tag:                9876543210
     Part Number:              99U5474-010.A00LF
     Structure Length:         22h
  Memory Device 4
     Size:                     Not Installed
     Form Factor:              DIMM
     Memory Type:              Unknown
     Speed:                    Unknown
     Device Locator:           ChannelB-DIMM1
     Bank Locator:             BANK 3
     Total Width:              0 bits
     Data Width:               0 bits
     Device Set:               00h
     Type Detail:              None
     Manufacturer:             [Empty]
     Serial Number:            [Empty]
     Asset Tag:                9876543210
     Part Number:              [Empty]
     Structure Length:         22h
                               
                  +-----------------------------------------+
                  |                   HDD                   |
                  +-----------------------------------------+
  Primary/Master HDD
     HDD Model:                SSD Smartbuy 60GB
     HDD Size:                 57241 MB (55.90 GB)
     Interface Type:           Serial ATA III (SATA/600)
     Form Factor:              2.5"
     Rotation Rate:            SSD
     Geometry:                 Heads: 16, Sectors: 63, Tracks: 16383
     Compatibility:            ATA8-ACS
     Serial Number:            DA5A07471EEE00690280
     Controller Revision:      S8FM07.7
     HDD Marketing Size:       60022 MB (60.02 GB)
     Buffer Size:              Unknown
     Buffer Type:              Not Specified
     Reallocated Sectors:      0
     HDD Health Status:        Good
     SSD Remaining Life:       100 %
     Total Host Writes:        1520.0 GB
     ECC bytes:                None
     Security Erase Time:      60 min
     Enh. Security Erase:      60 min
     Current APM Value:        None
     Acoustic Management:      None
     Device Location:          Primary/Master
  Transfer Modes
     SATA Speed:               600 MB/s, Active: 600 MB/s
     PIO Mode Support:         4
     SW DMA Mode Support:      Not Supported
     MW DMA Mode Support:      2, Active: None
     UDMA Mode Support:        6 (UltraDMA/133), Active: 5 (UltraDMA/100)
     Sectors per Interrupt:    16, Active: 16
  HDD Features
     SATA NCQ Command:                    [X]
     SSD TRIM Command:                    [X]
     DMA Transfer:                        [X]
     LBA Supported:                       [X]
     Block Mode:                          [X]
     Double Word I/O:                     [X]
     Standard Standby Timer:              [X]
     IORDY Supported:                     [X]
     IORDY may be Disabled:               [X]
     S.M.A.R.T.:                          [X] enabled
     S.M.A.R.T. Self-test:                [X] enabled
     S.M.A.R.T. Error Logging:            [X] enabled
     Security Mode Feature Set:           [X] disabled
     Removable Media:                     [ ]
     Power Management:                    [X] enabled
     PACKET Command:                      [ ]
     Write Cache:                         [X] enabled
     Look-ahead:                          [X] enabled
     Release Interrupt:                   [ ]
     Service Interrupt:                   [ ]
     Device Reset Command:                [ ]
     Host Protected Area:                 [X] enabled
     Write Verify Command:                [ ]
     Write Buffer Command:                [X] enabled
     Read Buffer Command:                 [X] enabled
     NOP Command:                         [ ]
     Identify Device DMA Command:         [ ]
     Download Microcode Command:          [X] enabled
     Read/Write DMA Queued:               [ ]
     CFA Feature Set:                     [ ]
     Advanced Power Management:           [X] disabled
     Removable Media Status:              [ ]
     Power-up in Standby:                 [ ]
     Set Features Req. to Spinup:         [ ]
     Set Max Security Extension:          [X] disabled
     Automatic Acoustic Management:       [ ]
     48-bit Address:                      [X] enabled
     Device Configuration Overlay:        [X] enabled
     Flush Cache Command:                 [X] enabled
     Flush Cache Ext Command:             [X] enabled
     Media Serial Number:                 [ ]
     Media Card Pass Through:             [ ]
     Streaming Feature Set:               [ ]
     General Purpose Logging:             [X] enabled
     Write DMA/Multiple FUA EXT:          [X] enabled
     Write DMA Queued FUA EXT:            [ ]
     World Wide Name:                     [ ]
  S.M.A.R.T.
     ID  | Attribute Name            |Threshold|Worst|Value| Raw Value
     ----+---------------------------+---------+-----+-----+-----------
     1   | Raw Read Error Rate       |       50|  100|  100|     0
     9   | Power On Hours Count      |        0|  100|  100|  1107
     12  | Drive Power Cycle Count   |        0|  100|  100|   793
     168 | SATA PHY Error Count      |        0|  100|  100| 1210307
     170 | Available Reserved Space  |       10|  100|  100|   193
     173 | Average Erase Count       |        0|  100|  100| 3539092
     192 | Unsafe Shutdown Count     |        0|  100|  100|    27
     218 | Vendor Specific           |       50|  100|  100|  1301
     241 | Total Host Writes         |        0|  100|  100|  1520
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard disk drives)
     Device Description:       Disk drive
     Friendly Name:            SSD Smartbuy 60GB ATA Device
     Device Class:             DiskDrive
     Device Location:          Channel 0, Target 0, Lun 0
     Driver Provider:          Microsoft
     Driver Version:           6.1.7600.16385
     Driver Date:              6-21-2006
     Inf File:                 disk.inf
     Service Name:             disk
     Hardware ID:              IDE\DiskSSD_Smartbuy_60GB_______________________S8FM07.7
     Compatible ID:            GenDisk
                               
  Secondary/Master HDD
     HDD Model:                WDC WD1001FALS-00J7B0
     HDD Size:                 953869 MB (931.51 GB)
     Interface Type:           Serial ATA II (SATA/300)
     Geometry:                 Heads: 16, Sectors: 63, Tracks: 16383
     Compatibility:            ATA8-ACS
     Serial Number:            WD-WMATV0357962
     Controller Revision:      05.00K05
     HDD Marketing Size:       1000204 MB (1000.20 GB)
     Buffer Size:              32 MB
     Buffer Type:              Not Specified
     HDD Temperature:          43 °C (109 °F)
     Reallocated Sectors:      0
     HDD Health Status:        Good
     ECC bytes:                50
     Security Erase Time:      194 min
     Enh. Security Erase:      194 min
     Current APM Value:        None
     Acoustic Management:      80h (80h Recommended) - Enabled
     Device Location:          Secondary/Master
  Transfer Modes
     SATA Speed:               300 MB/s
     PIO Mode Support:         4
     SW DMA Mode Support:      Not Supported
     MW DMA Mode Support:      2, Active: None
     UDMA Mode Support:        6 (UltraDMA/133), Active: 5 (UltraDMA/100)
     Sectors per Interrupt:    16, Active: 16
  HDD Features
     SATA NCQ Command:                    [X]
     SSD TRIM Command:                    [ ]
     DMA Transfer:                        [X]
     LBA Supported:                       [X]
     Block Mode:                          [X]
     Double Word I/O:                     [ ]
     Standard Standby Timer:              [X]
     IORDY Supported:                     [X]
     IORDY may be Disabled:               [X]
     S.M.A.R.T.:                          [X] enabled
     S.M.A.R.T. Self-test:                [X] enabled
     S.M.A.R.T. Error Logging:            [X] enabled
     Security Mode Feature Set:           [X] disabled
     Removable Media:                     [ ]
     Power Management:                    [X] enabled
     PACKET Command:                      [ ]
     Write Cache:                         [X] enabled
     Look-ahead:                          [X] enabled
     Release Interrupt:                   [ ]
     Service Interrupt:                   [ ]
     Device Reset Command:                [ ]
     Host Protected Area:                 [X] enabled
     Write Verify Command:                [ ]
     Write Buffer Command:                [X] enabled
     Read Buffer Command:                 [X] enabled
     NOP Command:                         [X] enabled
     Identify Device DMA Command:         [ ]
     Download Microcode Command:          [X] enabled
     Read/Write DMA Queued:               [ ]
     CFA Feature Set:                     [ ]
     Advanced Power Management:           [ ]
     Removable Media Status:              [ ]
     Power-up in Standby:                 [X] disabled
     Set Features Req. to Spinup:         [X] enabled
     Set Max Security Extension:          [X] disabled
     Automatic Acoustic Management:       [X] enabled
     48-bit Address:                      [X] enabled
     Device Configuration Overlay:        [X] enabled
     Flush Cache Command:                 [X] enabled
     Flush Cache Ext Command:             [X] enabled
     Media Serial Number:                 [ ]
     Media Card Pass Through:             [ ]
     Streaming Feature Set:               [ ]
     General Purpose Logging:             [X] enabled
     Write DMA/Multiple FUA EXT:          [ ]
     Write DMA Queued FUA EXT:            [ ]
     World Wide Name:                     [X] enabled
  S.M.A.R.T.
     ID  | Attribute Name            |Threshold|Worst|Value| Raw Value
     ----+---------------------------+---------+-----+-----+-----------
     1   | Raw Read Error Rate       |       51|  200|  200|     0
     3   | Spin-up Time              |       21|  253|  253|  5483
     4   | Start/Stop Count          |        0|   90|   90| 10384
     5   | Reallocated Sectors Count |      140|  200|  200|     0
     7   | Seek Error Rate           |       51|  200|  200|     0
     9   | Power On Hours Count      |        0|   73|   73| 19809
     10  | Spin-up Retry Count       |       51|  100|  100|     0
     11  | Recalibration Retries     |       51|  100|  100|     0
     12  | Drive Power Cycle Count   |        0|   90|   90| 10100
     192 | Power-Off Retract Count   |        0|  198|  198|  1714
     193 | Load/Unload Cycle Count   |        0|  197|  197| 10382
     194 | Drive Temperature         |        0|   89|  107|    43
     196 | Reallocation Event Count  |        0|  200|  200|     0
     197 | Current Pending Sectors   |        0|  200|  200|     0
     198 | Uncorrectable Sectors     |        0|  200|  200|     0
     199 | UltraDMA CRC Error Rate   |        0|  200|  200|   312
     200 | Write Error Rate          |       51|  200|  200|     0
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard disk drives)
     Device Description:       Disk drive
     Friendly Name:            WDC WD1001FALS-00J7B0 ATA Device
     Device Class:             DiskDrive
     Device Location:          Channel 1, Target 0, Lun 0
     Driver Provider:          Microsoft
     Driver Version:           6.1.7600.16385
     Driver Date:              6-21-2006
     Inf File:                 disk.inf
     Service Name:             disk
     Hardware ID:              IDE\DiskWDC_WD1001FALS-00J7B0___________________05.00K05
     Compatible ID:            GenDisk
                               
                  +-----------------------------------------+
                  |              Storage (ASPI)             |
                  +-----------------------------------------+
     ASPI devices not found
                               
                  +-----------------------------------------+
                  |              Logical Drives             |
                  +-----------------------------------------+
  Local Drives
  C:[SYSTEM]
     Drive Letter:             C:
     Drive Type:               Fixed Disk
     Volume Label:             SYSTEM
     File System:              FAT
     Volume Serial Number:     2255-1BEA
     Total Size:               2047.0 MB
     Free Space:               402.1 MB (19.6%)
  D:[UTILITIES]
     Drive Letter:             D:
     Drive Type:               Fixed Disk
     Volume Label:             UTILITIES
     File System:              FAT
     Volume Serial Number:     2E4A-1BEB
     Total Size:               2047.1 MB
     Free Space:               113.5 MB (5.5%)
  E:[INSTALL]
     Drive Letter:             E:
     Drive Type:               Fixed Disk
     Volume Label:             INSTALL
     File System:              NTFS
     Volume Serial Number:     08B6-AD4A
     Total Size:               53.0 GB
     Free Space:               146.5 MB (0.3%)
  F:[WIN10]
     Drive Letter:             F:
     Drive Type:               Fixed Disk
     Volume Label:             WIN10
     File System:              NTFS
     Volume Serial Number:     E804-72DE
     Total Size:               30.0 GB
     Free Space:               8.5 GB (28.3%)
  G:[WIN7]
     Drive Letter:             G:
     Drive Type:               Fixed Disk
     Volume Label:             WIN7
     File System:              NTFS
     Volume Serial Number:     48B9-FCDB
     Total Size:               55.9 GB
     Free Space:               2.7 GB (4.8%)
  H:[MUSIC]
     Drive Letter:             H:
     Drive Type:               Fixed Disk
     Volume Label:             MUSIC
     File System:              NTFS
     Volume Serial Number:     38D2-852D
     Total Size:               834.5 GB
     Free Space:               36.4 GB (4.4%)
  I:[WINXP]
     Drive Letter:             I:
     Drive Type:               Fixed Disk
     Volume Label:             WINXP
     File System:              NTFS
     Volume Serial Number:     A297-0D56
     Total Size:               10.0 GB
     Free Space:               5.9 GB (58.6%)
                               
                  +-----------------------------------------+
                  |               USB Devices               |
                  +-----------------------------------------+
  USB Device 1
     Vendor (8087h):           Intel Corp.
     Device (8000h):           Integrated Rate Matching Hub
     Manufacturer:             
     Product:                  
     Serial Number:            
     Device Version:           0.05
     Class (09h):              Hub
     SubClass (00h):           Unused
     Protocol (01h):           Single TT
     Configuration:            
     USB Version:              2.00
     Speed:                    480 Mb/s
     Transfer Type:            Interrupt
     Data Packet Size:         64 bytes
     Max Power:                Remote Wakeup
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Generic USB Hub)
     Device Description:       Generic USB Hub
     Device Class:             USB
     Device Location:          Port_#0001.Hub_#0002
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.18328
     Driver Date:              6-21-2006
     Inf File:                 usb.inf
     Service Name:             usbhub
     Hardware ID:              USB\VID_8087&PID_8000&REV_0005
     Compatible ID:            USB\Class_09&SubClass_00&Prot_00
  Interface 1
     Class (09h):              Hub
     SubClass (00h):           Unused
     Protocol (00h):           Full Speed (or Root) Hub
     Interface:                
                               
  USB Device 2
     Vendor (8087h):           Intel Corp.
     Device (8008h):           Integrated Rate Matching Hub
     Manufacturer:             
     Product:                  
     Serial Number:            
     Device Version:           0.05
     Class (09h):              Hub
     SubClass (00h):           Unused
     Protocol (01h):           Single TT
     Configuration:            
     USB Version:              2.00
     Speed:                    480 Mb/s
     Transfer Type:            Interrupt
     Data Packet Size:         64 bytes
     Max Power:                Remote Wakeup
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Generic USB Hub)
     Device Description:       Generic USB Hub
     Device Class:             USB
     Device Location:          Port_#0001.Hub_#0001
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.18328
     Driver Date:              6-21-2006
     Inf File:                 usb.inf
     Service Name:             usbhub
     Hardware ID:              USB\VID_8087&PID_8008&REV_0005
     Compatible ID:            USB\Class_09&SubClass_00&Prot_00
  Interface 1
     Class (09h):              Hub
     SubClass (00h):           Unused
     Protocol (00h):           Full Speed (or Root) Hub
     Interface:                
                               
  USB Device 3
     Vendor (0458h):           KYE Systems Corp. (Genius)
     Device (002Ch):           Wireless TwinTouch Optical Office
     Manufacturer:             KYE SYSTEMS CORP.
     Product:                  Wireless TwinTouch Optical Office
     Serial Number:            
     Device Version:           1.13
     Class (00h):              Unknown
     SubClass (00h):           Unknown
     Protocol (00h):           Unknown
     Configuration:            HID Keyboard / Mouse
     USB Version:              1.10
     Speed:                    Low (1.5 Mb/s)
     Transfer Type:            Interrupt
     Data Packet Size:         8 bytes
     Max Power:                100 mA Remote Wakeup
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard USB Host Controller)
     Device Description:       USB Composite Device
     Device Class:             USB
     Device Location:          Port_#0004.Hub_#0001
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.18328
     Driver Date:              6-21-2006
     Inf File:                 usb.inf
     Service Name:             usbccgp
     Hardware ID:              USB\VID_0458&PID_002C&REV_010D
     Compatible ID:            IUSB3\DevClass_00&SubClass_00&Prot_00
  Interface 1
     Class (03h):              Human Interface Devices
     SubClass (01h):           Boot Interface Subclass
     Protocol (01h):           Keyboard
     Interface:                EP1 Interrupt
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       USB Input Device
     Device Class:             HIDClass
     Device Location:          0000.0014.0000.004.000.000.000.000.000
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.18199
     Driver Date:              6-21-2006
     Inf File:                 input.inf
     Service Name:             HidUsb
     Hardware ID:              USB\VID_0458&PID_002C&REV_010D&MI_00
     Compatible ID:            USB\Class_03&SubClass_01&Prot_01
  Interface 2
     Class (03h):              Human Interface Devices
     SubClass (01h):           Boot Interface Subclass
     Protocol (02h):           Mouse
     Interface:                EP2 Interrupt
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       USB Input Device
     Device Class:             HIDClass
     Device Location:          0000.0014.0000.004.000.000.000.000.000
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.18199
     Driver Date:              6-21-2006
     Inf File:                 input.inf
     Service Name:             HidUsb
     Hardware ID:              USB\VID_0458&PID_002C&REV_010D&MI_01
     Compatible ID:            USB\Class_03&SubClass_01&Prot_02
                               
  USB Device 4
     Vendor (0458h):           KYE Systems Corp. (Genius)
     Device (003Ah):           Scroll Mouse
     Manufacturer:             Genius
     Product:                  USB Optical Mouse
     Serial Number:            
     Device Version:           1.00
     Class (00h):              Unknown
     SubClass (00h):           Unknown
     Protocol (00h):           Unknown
     Configuration:            
     USB Version:              2.00
     Speed:                    480 Mb/s
     Transfer Type:            Interrupt
     Data Packet Size:         8 bytes
     Max Power:                100 mA Remote Wakeup
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             (Standard system devices)
     Device Description:       USB Input Device
     Device Class:             HIDClass
     Device Location:          Port_#0006.Hub_#0001
     Driver Provider:          Microsoft
     Driver Version:           6.1.7601.18199
     Driver Date:              6-21-2006
     Inf File:                 input.inf
     Service Name:             HidUsb
     Hardware ID:              USB\VID_0458&PID_003A&REV_0100
     Compatible ID:            USB\Class_03&SubClass_01&Prot_02
  Interface 1
     Class (03h):              Human Interface Devices
     SubClass (01h):           Boot Interface Subclass
     Protocol (02h):           Mouse
     Interface:                
                               
                  +-----------------------------------------+
                  |            Physical Printers            |
                  +-----------------------------------------+
     LPT/PnP or USB printer not found
                               
                  +-----------------------------------------+
                  |            Installed Printers           |
                  +-----------------------------------------+
  Local Printers
  Installed Printer 1
     Printer Name:             Microsoft XPS Document Writer
     Printer Port:             XPSPort:
     Default Printer:          Yes
     Printer Type:             Local
     Print Processor:          winprint
     Data Type:                RAW
                               
  Installed Printer 2
     Printer Name:             Fax
     Printer Port:             SHRFAX:
     Default Printer:          No
     Printer Type:             Local
     Print Processor:          winprint
     Data Type:                RAW
                               
                  +-----------------------------------------+
                  |              Slots (SMBIOS)             |
                  +-----------------------------------------+
  Slot PCI Express
     Slot Type:                PCI Express
     Current Usage:            In Use
     Data Bus Width:           16x or x16
     Slot Designation:         J6B2
     Slot Length:              Long Length
     Slot ID:                  0
  Slot PCI Express
     Slot Type:                PCI Express
     Current Usage:            In Use
     Data Bus Width:           1x or x1
     Slot Designation:         J6B1
     Slot Length:              Short Length
     Slot ID:                  1
  Slot PCI Express
     Slot Type:                PCI Express
     Current Usage:            In Use
     Data Bus Width:           8x or x8
     Slot Designation:         J6D1
     Slot Length:              Short Length
     Slot ID:                  2
  Slot PCI Express
     Slot Type:                PCI Express
     Current Usage:            In Use
     Data Bus Width:           16x or x16
     Slot Designation:         J7B1
     Slot Length:              Short Length
     Slot ID:                  3
  Slot PCI Express
     Slot Type:                PCI Express
     Current Usage:            In Use
     Data Bus Width:           1x or x1
     Slot Designation:         J8B4
     Slot Length:              Short Length
     Slot ID:                  4
  Slot PCI
     Slot Type:                PCI
     Current Usage:            In Use
     Data Bus Width:           32 bit
     Slot Designation:         J8B3
     Slot Length:              Short Length
     Slot ID:                  6
                               
                  +-----------------------------------------+
                  |              Ports (SMBIOS)             |
                  +-----------------------------------------+
  Port 1 Mouse Port
     Int. Connector Type:      None
     Ext. Connector Type:      PS/2
     Port Type:                Mouse Port
     Int. Designator:          J1A1
     Ext. Designator:          PS2Mouse
  Port 2 Keyboard Port
     Int. Connector Type:      None
     Ext. Connector Type:      PS/2
     Port Type:                Keyboard Port
     Int. Designator:          J1A1
     Ext. Designator:          Keyboard
  Port 3 Other
     Int. Connector Type:      None
     Ext. Connector Type:      Mini-Centronics Type-14
     Port Type:                Other
     Int. Designator:          J2A1
     Ext. Designator:          TV Out
  Port 4 Serial Port 16550A Compatible
     Int. Connector Type:      None
     Ext. Connector Type:      DB-9 pin male
     Port Type:                Serial Port 16550A Compatible
     Int. Designator:          J2A2A
     Ext. Designator:          COM A
  Port 5 Video Port
     Int. Connector Type:      None
     Ext. Connector Type:      DB-15 pin female
     Port Type:                Video Port
     Int. Designator:          J2A2B
     Ext. Designator:          Video
  Port 6 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          J3A1
     Ext. Designator:          USB1
  Port 7 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          J3A1
     Ext. Designator:          USB2
  Port 8 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          J3A1
     Ext. Designator:          USB3
  Port 9 Other
     Int. Connector Type:      Other
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          J9A1 - TPM HDR
     Ext. Designator:          
  Port 10 Other
     Int. Connector Type:      Other
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          J9C1 - PCIE DOCKING CONN
     Ext. Designator:          
  Port 11 Other
     Int. Connector Type:      Other
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          J2B3 - CPU FAN
     Ext. Designator:          
  Port 12 Other
     Int. Connector Type:      Other
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          J6C2 - EXT HDMI
     Ext. Designator:          
  Port 13 Other
     Int. Connector Type:      Other
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          J3C1 - GMCH FAN
     Ext. Designator:          
  Port 14 Other
     Int. Connector Type:      Other
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          J1D1 - ITP
     Ext. Designator:          
  Port 15 Other
     Int. Connector Type:      Other
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          J9E2 - MDC INTPSR
     Ext. Designator:          
  Port 16 Other
     Int. Connector Type:      Other
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          J9E4 - MDC INTPSR
     Ext. Designator:          
  Port 17 Other
     Int. Connector Type:      Other
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          J9E3 - LPC HOT DOCKING
     Ext. Designator:          
  Port 18 Other
     Int. Connector Type:      Other
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          J9E1 - SCAN MATRIX
     Ext. Designator:          
  Port 19 Other
     Int. Connector Type:      Other
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          J9G1 - LPC SIDE BAND
     Ext. Designator:          
  Port 20 Other
     Int. Connector Type:      Other
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          J8F1 - UNIFIED
     Ext. Designator:          
  Port 21 Other
     Int. Connector Type:      Other
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          J6F1 - LVDS
     Ext. Designator:          
  Port 22 Other
     Int. Connector Type:      Other
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          J2F1 - LAI FAN
     Ext. Designator:          
  Port 23 Other
     Int. Connector Type:      Other
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          J2G1 - GFX VID
     Ext. Designator:          
  Port 24 Other
     Int. Connector Type:      Other
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          J1G6 - AC JACK
     Ext. Designator:          
                               
                  +-----------------------------------------+
                  |                 Network                 |
                  +-----------------------------------------+
  Network
     Network Name:             A2KKV
     User Name:                kkv1
     User Role:                Administrator
     Logon Domain:             A2KKV
  Interface 1
     Description:              TAP-Windows Adapter V9
     MAC Address:              00-FF-CA-D1-AF-0D
     Adapter Type:             Ethernet
     Link Speed:               100.0 Mbps
     MTU Size:                 1500 byte
     Adapter Status:           Enabled
     Operational Status:       Non Operational
     DHCP Server:              Unknown
     Gateway:                  0.0.0.0
  Interface 2
     Adapter Vendor:           Realtek Semiconductor
     Adapter Name:             RTL8111/8168/8411 PCI Express Gigabit Ethernet Controller
     Subsys Vendor:            Giga-Byte Technology
     Subsystem ID:             GA-EP45-DS5 Motherboard
     Bus Type:                 PCI-E
     Description:              Realtek PCIe GBE Family Controller
     MAC Address:              74-D4-35-CD-93-A8
     Adapter Type:             Ethernet
     Link Speed:               100.0 Mbps
     MTU Size:                 1500 byte
     Adapter Status:           Enabled
     Operational Status:       Operational
     DHCP Server:              192.168.1.1
     IP Address:               192.168.1.141
     IP Address Subnet Mask:   255.255.255.0
     Gateway:                  192.168.1.1
     DNS Server:               192.168.1.1
                               
                  +-----------------------------------------+
                  |                 Monitor                 |
                  +-----------------------------------------+
  Monitor
     Monitor Vendor:           LG Electronics Inc.
     Monitor Model:            LG FLATRON F920P
     Viewable Size:            17.7" (45.0 sm)
     Serial Number:            319823
     Manufacture Date:         March 2005
     EDID Version:             1.3
     Monitor ID:               GSM4A88
     Aspect Ratio:             4:3
     Horizontal Size:          36 sm
     Vertical Size:            27 sm
     Gamma Factor:             2.910
     Display Type:             RGB Color
     Input Signal:             Analog
     Internal Model:           F920P
     Vertical Frequency:       50-160 Hz
     Horizontal Frequency:     30-111 kHz
  DPMS Features
     Active Off:               [X]
     Suspend:                  [X]
     Standby:                  [X]
  Supported Modes
     Mode 1:                   720x400   @ 70 Hz (VGA)
     Mode 2:                   720x400   @ 88 Hz (XGA2)
     Mode 3:                   640x480   @ 60 Hz (VGA)
     Mode 4:                   640x480   @ 67 Hz (Mac II)
     Mode 5:                   640x480   @ 72 Hz (VESA)
     Mode 6:                   640x480   @ 75 Hz (VESA)
     Mode 7:                   800x600   @ 56 Hz (VESA)
     Mode 8:                   800x600   @ 60 Hz (VESA)
     Mode 9:                   800x600   @ 72 Hz (VESA)
     Mode 10:                  800x600   @ 75 Hz (VESA)
     Mode 11:                  832x624   @ 75 Hz (Mac II)
     Mode 12:                  1024x768  @ 87 Hz (interlaced)
     Mode 13:                  1024x768  @ 60 Hz (VESA)
     Mode 14:                  1024x768  @ 70 Hz (VESA)
     Mode 15:                  1024x768  @ 75 Hz (VESA)
     Mode 16:                  1280x1024 @ 75 Hz (VESA)
     Mode 17:                  1920x1440 @ 70 Hz
     Mode 18:                  2048x1536 @ 60 Hz
     Mode 19:                  1024x768  @ 120 Hz
     Mode 20:                  1280x1024 @ 100 Hz
     Mode 21:                  1280x1024 @ 85 Hz
     Mode 22:                  1600x1200 @ 75 Hz
     Mode 23:                  1600x1200 @ 85 Hz
     Mode 24:                  1152x864  @ 120 Hz
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             LGE
     Device Description:       LGE F920P (GSM4A88 EDID Override)
     Device Class:             Monitor
     Driver Provider:          EnTech Taiwan
     Driver Version:           1.0.0.0
     Inf File:                 oem4.inf
     Service Name:             monitor
     Hardware ID:              MONITOR\GSM4A88
     Compatible ID:            *PNP09FF
                               
                  +-----------------------------------------+
                  |                  Video                  |
                  +-----------------------------------------+
  Video
     Video Chip Vendor:        ATI Technologies Inc
     Video Chip:               Pitcairn PRO [Radeon HD 7800 Series]
     Subsystem Vendor:         Giga-Byte Technology
     Video Memory Size:        2 GB
     Video BIOS Version:       015.021.000.003
     Video BIOS Date:          2012/08/05 21:33
     Part Number:              113-xxx-xxx
     Core Temperature:         35 °C (95 °F)
     Current Core Clock:       300 MHz
     Current Memory Clock:     150 MHz
     Core Voltage:             0.825 V
     Core Usage:               0 %
     Performance Level:        0
     Bus Type:                 PCI-E
  PCI-E Capabilities
     PCI Express Version:      2.0
     Device/Port Type:         Legacy PCI-E Endpoint
     Link Speed:               8.0 GB/s (Current: 2.5 GB/s)
     Link Width:               x16 (Current: x16)
     Link Port Number:         0
     Physical Slot Number:     0
  Driver
     Driver Status:            The device is working properly
     Manufacturer:             Advanced Micro Devices, Inc.
     Device Description:       AMD Radeon HD 7800 Series
     Device Class:             Display
     Device Location:          PCI bus 1, device 0, function 0
     Driver Provider:          Advanced Micro Devices, Inc.
     Driver Version:           14.501.1003.0
     Driver Date:              11-20-2014
     Inf File:                 oem15.inf
     Service Name:             amdkmdap
     Hardware ID:              PCI\VEN_1002&DEV_6819&SUBSYS_25531458&REV_00
     Compatible ID:            PCI\VEN_1002&DEV_6819&REV_00
                               
                  +-----------------------------------------+
                  |           Hardware Monitoring           |
                  +-----------------------------------------+
  Processor 
     Processor:                Intel Core i3-4160 3600 MHz
     Core Voltage:             0.925 V
     Package Temperature:      38 °C (100 °F)
  Core 1
     Temperature Core:         36 °C (97 °F)
     Core Clock:               1696.1 MHz (Original: 3600 MHz)
     FSB Clock:                99.8 MHz
     Multiplier:               17.0
  Core 2
     Temperature Core:         38 °C (100 °F)
     Core Clock:               3591.7 MHz (Original: 3600 MHz)
     FSB Clock:                99.8 MHz
     Multiplier:               36.0
  Video Card 
     Video Chip:               Pitcairn PRO [Radeon HD 7800 Series]
     Core Temperature:         35 °C (95 °F)
     Current Core Clock:       300 MHz
     Current Memory Clock:     150 MHz
     Core Voltage:             0.825 V
     Core Usage:               0 %
     Performance Level:        0
  Disk Drive 1 
     HDD Model:                SSD Smartbuy 60GB
     Total Host Writes:        1520.0 GB
  Disk Drive 2 
     HDD Model:                WDC WD1001FALS-00J7B0
     HDD Temperature:          43 °C (109 °F)
                               
                  +-----------------------------------------+
                  |          Drivers Troubleshooter         |
                  +-----------------------------------------+
  List of Problem Devices
     All devices are working properly
                               
                  +-----------------------------------------+
                  |             HDD Diagnostics             |
                  +-----------------------------------------+
  HDD 1 Status
     HDD Model:                SSD Smartbuy 60GB
     HDD Size:                 57241 MB (55.90 GB)
     Interface Type:           Serial ATA III (SATA/600)
     Serial Number:            DA5A07471EEE00690280
     Controller Revision:      S8FM07.7
     HDD Marketing Size:       60022 MB (60.02 GB)
     Buffer Size:              Unknown
     Device Location:          Primary/Master
     Reallocated Sectors:      0
     HDD Health Status:        Good
     SSD Remaining Life:       100 %
     Total Host Writes:        1520.0 GB
                               
  HDD 2 Status
     HDD Model:                WDC WD1001FALS-00J7B0
     HDD Size:                 953869 MB (931.51 GB)
     Interface Type:           Serial ATA II (SATA/300)
     Serial Number:            WD-WMATV0357962
     Controller Revision:      05.00K05
     HDD Marketing Size:       1000204 MB (1000.20 GB)
     Buffer Size:              32767.5 kB
     Device Location:          Secondary/Master
     HDD Temperature:          43 °C (109 °F)
     Reallocated Sectors:      0
     HDD Health Status:        Good
                               
                  +-----------------------------------------+
                  |                 Windows                 |
                  +-----------------------------------------+
  Windows
     Operating System:         MS Windows 7 Ultimate x64 Edition (6.1.7601 Service Pack 1)
     OS Language:              Russian (Russia)
     Windows Folder:           G:\Windows
     Installation Date:        December 18, 2014
     Kernel Type:              Multiprocessor Free
     Registered Owner:         kkv1
     Registered Organization:  Microsoft
     Product ID:               00426-OEM-8992662-00400
     Product Key:              XXXXX-XXXXX-XXXXX-XXXXX-XXXXX
     System UpTime:            0 Hour(s) 5 Minutes 16 Seconds
     IE Version:               9.11.9600.17691
     DirectX Version:          DirectX 11
  Regional Settings
     Country:                  Russia
     Language:                 Russian
     Time Zone:                Russia TZ 2 Standard Time (GMT+3)
     Currency Name:            Russian Ruble
     Measurment System:        Metric
     ANSI Code Page:           1251
     OEM Code Page:            866
                               
                  +-----------------------------------------+
                  |            Installed Programs           |
                  +-----------------------------------------+
  Installed Programs
     Program Name                                       | Version        |                      Publisher|       Date|      Size| 
     ---------------------------------------------------+----------------+-------------------------------+-----------+----------+------
     ASTRA32 - Advanced System Information Tool         | 3.23           |                    Sysinfo Lab|           |          | 
     Mozilla Firefox (x86 ru)                           | 37.0.2         |                        Mozilla|           |   84.7 MB| 
     OpenOffice 4.1.1                                   | 4.11.9775      |     Apache Software Foundation| 22.01.2015|  332.4 MB| 
     OpenVPN                                            | 2.3.6-I601     |                               |           |          | 
     Realtek Ethernet Controller Driver                 | 7.90.826.2014  |                        Realtek| 18.12.2014|          | 
     Realtek High Definition Audio Driver               | 6.0.1.7246     |    Realtek Semiconductor Corp.| 22.01.2015|          | 
     Sound Blaster Audigy 2 ZS                          | 1.0            |    Creative Technology Limited|           |          | 
     TAP-Windows                                        | 9.21.1         |                               |           |          | 
     WinCDEmu                                           | 4.0            |                       Sysprogs|           |          | 
     foobar2000                                         | 1.3.7          |                Peter Pawlowski|           |     18 MB| 
                               
                  +-----------------------------------------+
                  |            Installed Hotfixes           |
                  +-----------------------------------------+
  Installed Hotfixes
     Hotfix for Microsoft Windows (KB2534111):18.12.2014
     Hotfix for Microsoft Windows (KB2847077):18.12.2014
     Hotfix for Microsoft Windows (KB2977728):
     Hotfix for Microsoft Windows (KB3006137):
     Hotfix for Microsoft Windows (KB3009736):                              

                                [End of Report]                               
