## FujiFilm Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | Version | undef |
> 0x0010 | InternalSerialNumber | string | (this number is unique, and contains the date of manufacture, but doesn't necessarily correspond to the camera body number -- this needs to be checked)
> 0x1000 | Quality | string |
> 0x1001 | Sharpness | int16u |
> 0x1 = Soft 0x2 = Soft2 0x3 = Normal 0x4 = Hard 0x5 = Hard2 0x82 = Medium Soft 0x84 = Medium Hard 0x8000 = Film Simulation 0xffff = n/a |
> 0x1002 | WhiteBalance | int16u |
> 0x0 = Auto 0x100 = Daylight 0x200 = Cloudy 0x300 = Daylight Fluorescent 0x301 = Day White Fluorescent 0x302 = White Fluorescent 0x303 = Warm White Fluorescent 0x304 = Living Room Warm White Fluorescent 0x400 = Incandescent 0x500 = Flash 0x600 = Underwater 0xf00 = Custom 0xf01 = Custom2 0xf02 = Custom3 0xf03 = Custom4 0xf04 = Custom5 0xff0 = Kelvin |
> 0x1003 | Saturation | int16u |
> 0x0 = Normal 0x80 = Medium High 0x100 = High 0x180 = Medium Low 0x200 = Low 0x300 = None (B&W) 0x301 = B&W Red Filter 0x302 = B&W Yellow Filter 0x303 = B&W Green Filter 0x310 = B&W Sepia 0x400 = Low 2 0x8000 = Film Simulation |
> 0x1004 | Contrast | int16u |
> 0x0 = Normal 0x80 = Medium High 0x100 = High 0x180 = Medium Low 0x200 = Low 0x8000 = Film Simulation |
> 0x1005 | ColorTemperature | int16u |
> 0x1006 | Contrast | int16u | 0x0 = Normal 0x100 = High 0x300 = Low
> 0x100a | WhiteBalanceFineTune | int32s[2] |
> 0x100b | NoiseReduction | int16u | 0x40 = Low 0x80 = Normal 0x100 = n/a
> 0x100e | HighISONoiseReduction | int16u | 0x0 = Normal 0x100 = Strong 0x180 = Medium Strong 0x200 = Weak 0x280 = Medium Weak
> 0x1010 | FujiFlashMode | int16u | 0 = Auto 1 = On 2 = Off 3 = Red-eye reduction 4 = External
> 0x1011 | FlashExposureComp | rational64s |
> 0x1020 | Macro | int16u | 0 = Off 1 = On
> 0x1021 | FocusMode | int16u | 0 = Auto 1 = Manual
> 0x1022 | AFPointSet | int16u | ("No" for manual and AF-multi focus modes) 0 = No 1 = Yes
> 0x1023 | FocusPixel | int16u[2] |
> 0x1030 | SlowSync | int16u | 0 = Off 1 = On
> 0x1031 | PictureMode | int16u |
> 0x0 = Auto 0x1 = Portrait 0x2 = Landscape 0x3 = Macro 0x4 = Sports 0x5 = Night Scene 0x6 = Program AE 0x7 = Natural Light 0x8 = Anti-blur 0x9 = Beach & Snow 0xa = Sunset 0xb = Museum 0xc = Party 0xd = Flower 0xe = Text 0xf = Natural Light & Flash 0x10 = Beach 0x11 = Snow 0x12 = Fireworks 0x13 = Underwater 0x14 = Portrait with Skin Correction 0x16 = Panorama 0x17 = Night (tripod) 0x18 = Pro Low-light 0x19 = Pro Focus 0x1a = Portrait 2 0x1b = Dog Face Detection 0x1c = Cat Face Detection 0x40 = Advanced Filter 0x100 = Aperture-priority AE 0x200 = Shutter speed priority AE 0x300 = Manual |
> 0x1032 | ExposureCount | int16u | (number of exposures used for this image)
> 0x1033 | EXRAuto | int16u | 0 = Auto 1 = Manual
> 0x1034 | EXRMode | int16u | 0x100 = HR (High Resolution) 0x200 = SN (Signal to Noise priority) 0x300 = DR (Dynamic Range priority)
> 0x1040 | ShadowTone | int32s | -32 = Hard -16 = Medium-hard 0 = Normal 16 = Medium-soft 32 = Soft
> 0x1041 | HighlightTone | int32s | -32 = Hard -16 = Medium-hard 0 = Normal 16 = Medium-soft 32 = Soft
> 0x1050 | ShutterType | int16u | 0 = Mechanical 1 = Electronic
> 0x1100 | AutoBracketing | int16u | 0 = Off 1 = On 2 = No flash & flash
> 0x1101 | SequenceNumber | int16u |
> 0x1201 | AdvancedFilter | int32u |
> 0x10000 = Pop Color 0x20000 = Hi Key 0x30000 = Toy Camera 0x40000 = Miniature 0x50000 = Dynamic Tone 0x60001 = Partial Color Red 0x60002 = Partial Color Yellow 0x60003 = Partial Color Green 0x60004 = Partial Color Blue 0x60005 = Partial Color Orange 0x60006 = Partial Color Purple 0x70000 = Soft Focus 0x90000 = Low Key |
> 0x1210 | ColorMode | int16u | 0x0 = Standard 0x10 = Chrome 0x30 = B & W
> 0x1300 | BlurWarning | int16u | 0 = None 1 = Blur Warning
> 0x1301 | FocusWarning | int16u | 0 = Good 1 = Out of focus
> 0x1302 | ExposureWarning | int16u | 0 = Good 1 = Bad exposure
> 0x1304 | GEImageSize | string | (GE models only)
> 0x1400 | DynamicRange | int16u | 1 = Standard 3 = Wide
> 0x1401 | FilmMode | int16u | 0x0 = F0/Standard (Provia) 0x100 = F1/Studio Portrait 0x110 = F1a/Studio Portrait Enhanced Saturation 0x120 = F1b/Studio Portrait Smooth Skin Tone (Astia) 0x130 = F1c/Studio Portrait Increased Sharpness 0x200 = F2/Fujichrome (Velvia) 0x300 = F3/Studio Portrait Ex 0x400 = F4/Velvia 0x500 = Pro Neg. Std 0x501 = Pro Neg. Hi 0x600 = Classic Chrome
> 0x1402 | DynamicRangeSetting | int16u |
> 0x0 = Auto (100-400%) 0x1 = Manual 0x100 = Standard (100%) 0x200 = Wide1 (230%) 0x201 = Wide2 (400%) 0x8000 = Film Simulation |
> 0x1403 | DevelopmentDynamicRange | int16u |
> 0x1404 | MinFocalLength | rational64s |
> 0x1405 | MaxFocalLength | rational64s |
> 0x1406 | MaxApertureAtMinFocal | rational64s |
> 0x1407 | MaxApertureAtMaxFocal | rational64s |
> 0x140b | AutoDynamicRange | int16u |
> 0x1422 | ImageStabilization | int16u[3] | [Value 0] 0 = None 1 = Optical 2 = Sensor-shift 512 = Digital [Value 1] 0 = Off 1 = On (mode 1, continuous) 2 = On (mode 2, shooting only)
> 0x1431 | Rating | int32u |
> 0x1436 | ImageGeneration | int16u | 0 = Original Image 1 = Re-developed from RAW
> 0x3820 | FrameRate | int16u |
> 0x3821 | FrameWidth | int16u |
> 0x3822 | FrameHeight | int16u |
> 0x4100 | FacesDetected | int16u |
> 0x4103 | FacePositions | int16u[n] | (left, top, right and bottom coordinates in full-sized image for each face detected)
> 0x4282 | FaceRecInfo | - | --> FujiFilm FaceRecInfo Tags
> 0x8000 | FileSource | string |
> 0x8002 | OrderNumber | int32u |
> 0x8003 | FrameNumber | int16u |
> 0xb211 | Parallax | rational64s | (only found in MPImage2 of .MPO images)

## FujiFilm FaceRecInfo Tags

Face recognition information.

> Tag Name | Writable | Values / Notes
> --- | --- | ---
> Face1Birthday | N |
> Face1Category | N | Bit 1 = Partner Bit 2 = Family Bit 3 = Friend
> Face1Name | N |
> Face2Birthday | N |
> Face2Category | N | Bit 1 = Partner Bit 2 = Family Bit 3 = Friend
> Face2Name | N |
> Face3Birthday | N |
> Face3Category | N | Bit 1 = Partner Bit 2 = Family Bit 3 = Friend
> Face3Name | N |
> Face4Birthday | N |
> Face4Category | N | Bit 1 = Partner Bit 2 = Family Bit 3 = Friend
> Face4Name | N |
> Face5Birthday | N |
> Face5Category | N | Bit 1 = Partner Bit 2 = Family Bit 3 = Friend
> Face5Name | N |
> Face6Birthday | N |
> Face6Category | N | Bit 1 = Partner Bit 2 = Family Bit 3 = Friend
> Face6Name | N |
> Face7Birthday | N |
> Face7Category | N | Bit 1 = Partner Bit 2 = Family Bit 3 = Friend
> Face7Name | N |
> Face8Birthday | N |
> Face8Category | N | Bit 1 = Partner Bit 2 = Family Bit 3 = Friend
> Face8Name | N |

## FujiFilm RAF Tags

FujiFilm RAF images contain meta information stored in a proprietary FujiFilm RAF format, as well as EXIF information stored inside an embedded JPEG preview image. The table below lists tags currently decoded from the RAF-format information.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0100 | RawImageFullSize | N | (including borders)
> 0x0121 | RawImageSize | N |
> 0x0130 | FujiLayout | N |
> 0x2000 | WB_GRGBLevelsAuto | N |
> 0x2100 | WB_GRGBLevelsDaylight | N |
> 0x2200 | WB_GRGBLevelsCloudy | N |
> 0x2300 | WB_GRGBLevelsDaylightFluor | N |
> 0x2301 | WB_GRGBLevelsDayWhiteFluor | N |
> 0x2302 | WB_GRGBLevelsWhiteFluorescent | N |
> 0x2310 | WB_GRGBLevelsWarmWhiteFluor | N |
> 0x2311 | WB_GRGBLevelsLivingRoomWarmWhiteFluor | N |
> 0x2400 | WB_GRGBLevelsTungsten | N |
> 0x2ff0 | WB_GRGBLevels | N |
> 0xc000 | RAFData | - | --> FujiFilm RAFData Tags

## FujiFilm RAFData Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | RawImageWidth | N |
> 4 | RawImageWidth RawImageHeight | N N |
> 8 | RawImageHeight | N |

## FujiFilm IFD Tags

Tags found in the FujiIFD information of RAF images from some models.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0xf000 | FujiIFD | - | --> FujiFilm IFD Tags
> 0xf001 | RawImageFullWidth | N |
> 0xf002 | RawImageFullHeight | N |
> 0xf003 | BitsPerSample | N |
> 0xf007 | StripOffsets | N |
> 0xf008 | StripByteCounts | N |
> 0xf00a | BlackLevel | N |
> 0xf00c | WB_GRBLevelsStandard | N |
> 0xf00d | WB_GRBLevelsDaylight | N |
> 0xf00e | WB_GRBLevels | N |

## FujiFilm FFMV Tags

Information found in the FFMV atom of MOV videos.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | MovieStreamName | N |

## FujiFilm MOV Tags

This information is found in MOV videos from some FujiFilm cameras.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | N |
> 24 | Model | N |
> 46 | ExposureTime | N |
> 50 | FNumber | N |
> 58 | ExposureCompensation | N |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Dec 19, 2014

<-- ExifTool Tag Names