****************************************************************************
		    Fast Ethernet Controller Provider Inc.
		       PCI 10/100 Fast Ethernet Adapter

	      NDIS 3 Miniport Driver For Windows 95 Installation
	      ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

	   Copyright (C) 2000 Fast Ethernet Controller Provider Inc.
			     All rights reserved.
****************************************************************************

The driver conforms to the Network Driver Interface Specification(NDIS) 3.1, 
and used with Microsoft Windows 95, Windows 95 OSR2


Contents
--------
    A) Installing NDIS 3 Miniport driver on Microsoft Windows 95
    B) Installing NDIS 3 Miniport driver on Microsoft Windows 95 OSR2
    C) Configuring NDIS 3 Miniport driver on Microsoft Windows 95 (OSR2)


A) Installing NDIS 3 Miniport driver on Microsoft Windows 95
============================================================
  1. Plug the PCI 10/100 Fast Ethernet Adapter into one of the Master PCI 
     slots of your PCI platform.

  2. Turn ON the power of PC then boot from Windows 95.

  3. Windows95 will prompt "PCI Ethernet Controller" in "New Hardware Found"
     dialog box.

  4. Select "Driver from disk provided by hardware manufacturer" from 
     "New Hardware Found" dialog box, then click OK button.

  5. Insert the PCI 10/100 Fast Ethernet Adapter Driver Diskette in your 
     floppy drive.

  6. Enter the driver pathname, i.e. A:\WIN95 (or B:\WIN95), then click OK 
     button from "Install from Disk" dialog box.

  7. Follow the screen's prompt, insert "Windows 95 CD-ROM" and click
     OK button from "Insert Disk" dialog box.

  8. Otherwise enter the full pathname of the "Windows 95 CD-ROM" 
     installation files in "Copying Files..." dialog box, then click OK 
     button.

  9. Windows 95 will copy the driver (FastNIC.SYS) from A:\WIN95 to 
     C:\WINDOWS\SYSTEM directory and the FastNIC.INF file from A:\WIN95 to 
     C:\WINDOWS\INF directory.

 10. Remove the FPCI 10/100 Fast Ethernet Adapter Driver Diskette from your
     floppy drive.

 11. Restart your computer for the network function to take effective.


NOTICE!!
  C:\WINDOWS is the directory where your Windows 95 O.S. is located.


B) Installing NDIS 3 Miniport driver on Microsoft Windows 95 OSR2
=================================================================
  1. Plug the PCI 10/100 Fast Ethernet Adapter into one of the Master PCI 
     slots of your PCI platform.

  2. Turn ON the power of PC then boot from Windows 95.

  3. Windows 95 will prompt "PCI Ethernet Controller" in "New Hardware Found"
     dialog box and "Update Device Driver Wizard" dialog box.

  4. Insert the PCI 10/100 Fast Ethernet Adapter Driver Diskette in your 
     floppy drive.

  5. Click "Next" button from "Update Device Driver Wizard" dialog box.

  6. Click "Other location" button from "Update Device Driver Wizard" dialog
     box.

  7. Type "A:\Win95" from "Select other location".

  8. Windows 95 will prompt "PCI 10/100 Fast Ethernet Adapter" in 
     "Update Device Driver Wizard" dialog box.

  9. Click "Finish" button from "Update Device Driver Wizard" dialog box.

 10. Click OK button when the screen prompts the following message;
       "Please insert 'PCI 10/100 Fast Ethernet Adapter Driver Diskette'"

 11. Enter the full pathname "A:\WIN95" of the FastNIC.INF file, then click 
     OK button from "Copying Files..." dialog box.

 12. Following the screen's prompt, insert "Windows 95 CD-ROM" and click 
     OK button from "Insert Disk" dialog box.

 13. Windows 95 will copy the driver(FastNIC.SYS) from A:\WIN95 to 
     C:\WINDOWS\SYSTEM directory and the FastNIC.INF file from A:\WIN95 to
     C:\WINDOWS\INF directory.
 
 14. Remove the PCI 10/100 Fast Ethernet Adapter Driver Diskette from your 
     floppy drive.

 15. Restart your computer for the network function to take effect.


NOTICE!!
  C:\WINDOWS is the directory where your Windows 95 OSR2 O.S. is located.



C) Configuring NDIS 3 Miniport driver on Microsoft Windows 95(OSR2)
===================================================================
  1. Click the "My Computer" icon in the Main Program Group.

  2. Click the "Control Panel" icon from My Computer window.

  3. Click the "Network" icon from the Control Panel window.

  4. Select "PCI 10/100 Fast Ethernet Adapter" item from "Network" dialog 
     box, then click "Properties" button.

  5. Click "Advanced" button from "PCI 10/100 Fast Ethernet Adapter" dialog 
     box.

  6. Select the Media Type value (AutoDetect, 10BaseT, 10BaseT Full_Duplex,
     100BaseTX, 100BaseTX Full_Duplex) from "Value" item, then click OK 
     button from "PCI 10/100 Fast Ethernet Adapter Properties" dialog box.

  7. Click OK button from "Network" dialog box.

  8. Restart your computer to implement the new configuration.




Trademarks:
Microsoft Windows 95 is a trademark of Microsoft Corporation.
