
        Legend/D-Link DFE-530TX PCI Fast Ethernet Adapter Installation
                   for Banyan Vines


 Getting Started
 ---------------
    There are two methods of copying files from the Banyan VINES
    workstation to the bootable diskette or subdirectory on the hard
    disk.

    Method 1
    --------
    - Execute the 'INSTALL' command included in the diskette labeled
      "VINES MASTER DISK".

    - Follow the given instructions for copying files.

    Method 2
    --------
    - Execute the 'BAN' command.

    - Login to VINES system.

    - Execute the 'PCCOPY' command.

    - Select the 'NDIS Ethernet' option and follow the instructions for
      copying files.

    - Prepared bootable diskette in Drive B. Then, copy the appropriate
      NDIS driver file DLKFET.DOS to Drive B.

    - Create a CONFIG.SYS file with the following statements:

        DEVICE=PROTMAN.DOS /I:A:\
        DEVICE=DLKFET.DOS

      NOTE:  A:\ is the path where Banyan VINES workstation files reside.

    - Create a DLKFET.NIF file containing the following statements:



        Model = Legend/D-Link DFE-530TX PCI Fast Ethernet Adapter
        Path = A:\
        DeviceDriver = DLKFET.DOS
        DeviceName = DLKFET$
        Type = NDIS

      NOTE:  A:\ is the path where Banyan VINES workstation files reside.

    - Create a PROTOCOL.INI file with the following lines:

        [PROTOCOL MANAGER]
        drivername = PROTMAN$

        [VINES_XIF]
        drivername = NDISBAN$
        bindings = "DLKFET"

        [DLKFET]
        drivername = DLKFET$

    - Execute the 'PCCONFIG' command.

      A "CONFIGURING A PC FOR THE NETWORK" message appears on the
      screen. The program then provides some options you can select.

    - Select "1 - Network Card Settings".

      Another screen appears for selecting some options.

    - Select "NDIS Ethernet".

    - Select the appropriate configuration of the adapter.

    - After configuring the adapter, you return to the main screen.

      Select "2 - Login Environment Settings".

    - From the next screen, select "NDIS Ethernet".

      The 'PCCONFIG.DB' file will then be created.

    - Reboot your computer.

    - Login to VINES by executing the 'BAN' command.
