****************************************************************************
		    Fast Ethernet Controller Provider Inc.
		       PCI 10/100 Fast Ethernet Adapter

			  NDIS 2 Driver Installation
			  ~~~~~~~~~~~~~~~~~~~~~~~~~~

	   Copyright (C) 1999 Fast Ethernet Controller Provider Inc.
			     All rights reserved.
****************************************************************************
 

The drivers you need are in the directories MSLANMAN.DOS, MSLANMAN.OS2 and
NDIS.  The NDIS drivers contained in these subdirectories are used with 3Com
3+Open, Microsoft OS/2 LAN Manager OEM distribution, Release 1.x or 2.x,
and other compatible OEM versions of LAN Manager.  The driver can also be 
used with IBM LAN Server 3.0, 4.0, Banyan VINES, ARTISOFT LANtastic 5.0, 6.0,
Wollongong Pathway Access, Microsoft Windows for Workgroups v3.11, DEC 
PATHWORKS, Sun PC-NFS etc.



The drivers named FastNIC conform to the Network Driver Interface 
Specification (NDIS) defined by Microsoft/3Com.

Included in MSLANMAN.DOS, and NDIS subdirectories are the following files:

\MSLANMAN.DOS\DRIVERS\Fast\FastNIC\

	FastNIC.DOS		The DOS NDIS MAC driver
	PROTOCOL.INI		A sample section of PROTOCOL.INI file

\MSLANMAN.DOS\DRIVERS\NIF\

	FastNIC.NIF		Network Information File

\MSLANMAN.OS2\DRIVERS\Fast\FastNIC\

	FastNIC.OS2		The OS2 NDIS MAC driver
	PROTOCOL.INI		A sample section of PROTOCOL.INI file

\MSLANMAN.OS2\DRIVERS\NIF\

	FastNIC.NIF		Network Information File


\NDIS\

	NDIS.TXT		This readme file

	WFW311.TXT		The Installation guide for Windows for
				Workgroups v3.11

	LANMAN.TXT		The Installation guide for LAN Manager

	LANSVR.TXT		The Installation guide for Lan Server

	BANYAN.TXT		The Installation guide for Banyan VINES

	LANTASTI.TXT		The Installation guide for ARTISOFT 
				LANtastic 5.0, 6.0

	PATHWORK.TXT		The Installation guide for DEC PATHWORKS

	PCNFS.TXT		The Installation guide for Sun PC-NFS


\NDIS\DOS\

	FastNIC.NIF		Network Information File for IBM Lan Support
				Program
	FastNIC.DOS		The DOS NDIS 2 driver
	OEMSETUP.INF		Network Information File for Windows for 
				Workgroups v3.11
	PROTOCOL.INI		A sample section of PROTOCOL.INI file


\NDIS\OS2\

	FastNICO.NIF		Network Information File for IBM LAN Server
				3.0, 4.0
	FastNIC.OS2		The OS2 NDIS 2 driver
	PROTOCOL.INI		A sample section of PROTOCOL.INI file


Sample PROTOCOL.INI Files and Parameters
----------------------------------------
[ETHPCI_NIF]

  DriverName = FSTNIC$
; Slot = 1            ;; {1-4}
; SIA_Mode = AUTODETECT
; {SIA_Mode = UTP, UTP_FD,UTP_100,UTP_100FD, AUTODETECT}

There are several parameters included in the ETHPCI_NIF section of the
PROTOCOL.INI file. However, the only parameter that you should specify
is the "drivername."

If you change other parameter settings, such as the SIA_MODE, make sure
that it matches the hardware settings.  Otherwise, the adapter may fail.

If you don't specify these settings, Fast Ethernet Controller Provider's 
NDIS 2 driver will automatically detect them.


SLOT	  Specifies which network adapter is used by the driver. If you have 
	  only one Fast Ethernet Controller Provider's FastNIC PCI Adapter 
	  in your machine, this parameter is unnecessary!  For two or more 
	  Fast Ethernet Controller Provider's PCI LAN cards, this parameter
	  is required and cannot be omitted from PROTOCOL.INI. For the first
	  FastNIC adapter, Slot=1, and the second one, Slot=2, third, Slot=3
	  ,..., etc.

SIA_MODE  Specifies the medium type used by the adapter.
	  Acceptable values for this parameter are AUTODETECT, UTP, UTP_FD
	  ,UTP_100 and UTP_100FD. If you didn't specify this settings it
	  would be AUTODETECT for FastNIC.

            UTP:	10BaseT, UTP_100: Fast Ethernet (100BaseTx)
            UTP_FD: 	10BaseT with Full_Duplex
            UTP_100FD:	100BaseTx with Full_Duplex

            Default:	AUTODETECT
