**
**
**  VIA Networking Velocity Family Gigabit Ethernet Adapter
**
**  Driver Component for Windows XP Embedded SP1
**
**  v1.29   May, 2004
**
**

Release note
============

    This component is adapted from logo'ed driver for Windows XP
    for the Velocity Family Gigabit Ethernet Adapter.

    VNT provides the user with this sample component implementation,
    to ease development and test effort. The user, however,
    is advised to obtain the latest available driver and author
    his or her own components.


File description
================

    GETND5B.SYS         The NDIS5 driver for Windows XP Embedded SP1.
    GETNDIS.INF         The installation information file.
    GETNDIS.CAT         CAT file for this driver.
    GETNDIS.SLD         Driver component description file.
    XPE.TXT             This file.


Import the driver component
===========================

    1.Component Database Manager
    (1) Open "Component Database Manager" under Microsoft Windows
        Embedded Studio.
    (2) Click on the "Database", "Import...", and then SLD files "..." buttons.
        Navigate to directory of this driver component and then choose
        the .SLD file. Click on the "Import" and then "Close" buttons
        to close the dialog.
    (3) Close Component Database Manager.

    2.Target Designer
    (1) In Tools -> Options... -> Tab "Build" -> Extra Files Folder,
        fill the directory of this driver component.


Note
====

    1. The Flow Control setting "Hardware Default (Auto)" means the flow control
       ability depends on the auto-negotiation result with the link partner.
       In other settings ("Enable Tx", "Enable Rx", "Enable Tx/Rx"), driver will
       set the Tx or Rx flow control ability without auto-negotiation.
