

U-Boot 1.1.3 (Mar 19 2011 - 17:37:48)

Board: Ralink APSoC DRAM:  32 MB
relocate_code Pointer at: 81fb0000
config usb..

 The Flash ID =0000227E 
flash_protect ON: from 0xBF000000 to 0xBF01D40F
protect on 0
*** Warning - bad CRC, using default environment

============================================ 
Ralink UBoot Version: 3.3
-------------------------------------------- 
ASIC 3052_MP2 (Port5<->None)
DRAM component: 128 Mbits
DRAM bus: 32 bit
Total memory: 32 MBytes
Flash component: NOR Flash
Date:Mar 19 2011  Time:17:37:48
============================================ 
icache: sets:256, ways:4, linesz:32 ,total:32768
dcache: sets:128, ways:4, linesz:32 ,total:16384 

 ##### The CPU freq = 320 MHZ #### 

SDRAM bus set to 16 bit 
 SDRAM size =32 Mbytes

 eth_register  
Eth0 (10/100-M)
 enetvar=ethaddr,Eth addr:00:AA:BB:CC:DD:10
 00:AA:BB:CC:DD:10:

 eth_current->name = Eth0 (10/100-M)


 netboot_common, argc= 2 
 *************buf = 0x81fcd5c0
 **********NexTxPacket = 81fe4680

 NetTxPacket = 0x81FE4680 

 NetRxPackets[0] = 0x81FE4C80

 NetRxPackets[1] = 0x81FE5280

 NetRxPackets[2] = 0x81FE5880

 NetRxPackets[3] = 0x81FE5E80

 NetRxPackets[4] = 0x81FE6480

 NetRxPackets[5] = 0x81FE6A80

 NetRxPackets[6] = 0x81FE7080

 NetRxPackets[7] = 0x81FE7680

 NetRxPackets[8] = 0x81FE7C80

 NetRxPackets[9] = 0x81FE8280

 NetRxPackets[10] = 0x81FE8880

 NetRxPackets[11] = 0x81FE8E80

 NetRxPackets[12] = 0x81FE9480

 NetRxPackets[13] = 0x81FE9A80

 NetRxPackets[14] = 0x81FEA080

 NetRxPackets[15] = 0x81FEA680

 NetRxPackets[16] = 0x81FEAC80

 NetRxPackets[17] = 0x81FEB280

 NetRxPackets[18] = 0x81FEB880

 NetRxPackets[19] = 0x81FEBE80

 KSEG1ADDR(NetTxPacket) = 0xA1FE4680 

 NetLoop,call eth_halt ! 

 NetLoop,call eth_init ! 
Trying Eth0 (10/100-M)

 Waitting for RX_DMA_BUSY status Start... done

 Header Payload scatter function is Disable !! 

 ETH_STATE_ACTIVE!! 

 NetOurIP 

Please choose the operation: 
   1: Load system code to SDRAM via TFTP. 
   2: Load system code then write to Flash via TFTP. 
   3: Boot system code via Flash (default).
   4: Entr boot command line interface.
   9: Load Boot Loader code then write to Flash via TFTP. 

You choosed 2



 eth_register  
Eth0 (10/100-M)
 enetvar=ethaddr,Eth addr:00:AA:BB:CC:DD:10
 00:AA:BB:CC:DD:10:

 eth_current->name = Eth0 (10/100-M)

   
2: System Load Linux Kernel then write to Flash via TFTP. 
 Warning!! Erase Linux in Flash then burn new one. Are you sure?(Y/N)
 Please Input new ones /or Ctrl-C to discard
	Input device IP (192.168.1.1) ==:

	Input server IP (192.168.1.2) ==:

	Input Linux Kernel filename () ==:lede-rt305x-hg232-squashfs-sysupgrade-170510.bin

 netboot_common, argc= 3 
 *************buf = 0x81fcd5c0
 **********NexTxPacket = 81fe4680

 NetTxPacket = 0x81FE4680 

 NetRxPackets[0] = 0x81FE4C80

 NetRxPackets[1] = 0x81FE5280

 NetRxPackets[2] = 0x81FE5880

 NetRxPackets[3] = 0x81FE5E80

 NetRxPackets[4] = 0x81FE6480

 NetRxPackets[5] = 0x81FE6A80

 NetRxPackets[6] = 0x81FE7080

 NetRxPackets[7] = 0x81FE7680

 NetRxPackets[8] = 0x81FE7C80

 NetRxPackets[9] = 0x81FE8280

 NetRxPackets[10] = 0x81FE8880

 NetRxPackets[11] = 0x81FE8E80

 NetRxPackets[12] = 0x81FE9480

 NetRxPackets[13] = 0x81FE9A80

 NetRxPackets[14] = 0x81FEA080

 NetRxPackets[15] = 0x81FEA680

 NetRxPackets[16] = 0x81FEAC80

 NetRxPackets[17] = 0x81FEB280

 NetRxPackets[18] = 0x81FEB880

 NetRxPackets[19] = 0x81FEBE80

 KSEG1ADDR(NetTxPacket) = 0xA1FE4680 

 NetLoop,call eth_halt ! 

 NetLoop,call eth_init ! 
Trying Eth0 (10/100-M)

 Waitting for RX_DMA_BUSY status Start... done

 Header Payload scatter function is Disable !! 

 ETH_STATE_ACTIVE!! 
TFTP from server 192.168.1.2; our IP address is 192.168.1.1
Filename 'lede-rt305x-hg232-squashfs-sysupgrade-170510.bin'.

 TIMEOUT_COUNT=10,Load address: 0x80100000
Loading: *
ArpTimeoutCheck 

ArpTimeoutCheck 
T T T T T T T T T T 
Abort
upload acSysInfo = SLAVESS
upload acSysInfo = SLAVESS
upload acSysInfo = SLAVESS

 b_end =BFFFFFFF
Un-Protecting sectors 127..127 in bank 1
Un-Protected 1 sectors

 b_end =BFFFFFFF
Erase Flash from 0xbffe0000 to 0xbfffffff in Bank # 1 

 erase sector  = 127 
sect = 127,s_last = 127,erase poll = 874096
 done
Erased 1 sectors
done

 b_end =BFFFFFFF
Protecting sectors 127..127 in bank 1
Protected 1 sectors
Error: start and/or end address not on sector boundary
Error: start and/or end address not on sector boundary
update main system...

 Copy linux image[0 byte] to Flash[0xBF020000].... 
Zero length ???

 b_end =BFFFFFFF
Un-Protecting sectors 127..127 in bank 1
Un-Protected 1 sectors

 b_end =BFFFFFFF
Erase Flash from 0xbffe0000 to 0xbfffffff in Bank # 1 

 erase sector  = 127 
sect = 127,s_last = 127,erase poll = 895976
 done
Erased 1 sectors
done

 b_end =BFFFFFFF
Protecting sectors 127..127 in bank 1
Protected 1 sectors
Boot from main system!
## Booting image at bf020000 ...
   Image Name:   MIPS LEDE Linux-4.4.61
   Image Type:   MIPS Linux Kernel Image (lzma compressed)
   Data Size:    5155918 Bytes =  4.9 MB
   Load Address: 80000000
   Entry Point:  80000000
   Verifying Checksum ... OK
  IH_COMP_LZMA Uncompressing Kernel Image ... OK
No initrd
## Transferring control to Linux (at address 80000000) ...
## Giving linux memsize in MB, 32

Starting kernel ...

[    0.000000] Linux version 4.4.61 (hyn@ubuntu) (gcc version 5.4.0 (LEDE GCC 5.4.0 r4053-21c2e93) ) #0 Tue May 9 08:01:07 2017
[    0.000000] SoC Type: Ralink RT3350 id:1 rev:2
[    0.000000] bootconsole [early0] enabled
[    0.000000] CPU0 revision is: 0001964c (MIPS 24KEc)
[    0.000000] MIPS: machine is HuaWei HG232
[    0.000000] Determined physical RAM map:
[    0.000000]  memory: 02000000 @ 00000000 (usable)
[    0.000000] Initrd not found or empty - disabling initrd
[    0.000000] Zone ranges:
[    0.000000]   Normal   [mem 0x0000000000000000-0x0000000001ffffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000000000000-0x0000000001ffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000000000000-0x0000000001ffffff]
[    0.000000] Primary instruction cache 32kB, VIPT, 4-way, linesize 32 bytes.
[    0.000000] Primary data cache 16kB, 4-way, VIPT, no aliases, linesize 32 bytes
[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 8128
[    0.000000] Kernel command line: console=ttyS0,57600 rootfstype=squashfs,jffs2
[    0.000000] PID hash table entries: 128 (order: -3, 512 bytes)
[    0.000000] Dentry cache hash table entries: 4096 (order: 2, 16384 bytes)
[    0.000000] Inode-cache hash table entries: 2048 (order: 1, 8192 bytes)
[    0.000000] Writing ErrCtl register=00029420
[    0.000000] Readback ErrCtl register=00029420
[    0.000000] Memory: 24656K/32768K available (2797K kernel code, 131K rwdata, 652K rodata, 3964K init, 191K bss, 8112K reserved, 0K cma-reserved)
[    0.000000] SLUB: HWalign=32, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[    0.000000] NR_IRQS:256
[    0.000000] CPU Clock: 320MHz
[    0.000000] clocksource_probe: no matching clocksources found
[    0.000000] clocksource: MIPS: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 11945377789 ns
[    0.000018] sched_clock: 32 bits at 160MHz, resolution 6ns, wraps every 13421772796ns
[    0.015728] Calibrating delay loop... 212.58 BogoMIPS (lpj=1062912)
[    0.100941] pid_max: default: 32768 minimum: 301
[    0.110404] Mount-cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.123540] Mountpoint-cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.148449] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.168112] futex hash table entries: 256 (order: -1, 3072 bytes)
[    0.180611] pinctrl core: initialized pinctrl subsystem
[    0.192618] NET: Registered protocol family 16
[    0.247407] rt2880_gpio 10000600.gpio: registering 24 gpios
[    0.258588] rt2880_gpio 10000600.gpio: registering 24 irq handlers
[    0.274246] clocksource: Switched to clocksource MIPS
[    0.287499] NET: Registered protocol family 2
[    0.298148] TCP established hash table entries: 1024 (order: 0, 4096 bytes)
[    0.312123] TCP bind hash table entries: 1024 (order: 0, 4096 bytes)
[    0.324768] TCP: Hash tables configured (established 1024 bind 1024)
[    0.337684] UDP hash table entries: 256 (order: 0, 4096 bytes)
[    0.349386] UDP-Lite hash table entries: 256 (order: 0, 4096 bytes)
[    0.362567] NET: Registered protocol family 1
[    9.896795] rt-timer 10000100.timer: maximum frequency is 3255Hz
[    9.910952] Crashlog allocated RAM at address 0x1f00000
[    9.962496] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    9.974246] jffs2: version 2.2 (NAND) (SUMMARY) (LZMA) (RTIME) (CMODE_PRIORITY) (c) 2001-2006 Red Hat, Inc.
[   10.122381] io scheduler noop registered
[   10.130218] io scheduler deadline registered (default)
[   10.141634] Serial: 8250/16550 driver, 2 ports, IRQ sharing disabled
[   10.156687] console [ttyS0] disabled
[   10.163768] 10000c00.uartlite: ttyS0 at MMIO 0x10000c00 (irq = 20, base_baud = 6666666) is a Palmchip BK-3103
[   10.183663] console [ttyS0] enabled
[   10.183663] console [ttyS0] enabled
[   10.197609] bootconsole [early0] disabled
[   10.197609] bootconsole [early0] disabled
[   10.216326] 1f000000.cfi: Found 1 x16 devices at 0x0 in 16-bit bank. Manufacturer ID 0x000001 Chip ID 0x002101
[   10.236682] Amd/Fujitsu Extended Query Table at 0x0040
[   10.247118]   Amd/Fujitsu Extended Query version 1.3.
[   10.257375] number of CFI chips: 1
[   10.311323] 3 ofpart partitions found on MTD device 1f000000.cfi
[   10.323594] Creating 3 MTD partitions on "1f000000.cfi":
[   10.334384] 0x000000000000-0x000000020000 : "u-boot"
[   10.348148] 0x000000fa0000-0x000001f60000 : "factory"
[   10.358527] mtd: partition "factory" extends beyond the end of device "1f000000.cfi" -- size truncated to 0x60000
[   10.383684] 0x000000020000-0x000000fa0000 : "firmware"
[   10.406645] rt3050-esw 10110000.esw: link changed 0x10
[   10.422381] mtk_soc_eth 10100000.ethernet eth0: mediatek frame engine at 0xb0100000, irq 5
[   10.440408] rt2880_wdt 10000120.watchdog: Initialized
[   10.453928] NET: Registered protocol family 10
[   10.472679] NET: Registered protocol family 17
[   10.482095] bridge: automatic filtering via arp/ip/ip6tables has been deprecated. Update your scripts to load br_netfilter if you need this.
[   10.507703] 8021q: 802.1Q VLAN Support v1.8
[   10.576465] Freeing unused kernel memory: 3964K (80381000 - 80760000)
[   10.618097] init: Console is alive
[   10.625742] init: - watchdog -
[   10.674894] kmodloader: loading kernel modules from /etc/modules-boot.d/*
[   10.767552] usbcore: registered new interface driver usbfs
[   10.779082] usbcore: registered new interface driver hub
[   10.790288] usbcore: registered new device driver usb
[   10.812454] Button Hotplug driver version 0.4.1
[   10.910734] SCSI subsystem initialized
[   10.938240] dwc2 101c0000.otg: Configuration mismatch. Forcing host mode
[   11.804788] dwc2 101c0000.otg: DWC OTG Controller
[   11.814568] dwc2 101c0000.otg: new USB bus registered, assigned bus number 1
[   11.828990] dwc2 101c0000.otg: irq 26, io mem 0x00000000
[   11.842438] hub 1-0:1.0: USB hub found
[   11.851354] hub 1-0:1.0: 1 port detected
[   11.876311] usbcore: registered new interface driver usb-storage
[   11.890414] kmodloader: done loading kernel modules from /etc/modules-boot.d/*
[   11.916131] init: - preinit -
[   12.220192] 8021q: adding VLAN 0 to HW filter on device eth0
[   12.247868] usb 1-1: new high-speed USB device number 2 using dwc2
Press the [f] key and hit [enter] to enter failsafe mode
Press the [1], [2], [3] or [4] key and hit [enter] to select the debug level
[   14.561490] procd: - early -
[   14.567785] procd: - watchdog -
[   15.217441] procd: - ubus -
[   15.274792] random: ubusd: uninitialized urandom read (4 bytes read, 25 bits of entropy available)
[   15.294170] random: ubusd: uninitialized urandom read (4 bytes read, 25 bits of entropy available)
[   15.312738] random: ubusd: uninitialized urandom read (4 bytes read, 25 bits of entropy available)
[   15.332060] random: ubusd: uninitialized urandom read (4 bytes read, 25 bits of entropy available)
[   15.350579] random: ubusd: uninitialized urandom read (4 bytes read, 25 bits of entropy available)
[   15.369596] random: ubusd: uninitialized urandom read (4 bytes read, 25 bits of entropy available)
[   15.388636] random: ubusd: uninitialized urandom read (4 bytes read, 25 bits of entropy available)
[   15.408272] procd: - init -
Please press Enter to activate this console.
[   15.777690] kmodloader: loading kernel modules from /etc/modules.d/*
[   15.846888] ip6_tables: (C) 2000-2006 Netfilter Core Team
[   15.890412] fuse init (API version 7.23)
[   15.911716] Loading modules backported from Linux version wt-2017-01-31-0-ge882dff19e7f
[   15.928043] Backport generated by backports.git backports-20160324-13-g24da7d3c
[   15.952723] ip_tables: (C) 2000-2006 Netfilter Core Team
[   15.986016] nf_conntrack version 0.5.0 (447 buckets, 1788 max)
[   16.120332] xt_time: kernel timezone is -0000
[   16.270240] PPP generic driver version 2.4.2
[   16.285750] NET: Registered protocol family 24
[   16.355879] rt2800_wmac 10180000.wmac: loaded eeprom from mtd device "factory"
[   16.370645] ieee80211 phy0: rt2x00_set_rt: Info - RT chipset 2872, rev 0200 detected
[   16.386366] ieee80211 phy0: rt2x00_set_rf: Info - RF chipset 0008 detected
[   16.474871] kmodloader: done loading kernel modules from /etc/modules.d/*
[   17.444295] usb 1-1: device descriptor read/64, error -145
[   17.694097] random: jshn: uninitialized urandom read (4 bytes read, 29 bits of entropy available)
[   17.853667] random: jshn: uninitialized urandom read (4 bytes read, 29 bits of entropy available)
[   18.466194] random: jshn: uninitialized urandom read (4 bytes read, 30 bits of entropy available)
[   31.170959] 8021q: adding VLAN 0 to HW filter on device eth0
[   31.256935] device eth0.1 entered promiscuous mode
[   31.266801] device eth0 entered promiscuous mode
[   31.328318] br-lan: port 1(eth0.1) entered forwarding state
[   31.339819] br-lan: port 1(eth0.1) entered forwarding state
[   32.754450] usb 1-1: device descriptor read/64, error -145
[   33.064369] usb 1-1: new high-speed USB device number 3 using dwc2
[   33.334407] br-lan: port 1(eth0.1) entered forwarding state
[   38.264310] usb 1-1: device descriptor read/64, error -145
[   53.574295] usb 1-1: device descriptor read/64, error -145
[   53.884304] usb 1-1: new high-speed USB device number 4 using dwc2
[   64.314295] usb 1-1: device not accepting address 4, error -145
[   64.514315] usb 1-1: new high-speed USB device number 5 using dwc2
[   74.944315] usb 1-1: device not accepting address 5, error -145
[   74.956568] usb usb1-port1: unable to enumerate USB device
[   77.324343] random: nonblocking pool is initialized



BusyBox v1.26.2 () built-in shell (ash)

     _________
    /        /\      _    ___ ___  ___
   /  LE    /  \    | |  | __|   \| __|
  /    DE  /    \   | |__| _|| |) | _|
 /________/  LE  \  |____|___|___/|___|                      lede-project.org
 \        \   DE /
  \    LE  \    /  -----------------------------------------------------------
   \  DE    \  /    Reboot (SNAPSHOT, r4101-54ea0f4)
    \________\/    -----------------------------------------------------------

=== WARNING! =====================================
There is no root password defined on this device!
Use the "passwd" command to set up a new password
in order to prevent unauthorized SSH logins.
--------------------------------------------------
