PandoraBox For Ralink/MTK APSoC. Copyright 2013-2014 D-Team Technology SZ 


LINUX started...

 THIS IS ASIC
[    0.000000] Linux version 3.10.62 (lintel@PandoraBox-Server) (gcc version 4.8.3 (PandoraBox/Linaro GCC 4.8-2014.04 svn-r333) ) #2 Sun Dec 28 18:31:07 CST 2014
[    0.000000] CPU Running in Little-Endian Mode !
[    0.000000] Ralink RT3350 Revsion:0x0 CPU:320MHz, Bus:106MHz Uart:106MHz
[    0.000000] Boot form:NOR FLASH
[    0.000000] bootconsole [early0] enabled
[    0.000000] CPU revision is: 0001964c (MIPS 24KEc)
[    0.000000] Software DMA cache coherency
[    0.000000] Determined physical RAM map:
[    0.000000]  memory: 02000000 @ 00000000 (usable)
[    0.000000] Initrd not found or empty - disabling initrd
[    0.000000] Zone ranges:
[    0.000000]   Normal   [mem 0x00000000-0x01ffffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x00000000-0x01ffffff]
[    0.000000] Primary instruction cache 32kB, VIPT, 4-way, linesize 32 bytes.
[    0.000000] Primary data cache 16kB, 4-way, VIPT, no aliases, linesize 32 bytes
[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 8128
[    0.000000] Kernel command line: console=ttyS1,115200n8 board=HG255D rootfstype=squashfs,jffs2
[    0.000000] PID hash table entries: 128 (order: -3, 512 bytes)
[    0.000000] Dentry cache hash table entries: 4096 (order: 2, 16384 bytes)
[    0.000000] Inode-cache hash table entries: 2048 (order: 1, 8192 bytes)
[    0.000000] Writing ErrCtl register=00040000
[    0.000000] Readback ErrCtl register=00040000
[    0.000000] Memory: 29108k/32768k available (2339k kernel code, 3660k reserved, 552k data, 180k init, 0k highmem)
[    0.000000] SLUB: HWalign=32, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[    0.000000] NR_IRQS:128
[    0.000000] console [ttyS1] enabled, bootconsole disabled
[    0.000000] console [ttyS1] enabled, bootconsole disabled
[    0.010000] Calibrating delay loop... 212.58 BogoMIPS (lpj=1062912)
[    0.090000] pid_max: default: 32768 minimum: 301
[    0.090000] Mount-cache hash table entries: 512
[    0.100000] pinctrl core: initialized pinctrl subsystem
[    0.110000] NET: Registered protocol family 16
[    0.110000] Ralink/MTK BootROM maped.
[    0.120000] General GPIO Driver for Ralink RT3350 Board. Copyright lintel 2005-2013 
[    0.130000] RT305X-GPIO0:registering 24 irq handlers
[    0.130000] RT305X-GPIO1:registering 16 irq handlers
[    0.140000] RT305X-GPIO2:registering 12 irq handlers
[    0.140000] MIPS: machine is HuaWei HG255D
[    0.150000] HG255D:Seems factory U-Boot, FACTORY1.
[    0.150000] ralink_register_flash:NOR Flash.
[    0.160000] Ralink/MTK PinCtrl registered.
[    0.160000] General PINCTRL Driver for Ralink RT3350 Board. Copyright lintel 2005-2014 
[    0.170000] PINCTRL:add 24 pins for RT305X-PINCTRL0.
[    0.170000] PINCTRL:add 16 pins for RT305X-PINCTRL1.
[    0.180000] PINCTRL:add 12 pins for RT305X-PINCTRL2.
[    0.180000] GPIO_MODE_REG:0xDF
[    0.210000] bio: create slab <bio-0> at 0
[    0.220000] Switching to clocksource MIPS
[    0.240000] NET: Registered protocol family 2
[    0.240000] TCP established hash table entries: 512 (order: 0, 4096 bytes)
[    0.250000] TCP bind hash table entries: 512 (order: -1, 2048 bytes)
[    0.260000] TCP: Hash tables configured (established 512 bind 512)
[    0.260000] TCP: reno registered
[    0.270000] UDP hash table entries: 256 (order: 0, 4096 bytes)
[    0.270000] UDP-Lite hash table entries: 256 (order: 0, 4096 bytes)
[    0.280000] NET: Registered protocol family 1
[    0.280000] Ralink SoC clocks api init.
[    0.290000] mips hpt frequency:160000000HZ
[    0.290000] Ralink/MTK APSoC GPIO Resource maped.
[    0.300000] Load Ralink Timer0 Module
[    0.300000] Load Ralink Timer1 Module
[    0.310000] Ralink DWC_OTG Host register.
[    0.370000] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.370000] jffs2: version 2.2 (NAND) (SUMMARY) (LZMA) (RTIME) (CMODE_PRIORITY) (c) 2001-2006 Red Hat, Inc.
[    0.390000] msgmni has been set to 56
[    0.390000] io scheduler noop registered
[    0.400000] io scheduler deadline registered (default)
[    0.400000] Serial: 8250/16550 driver, 2 ports, IRQ sharing disabled
[    0.410000] serial8250: ttyS0 at MMIO 0x10000500 (irq = 37) is a 16550A
[    0.420000] serial8250: ttyS1 at MMIO 0x10000c00 (irq = 12) is a 16550A
[    0.430000] Enable Ralink GDMA Controller Module 
[    0.470000] brd: module loaded
[    0.480000] physmap platform flash device: 01000000 at bf000000
[    0.480000] physmap-flash: Found 1 x16 devices at 0x0 in 16-bit bank. Manufacturer ID 0x000001 Chip ID 0x002101
[    0.490000] Amd/Fujitsu Extended Query Table at 0x0040
[    0.500000]   Amd/Fujitsu Extended Query version 1.3.
[    0.500000] number of CFI chips: 1
[    0.510000] Creating 4 MTD partitions on "physmap-flash":
[    0.510000] 0x000000000000-0x000000020000 : "U-Boot"
[    0.520000] 0x000000fa0000-0x000000fc0000 : "Factory"
[    0.530000] 0x000000000000-0x000001000000 : "fullflash"
[    0.540000] 0x000000020000-0x000000f80000 : "firmware"
[    0.550000] PandoraBox OOPS is ready!
[    0.560000] 3 uimage-fw partitions found on MTD device firmware
[    0.560000] 0x000000020000-0x000000140000 : "kernel"
[    0.570000] 0x000000140000-0x000000f40000 : "rootfs"
[    0.580000] mtd: device 5 (rootfs) set to be root filesystem
[    0.590000] 1 squashfs-split partitions found on MTD device rootfs
[    0.600000] 0x000000ba0000-0x000000f40000 : "rootfs_data"
[    0.600000] 0x000000f40000-0x000000f80000 : "panic_oops"
[    0.610000] mtdoops: Attached to MTD device 7
[    0.640000] rdm_major = 253
[    0.640000] EEPROM:Read from [Factory] offset 0x28,length 0x6.
[    0.650000] warning: ra_mtd_read_nm: rdlen is not equal to len
[    0.650000] GMAC1_MAC_ADRH -- : 0x0000000c
[    0.660000] GMAC1_MAC_ADRL -- : 0x43305277
[    0.660000] Ralink APSoC Ethernet Driver Initilization. v3.1  512 rx/tx descriptors allocated, mtu = 1500!
[    0.670000] Feature:{HW_CSO} {HW_VLAN_TX} {SKB_RECYCLE_2K} 
[    0.680000] EEPROM:Read from [Factory] offset 0x28,length 0x6.
[    0.680000] warning: ra_mtd_read_nm: rdlen is not equal to len
[    0.690000] GMAC1_MAC_ADRH -- : 0x0000000c
[    0.690000] GMAC1_MAC_ADRL -- : 0x43305277
[    0.700000] PROC INIT OK!
[    0.700000] rt305x switch driver registered.
[    0.710000] TCP: cubic registered
[    0.710000] NET: Registered protocol family 17
[    0.720000] 8021q: 802.1Q VLAN Support v1.8
[    0.720000] PandoraBox Samba accelerater.
[    0.740000] VFS: Mounted root (squashfs filesystem) readonly on device 31:5.
[    0.750000] Freeing unused kernel memory: 180K (802d3000 - 80300000)
procd: Console is alive
[    6.970000] usbcore: registered new interface driver usbfs
[    6.970000] usbcore: registered new interface driver hub
[    6.980000] usbcore: registered new device driver usb
[    6.990000] exFAT: Version 1.2.9
[    7.120000] ufsd: module license 'Commercial product' taints kernel.
[    7.120000] Disabling lock debugging due to kernel taint
[    7.150000] ufsd: driver (8.6, Dec 27 2014 15:31:04, LBD=ON, delalloc, ioctl, bdi) loaded at 80880000
[    7.150000] NTFS (with native replay) support included
[    7.150000] optimized: speed
[    7.150000] Built for PandoraBox 2013-12-27
[    7.150000] 
[    7.270000] SGI XFS with security attributes, large block/inode numbers, no debug enabled
[    7.320000] SCSI subsystem initialized
[    8.200000] dwc2 dwc2.0: DWC OTG Controller
[    8.200000] dwc2 dwc2.0: new USB bus registered, assigned bus number 1
[    8.210000] dwc2 dwc2.0: irq 18, io mem 0x00000000
[    8.210000] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002
[    8.220000] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    8.230000] usb usb1: Product: DWC OTG Controller
[    8.230000] usb usb1: Manufacturer: Linux 3.10.62 dwc2_hsotg
[    8.240000] usb usb1: SerialNumber: dwc2.0
[    8.240000] hub 1-0:1.0: USB hub found
[    8.250000] hub 1-0:1.0: 1 port detected
[    8.260000] leds-gpio leds-gpio: pins are not configured from the driver
[    8.280000] usbcore: registered new interface driver usb-storage
procd: - preinit -
[    9.070000] usb 1-1: new high-speed USB device number 2 using dwc2
Press the [f] key and hit [enter] to enter failsafe mode
Press the [1], [2], [3] or [4] key and hit [enter] to select the debug level
[    9.410000] usb 1-1: New USB device found, idVendor=090c, idProduct=1000
[    9.420000] usb 1-1: New USB device strings: Mfr=1, Product=2, SerialNumber=0
[    9.420000] usb 1-1: Product: USB DISK
[    9.430000] usb 1-1: Manufacturer: SMI Corporation
[    9.460000] usb-storage 1-1:1.0: USB Mass Storage device detected
[    9.460000] scsi0 : usb-storage 1-1:1.0
kmod: ran 1 iterations
[   13.050000] scsi 0:0:0:0: Direct-Access     SMI      USB DISK         1100 PQ: 0 ANSI: 0 CCS
[   13.210000] sd 0:0:0:0: [sda] 15974400 512-byte logical blocks: (8.17 GB/7.61 GiB)
[   13.220000] sd 0:0:0:0: [sda] Write Protect is off
[   13.220000] sd 0:0:0:0: [sda] No Caching mode page found
[   13.230000] sd 0:0:0:0: [sda] Assuming drive cache: write through
[   13.320000] sd 0:0:0:0: [sda] No Caching mode page found
[   13.330000] sd 0:0:0:0: [sda] Assuming drive cache: write through
[   13.340000]  sda: sda1
[   13.360000] sd 0:0:0:0: [sda] No Caching mode page found
[   13.360000] sd 0:0:0:0: [sda] Assuming drive cache: write through
[   13.370000] sd 0:0:0:0: [sda] Attached SCSI removable disk
[   13.990000] jffs2: notice: (365) jffs2_build_xattr_subsystem: complete building xattr subsystem, 1 of xdatum (0 unchecked, 1 orphan) and 33 of xref (0 dead, 33 orphan) found.
block: extroot: failed to load /tmp/jffs_cfg/etc/config/fstab: Entry not found
jffs2 is ready
jffs2 is ready
[   14.040000] jffs2: notice: (361) jffs2_build_xattr_subsystem: complete building xattr subsystem, 1 of xdatum (0 unchecked, 1 orphan) and 33 of xref (0 dead, 33 orphan) found.
switching to overlay
procd: - early -
procd: - ubus -
procd: - init -
Please press Enter to activate this console.
[   21.820000] NET: Registered protocol family 10
[   21.890000] RPC: Registered named UNIX socket transport module.
[   21.890000] RPC: Registered udp transport module.
[   21.900000] RPC: Registered tcp transport module.
[   21.900000] RPC: Registered tcp NFSv4.1 backchannel transport module.
[   22.010000] tun: Universal TUN/TAP device driver, 1.6
[   22.020000] tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>
[   22.040000] sit: IPv6 over IPv4 tunneling driver
[   22.070000] gre: GRE over IPv4 demultiplexor driver
[   22.080000] ip_gre: GRE over IPv4 tunneling driver
[   22.140000] gpiodev: gpio device registered with major 252
[   22.170000] nf_conntrack version 0.5.0 (457 buckets, 1828 max)
[   22.190000] ip6_tables: (C) 2000-2006 Netfilter Core Team
[   22.220000] Netfilter messages via NETLINK v0.30.
[   22.230000] ip_set: protocol 6
[   22.300000] Ralink APSoC Hardware Watchdog Timer
[   22.340000] hidraw: raw HID events driver (C) Jiri Kosina
[   22.370000] u32 classifier
[   22.370000]     input device check on
[   22.380000]     Actions configured
[   22.390000] Mirror/redirect action on
[   22.410000] fuse init (API version 7.22)
[   23.640000] 
[   23.640000] 
[   23.640000] === pAd = c17e0000, size = 1241408 ===
[   23.640000] 
[   23.650000] <-- RTMPAllocAdapterBlock, Status=0
[   23.660000] PandoraBox RT2860v2 AP Driver version-3.0.3.2(Dec 27 2014 15:31:26).
[   23.660000] RT305x_ChipSpecInit: CHIP_SPEC_ID_NUM(3)
[   23.740000] cm109: Keymap for Komunikate KIP1000 phone loaded
[   23.760000] usbcore: registered new interface driver cm109
[   23.760000] cm109: CM109 phone driver: 20080805 (C) Alfred E. Heggestad
[   23.780000] Loading modules backported from Linux version master-2014-05-22-0-gf2032ea
[   23.790000] Backport generated by backports.git backports-20140320-37-g5c33da0
[   23.840000] ip_tables: (C) 2000-2006 Netfilter Core Team
[   24.080000] usbcore: registered new interface driver usbhid
[   24.080000] usbhid: USB HID core driver
[   24.110000] usbcore: registered new interface driver usblp
[   24.280000] xt_time: kernel timezone is -0000
[   24.420000] cfg80211: Calling CRDA to update world regulatory domain
[   24.440000] cfg80211: World regulatory domain updated:
[   24.440000] cfg80211:  DFS Master region: unset
[   24.440000] cfg80211:   (start_freq - end_freq @ bandwidth), (max_antenna_gain, max_eirp), (dfs_cac_time)
[   24.450000] cfg80211:   (2402000 KHz - 2472000 KHz @ 40000 KHz), (N/A, 2000 mBm), (N/A)
[   24.460000] cfg80211:   (2457000 KHz - 2482000 KHz @ 40000 KHz), (N/A, 2000 mBm), (N/A)
[   24.470000] cfg80211:   (2474000 KHz - 2494000 KHz @ 20000 KHz), (N/A, 2000 mBm), (N/A)
[   24.480000] cfg80211:   (5170000 KHz - 5250000 KHz @ 160000 KHz), (N/A, 2000 mBm), (N/A)
[   24.490000] cfg80211:   (5250000 KHz - 5330000 KHz @ 160000 KHz), (N/A, 2000 mBm), (0 s)
[   24.500000] cfg80211:   (5490000 KHz - 5730000 KHz @ 160000 KHz), (N/A, 2000 mBm), (0 s)
[   24.500000] cfg80211:   (5735000 KHz - 5835000 KHz @ 80000 KHz), (N/A, 2000 mBm), (N/A)
[   24.510000] cfg80211:   (57240000 KHz - 63720000 KHz @ 2160000 KHz), (N/A, 0 mBm), (N/A)
[   25.870000] usbcore: registered new interface driver p54usb
[   25.890000] PPP generic driver version 2.4.2
[   25.900000] NET: Registered protocol family 24
[   26.160000] usbcore: registered new interface driver rt73usb
[   26.600000] usbcore: registered new interface driver rtl8187
[   26.800000] usbcore: registered new interface driver snd-usb-audio
[   27.600000] usbcore: registered new interface driver rt2800usb
[   41.870000] FAT-fs (sda1): Volume was not properly unmounted. Some data may be corrupt. Please run fsck.
[   43.770000] RtmpOSNetDevDetach(): RtmpOSNetDeviceDetach(), dev->name=ra0!
[   47.600000] 
[   47.600000] 
[   47.600000] === pAd = c1f88000, size = 1241408 ===
[   47.600000] 
[   47.610000] <-- RTMPAllocAdapterBlock, Status=0
[   47.620000] PandoraBox RT2860v2 AP Driver version-3.0.3.2(Dec 27 2014 15:31:26).
[   47.630000] RT305x_ChipSpecInit: CHIP_SPEC_ID_NUM(3)
[   49.140000] RX DESC a1f0b000  size = 2048
[   49.150000] <-- RTMPAllocTxRxRingMemory, Status=0
[   49.290000] APSDCapable[0]=0
[   49.290000] APSDCapable[1]=0
[   49.290000] APSDCapable[2]=0
[   49.300000] APSDCapable[3]=0
[   49.300000] APSDCapable[4]=0
[   49.300000] APSDCapable[5]=0
[   49.310000] APSDCapable[6]=0
[   49.310000] APSDCapable[7]=0
[   49.310000] APSDCapable[8]=0
[   49.320000] APSDCapable[9]=0
[   49.320000] APSDCapable[10]=0
[   49.320000] APSDCapable[11]=0
[   49.320000] APSDCapable[12]=0
[   49.330000] APSDCapable[13]=0
[   49.330000] APSDCapable[14]=0
[   49.330000] APSDCapable[15]=0
[   49.340000] default ApCliAPSDCapable[0]=0
[   49.690000] Key1Str is Invalid key length(0) or Type(0)
[   49.700000] Key2Str is Invalid key length(0) or Type(0)
[   49.700000] Key3Str is Invalid key length(0) or Type(0)
[   49.710000] Key4Str is Invalid key length(0) or Type(0)
[   49.800000] 1. Phy Mode = 9
[   49.810000] 2. Phy Mode = 9
[   49.810000] EEPROM:Read from [Factory] offset 0x0,length 0x200.
[   49.810000] warning: ra_mtd_read_nm: rdlen is not equal to len
[   49.820000] 3. Phy Mode = 9
[   49.820000] AntCfgInit: primary/secondary ant 0/1
MCS Set = ff ff 00 00 01
[   49.830000] SYNC - BBP R4 to 20MHz.l
[   57.280000] PandoraBox Smart Channel Sniffer started.
[   57.280000] ===============================================================
[   57.290000] Scanned BSSID list:
[   57.290000] 	ch1 bssid:fc:d7:33:22:23:f6
[   57.290000] 	ch1 bssid:60:83:34:8a:37:b4
[   57.300000] 	ch1 bssid:78:c1:a7:9c:99:51
[   57.300000] 	ch1 bssid:40:16:9f:be:11:6a
[   57.310000] 	ch1 bssid:52:3a:a0:0f:01:cb
[   57.310000] 	ch1 bssid:24:69:68:51:16:c6
[   57.320000] 	ch1 bssid:1c:fa:68:b6:6e:68
[   57.320000] 	ch1 bssid:c8:e7:d8:45:99:14
[   57.320000] 	ch1 bssid:8c:21:0a:89:3a:ca
[   57.330000] 	ch1 bssid:14:3d:f2:75:fa:60
[   57.330000] 	ch1 bssid:20:76:93:2a:9a:18
[   57.340000] 	ch3 bssid:4c:5e:0c:20:68:82
[   57.340000] 	ch3 bssid:24:0a:64:fe:30:e0
[   57.340000] 	ch3 bssid:c0:3d:46:00:8a:c1
[   57.350000] 	ch4 bssid:68:8a:f0:79:ad:58
[   57.350000] 	ch4 bssid:d4:ee:07:47:9d:9e
[   57.360000] 	ch4 bssid:8c:ab:8e:ba:32:88
[   57.360000] 	ch6 bssid:80:89:17:8e:44:fe
[   57.360000] 	ch6 bssid:40:16:9f:52:79:90
[   57.370000] 	ch6 bssid:20:dc:e6:fe:7a:cb
[   57.370000] 	ch7 bssid:c8:3a:35:43:21:70
[   57.380000] 	ch8 bssid:60:b6:17:93:c1:20
[   57.380000] 	ch8 bssid:9c:7d:a3:6d:bc:1c
[   57.380000] 	ch8 bssid:28:6c:07:40:81:36
[   57.390000] 	ch8 bssid:80:9f:ab:05:93:be
[   57.390000] 	ch11 bssid:ec:26:ca:27:ff:5c
[   57.400000] 	ch11 bssid:64:13:6c:b3:c1:94
[   57.400000] 	ch11 bssid:04:27:58:4b:7c:01
[   57.400000] 	ch11 bssid:a4:56:02:51:8c:57
[   57.410000] 	ch11 bssid:84:c9:b2:87:b9:7e
[   57.410000] 	ch11 bssid:d4:ee:07:09:07:76
[   57.420000] 	ch11 bssid:24:69:68:7a:70:74
[   57.420000] 	ch11 bssid:d4:ee:07:15:7f:84
[   57.430000] 	ch11 bssid:ec:26:ca:f0:7d:2f
[   57.430000] 	ch11 bssid:04:27:58:4b:7c:00
[   57.430000] 	ch11 bssid:f4:b8:a7:4a:87:45
[   57.440000] 	ch11 bssid:28:6c:07:c9:89:e8
[   57.440000] 	ch11 bssid:50:bd:5f:3a:56:04
[   57.450000] 	ch11 bssid:b0:95:8e:4d:5b:7b
[   57.450000] 	ch11 bssid:58:66:ba:aa:84:c0
[   57.450000] 	ch11 bssid:64:09:80:0e:55:1f
[   57.460000] Channel status:
[   57.460000] 	CH1  Dirty:926 CCA:342  Time:52695 Skip:NO
[   57.470000] 	CH2  Dirty:592 CCA:274  Time:68878 Skip:NO
[   57.470000] 	CH3  Dirty:706 CCA:118  Time:58948 Skip:NO
[   57.480000] 	CH4  Dirty:758 CCA:989  Time:230758 Skip:NO
[   57.480000] 	CH5  Dirty:620 CCA:284  Time:30243 Skip:NO
[   57.490000] 	CH6  Dirty:510 CCA:46  Time:7093 Skip:NO
[   57.490000] 	CH7  Dirty:746 CCA:96  Time:8007 Skip:NO
[   57.500000] 	CH8  Dirty:840 CCA:242  Time:15495 Skip:NO
[   57.500000] 	CH9  Dirty:676 CCA:165  Time:3955 Skip:NO
[   57.510000] 	CH10  Dirty:708 CCA:67  Time:14145 Skip:NO
[   57.510000] 	CH11  Dirty:1236 CCA:335  Time:119060 Skip:NO
[   57.520000] Channel Analysis:
[   57.520000] Rule 1, CCA value : Min Dirtiness ==> Select Channel 10 
[   57.530000] Min Dirty = 1218
[   57.530000] ExChannel = 6 , 0
[   57.540000] BW        = 40
[   57.540000] ===============================================================
[   57.550000] Main bssid = 00:0c:43:30:52:f8
[   57.550000] <==== rt28xx_init, Status=0
[   57.630000] 0x1300 = 00064380
[   65.250000] Raeth v3.1 (Tasklet,SkbRecycle)
[   65.260000] 
[   65.260000] phy_tx_ring = 0x01f06000, tx_ring = 0xa1f06000
[   65.270000] 
[   65.270000] phy_rx_ring0 = 0x01d32000, rx_ring0 = 0xa1d32000
[   65.280000] GMAC1_MAC_ADRH -- : 0x0000000c
[   65.280000] GMAC1_MAC_ADRL -- : 0x43305277
[   65.290000] RT305x_ESW: Link Status Changed
[   65.290000] CDMA_CSG_CFG = 81000007
[   65.290000] GDMA1_FWD_CFG = 710000
[   65.330000] device eth0.1 entered promiscuous mode
[   65.340000] device eth0 entered promiscuous mode
[   65.360000] br-lan: port 1(eth0.1) entered forwarding state
[   65.360000] br-lan: port 1(eth0.1) entered forwarding state
[   67.360000] br-lan: port 1(eth0.1) entered forwarding state
procd: - init complete -


[END] 17-5-9 20:46:22
