1. M4 run on flash bank A. M0 run on flash bank B and the binary code of M0 is
   embedded into the code of M4.
3. Compile the project in M0/ first and then compile the project in M4/. Then
   flash it into the chip with JLink.
