
           D-Link DFE-530TX PCI Fast Ethernet Adapter Installation
                     for the NetWare Server 6.5 Driver

 Contents
 --------
    -Getting Started
        -Upgrade the driver from the install menu
        -Installation from the install menu
	-Parameters supported by the DLKFET.LAN driver
       
 Getting Started
 ---------------

	Because the adapter driver has been builded in OS,upon os boot,
	the new adapter will be detected and driver will be loaded automatically.
	All what you should do is to configurate ipx/ip information for each 
	virtual board.
	
	Note: Althought this driver test carefully for NetWare 6.5 beta3,
	      it is also suitable for official version.			

    Upgrade the driver from the install menu
    ----------------------------------------------------
        - Start the NetWare Server.

          > CD \NWSERVER
          > SERVER

        - Execute "HDETECT" after booting up.  Type,
          : HDETECT

	- Press <Enter> key to continue.

	- Press <Tab> Key and select the "Network boards" field then 
	  Press <Enter> key.
	
	- Press <Tab> key then <Delete> key twice to delete old driver if they
	  existed.

        - Please insert released driver CD into CD-ROM drive.
	
	- Press <Insert> key twice then <F3> key to specify the directory
	  which includes DLKFET.LDI, DLKFET.LAN 
	
	  Ex. <CD volume>:\NETWARE\32BITLAN	

        - Select "DLKFET.LAN ....".

        - Press <Enter> key to specify "SLOT", "Node Address", "Media and Line 
	  Speed", and "Flow control ability" if necessary.

	- Press <Tab> key to highlight "Return to driver summary" then press <Enter>
	  Key.

	- Press <Tab> key to highlight "Continue" then <Enter> key to load driver.
	
	- Now you can continue to configure ipx/ip protocol for each virtual board. 	

   Installation from the install menu
   ------------------------------------------------------
        - Start the NetWare Server.

          > CD \NWSERVER
          > SERVER

        - Execute "HDETECT" after booting up.  Type,
          : HDETECT

	- Press <Enter> key to continue.

	- Press <Tab> Key and select the "Network boards" field then 
	  Press <Enter> key.
	
	- Press <Tab> key then <Insert> key to select listed driver.
 	
        - Select "DLKFET.LAN ....".

        - Press <Enter> key to specify "SLOT", "Node Address", "Media and Line 
	  Speed", and "Flow control ability" if necessary.

	- Press <Tab> key to highlight "Return to driver summary" then press <Enter>
	  Key.

	- Press <Tab> key to highlight "Continue" then <Enter> key to load driver.
	
	- Now you can continue to configure ipx/ip protocol for each virtual board. 



     Parameters supported by the DLKFET.LAN driver
       
	The following keywords are for driver v5.10 or later.
        ----------------------------------------------------------------
        CONNECTIONTYPE                  This keyword is used to specify media type.
        
            CONNECTIONTYPE=AutoSense
            CONNECTIONTYPE=10BASET
            CONNECTIONTYPE=10BASETFD
            CONNECTIONTYPE=100BASETX
            CONNECTIONTYPE=100BASETXFD
            
        FLOW_CONTROL                    This keyword is used to specify flow control
                                        ability.(Not supported in force mode)
            FLOW_CONTROL=DISABLE
            FLOW_CONTROL=ENABLE
            FLOW_CONTROL=HARDWARE_DEFAULT   (default)
        

	The following keywords are for driver v5.10 previously(v5.10 not included).
        ------------------------------------------------------------------------	
        SLOT     1      - Force the driver to search for the specified board

        AUTOSENSE       - This keyword configures the adapter to conduct
                          NWay Auto-negotiation to determine the network
                          speed and the duplex mode of the network connection.

        10BASET         - Force driver to 10Mbps half duplex mode.

        10BASETFD       - Force driver to 10Mbps full duplex mode.

        100BASETX       - Force driver to 100Mbps half duplex mode.

        100BASETXFD     - Force driver to 100Mbps full duplex mode.
        
     



