
; ====VIA FETCE4B Driver Registry====
IF CEPC_FETCE4B
        [HKEY_LOCAL_MACHINE\Comm\FETCE4B]
            "DisplayName"="FAST ETHERNET FETCE4B"
            "Group"="NDIS"
            "ImagePath"="FETCE4B.dll"

        [HKEY_LOCAL_MACHINE\Drivers\BuiltIn\PCI\Template\FETCE4B]
            "Dll"="NDIS.dll"
            "Class"=dword:02
            "SubClass"=dword:00
            "ProgIF"=dword:0
            "VendorID"=multi_sz:"1106","1106","1106","1106"
            "DeviceID"=multi_sz:"3043","3065","3106","3053"
            "Entry"="NdisPCIBusDeviceInit"
            "Transceiver"=dword:3
            "IsrDll"="giisr.dll"
            "IsrHandler"="ISRHandler"
            "PortIsIO"=dword:1
            "PortOffset"=dword:000c
            "PortSize"=dword:2
            "PortMask"=dword:FFFF

            ;
            ; FETCE4B General setting
            ;
            "AdapterType"=dword:5
            "DmaLen"=dword:0000C000
            "ReceiveBurstIndicate"=dword:00000040
            "ReceiveThreshold"=dword:0
            "TransmitThreshold"=dword:0
            "BurstLength"=dword:1
            "MapRegisters"=dword:00000020
            "EarlyReceive"=dword:0
            "EarlyTransmit"=dword:0
            "NwayForce"=dword:1
            "HWPhyReset"=dword:0
            "PMC"=dword:0
            "TransmitBuffers"=dword:00000040
            "ReceiveBuffers"=dword:00000040
            "AdaptiveInt"=dword:1
            "ValidatePacketLen"=dword:0


        ;
        ; FETCE4B card specific settings
        ; uncomment and/or adjust the following registry items if necessary
        ;
        [HKEY_LOCAL_MACHINE\Comm\PCI\FETCE4B1\Parms]
            ;"BusNumber"=dword:00000000
            ;"SlotNumber"=dword:00000008
            ;"AdapterCFID"=dword:30531106
            ;"NetworkAddress"="00-11-22-33-44-55"
            ;"ConnectionType"=dword:0
            ;"FlowCtrl"=dword:0
            ;"TxQueueNum"=dword:8    ;for VT6105M
            ;"8021pqtag"=dword:0     ;for VT6105M
            ;"VLANID"=dword:0        ;for VT6105M
            ;"Checksum"=dword:0      ;for VT6105M

        [HKEY_LOCAL_MACHINE\Comm\PCI\FETCE4B1\Parms\TcpIp]
            "EnableDHCP"=dword:1
            "DefaultGateway"=""
            "UseZeroBroadcast"=dword:0
            "IpAddress"=""
            "Subnetmask"=""
            "DNS"=""
            "WINS"=""

        ;
        ; FETCE4B card specific settings
        ; uncomment and/or adjust the following registry items if necessary
        ;
        ;[HKEY_LOCAL_MACHINE\Comm\PCI\FETCE4B2\Parms]
            ;"BusNumber"=dword:00000000
            ;"SlotNumber"=dword:00000008
            ;"AdapterCFID"=dword:30531106
            ;"NetworkAddress"="00-11-22-33-44-55"
            ;"ConnectionType"=dword:0
            ;"FlowCtrl"=dword:0
            ;"TxQueueNum"=dword:8    ;for VT6105M
            ;"8021pqtag"=dword:0     ;for VT6105M
            ;"VLANID"=dword:0        ;for VT6105M
            ;"Checksum"=dword:0      ;for VT6105M

        ;[HKEY_LOCAL_MACHINE\Comm\PCI\FETCE4B2\Parms\TcpIp]
        ;    "EnableDHCP"=dword:1
        ;    "DefaultGateway"=""
        ;    "UseZeroBroadcast"=dword:0
        ;    "IpAddress"=""
        ;    "Subnetmask"=""
        ;    "DNS"=""
        ;    "WINS"=""

ENDIF
