## EXIF Tags

EXIF stands for "Exchangeable Image File Format". This type of information is formatted according to the TIFF specification, and may be found in JPG, TIFF, PNG, JP2, PGF, MIFF, HDP, PSP and XCF images, as well as many TIFF-based RAW images, and even some AVI and MOV videos.

The EXIF meta information is organized into different Image File Directories (IFD's) within an image. The names of these IFD's correspond to the ExifTool family 1 group names. When writing EXIF information, the default Group listed below is used unless another group is specified.

The table below lists all EXIF tags. Also listed are TIFF, DNG, HDP and other tags which are not part of the EXIF specification, but may co-exist with EXIF tags in some images. Tags which are part of the EXIF 2.3 specification have an underlined Tag Name in the HTML version of this documentation. See http://www.cipa.jp/std/documents/e/DC-008-2012_E.pdf for the official EXIF 2.3 specification.

> Tag ID | Tag Name | Writable | Group | Values / Notes
> --- | --- | --- | --- | ---
> 0x0001 | InteropIndex | string! | InteropIFD | 'R03' = R03 - DCF option file (Adobe RGB) 'R98' = R98 - DCF basic file (sRGB) 'THM' = THM - DCF thumbnail file
> 0x0002 | InteropVersion | undef!: | InteropIFD |
> 0x000b | ProcessingSoftware | string | IFD0 | (used by ACD Systems Digital Imaging)
> 0x00fe | SubfileType | int32u! | IFD0 | 0x0 = Full-resolution Image 0x1 = Reduced-resolution image 0x2 = Single page of multi-page image 0x3 = Single page of multi-page reduced-resolution image 0x4 = Transparency mask 0x5 = Transparency mask of reduced-resolution image 0x6 = Transparency mask of multi-page image 0x7 = Transparency mask of reduced-resolution multi-page image 0x10001 = Alternate reduced-resolution image 0xffffffff = invalid Bit 0 = Reduced resolution Bit 1 = Single page Bit 2 = Transparency mask Bit 3 = TIFF/IT final page Bit 4 = TIFF-FX mixed raster content
> 0x00ff | OldSubfileType | int16u! | IFD0 | 1 = Full-resolution image 2 = Reduced-resolution image 3 = Single page of multi-page image
> 0x0100 | ImageWidth | int32u! | IFD0 |
> 0x0101 | ImageHeight | int32u! | IFD0 | (called ImageLength by the EXIF spec.)
> 0x0102 | BitsPerSample | int16u[n]! | IFD0 |
> 0x0103 | Compression | int16u!: | IFD0 | --> EXIF Compression Values
> 0x0106 | PhotometricInterpretation | int16u! | IFD0 |
> 0 = WhiteIsZero 1 = BlackIsZero 2 = RGB 3 = RGB Palette 4 = Transparency Mask 5 = CMYK 6 = YCbCr 8 = CIELab 9 = ICCLab 10 = ITULab 32803 = Color Filter Array 32844 = Pixar LogL 32845 = Pixar LogLuv 34892 = Linear Raw |
> 0x0107 | Thresholding | int16u! | IFD0 | 1 = No dithering or halftoning 2 = Ordered dither or halftone 3 = Randomized dither
> 0x0108 | CellWidth | int16u! | IFD0 |
> 0x0109 | CellLength | int16u! | IFD0 |
> 0x010a | FillOrder | int16u! | IFD0 | 1 = Normal 2 = Reversed
> 0x010d | DocumentName | string | IFD0 |
> 0x010e | ImageDescription | string | IFD0 |
> 0x010f | Make | string | IFD0 |
> 0x0110 | Model | string | IFD0 |
> 0x0111 | StripOffsets PreviewImageStart PreviewImageStart JpgFromRawStart | N int32u* int32u* int32u* | - IFD0 SubIFD1 SubIFD2 | (PreviewImageStart in IFD0 of CR2 images and SubIFD1 of DNG images, and JpgFromRawStart in SubIFD2 of DNG images)
> 0x0112 | Orientation | int16u | IFD0 |
> 1 = Horizontal (normal) 2 = Mirror horizontal 3 = Rotate 180 4 = Mirror vertical 5 = Mirror horizontal and rotate 270 CW 6 = Rotate 90 CW 7 = Mirror horizontal and rotate 90 CW 8 = Rotate 270 CW |
> 0x0115 | SamplesPerPixel | int16u! | IFD0 |
> 0x0116 | RowsPerStrip | int32u! | IFD0 |
> 0x0117 | StripByteCounts PreviewImageLength PreviewImageLength JpgFromRawLength | N int32u* int32u* int32u* | - IFD0 SubIFD1 SubIFD2 | (PreviewImageLength in IFD0 of CR2 images and SubIFD1 of DNG images, and JpgFromRawLength in SubIFD2 of DNG images)
> 0x0118 | MinSampleValue | int16u | IFD0 |
> 0x0119 | MaxSampleValue | int16u | IFD0 |
> 0x011a | XResolution | rational64u: | IFD0 |
> 0x011b | YResolution | rational64u: | IFD0 |
> 0x011c | PlanarConfiguration | int16u! | IFD0 | 1 = Chunky 2 = Planar
> 0x011d | PageName | string | IFD0 |
> 0x011e | XPosition | rational64u | IFD0 |
> 0x011f | YPosition | rational64u | IFD0 |
> 0x0120 | FreeOffsets | N | - |
> 0x0121 | FreeByteCounts | N | - |
> 0x0122 | GrayResponseUnit | int16u | IFD0 | 1 = 0.1 2 = 0.001 3 = 0.0001 4 = 1e-05 5 = 1e-06
> 0x0123 | GrayResponseCurve | N | - |
> 0x0124 | T4Options | N | - | Bit 0 = 2-Dimensional encoding Bit 1 = Uncompressed Bit 2 = Fill bits added
> 0x0125 | T6Options | N | - | Bit 1 = Uncompressed
> 0x0128 | ResolutionUnit | int16u: | IFD0 | (the value 1 is not standard EXIF) 1 = None 2 = inches 3 = cm
> 0x0129 | PageNumber | int16u[2] | IFD0 |
> 0x012c | ColorResponseUnit | N | - |
> 0x012d | TransferFunction | int16u[768]! | IFD0 |
> 0x0131 | Software | string | IFD0 |
> 0x0132 | ModifyDate | string | IFD0 | (called DateTime by the EXIF spec.)
> 0x013b | Artist | string | IFD0 | (becomes a list-type tag when the MWG module is loaded)
> 0x013c | HostComputer | string | IFD0 |
> 0x013d | Predictor | int16u! | IFD0 | 1 = None 2 = Horizontal differencing
> 0x013e | WhitePoint | rational64u[2] | IFD0 |
> 0x013f | PrimaryChromaticities | rational64u[6] | IFD0 |
> 0x0140 | ColorMap | N | - |
> 0x0141 | HalftoneHints | int16u[2] | IFD0 |
> 0x0142 | TileWidth | int32u! | IFD0 |
> 0x0143 | TileLength | int32u! | IFD0 |
> 0x0144 | TileOffsets | N | - |
> 0x0145 | TileByteCounts | N | - |
> 0x0146 | BadFaxLines | N | - |
> 0x0147 | CleanFaxData | N | - | 0 = Clean 1 = Regenerated 2 = Unclean
> 0x0148 | ConsecutiveBadFaxLines | N | - |
> 0x014a | SubIFD A100DataOffset | - N | - - | --> EXIF Tags (the data offset in original Sony DSLR-A100 ARW images)
> 0x014c | InkSet | int16u | IFD0 | 1 = CMYK 2 = Not CMYK
> 0x014d | InkNames | N | - |
> 0x014e | NumberofInks | N | - |
> 0x0150 | DotRange | string | IFD0 |
> 0x0151 | TargetPrinter | N | - |
> 0x0152 | ExtraSamples | N | - | 0 = Unspecified 1 = Associated Alpha 2 = Unassociated Alpha
> 0x0153 | SampleFormat | N | - | (SamplesPerPixel values) [Values 0-3]
> 1 = Unsigned 2 = Signed 3 = Float |  | 4 = Undefined 5 = Complex int 6 = Complex float |
> 0x0154 | SMinSampleValue | N | - |
> 0x0155 | SMaxSampleValue | N | - |
> 0x0156 | TransferRange | N | - |
> 0x0157 | ClipPath | N | - |
> 0x0158 | XClipPathUnits | N | - |
> 0x0159 | YClipPathUnits | N | - |
> 0x015a | Indexed | N | - | 0 = Not indexed 1 = Indexed
> 0x015b | JPEGTables | N | - |
> 0x015f | OPIProxy | N | - | 0 = Higher resolution image does not exist 1 = Higher resolution image exists
> 0x0190 | GlobalParametersIFD | - | - | --> EXIF Tags
> 0x0191 | ProfileType | N | - | 0 = Unspecified 1 = Group 3 FAX
> 0x0192 | FaxProfile | N | - |
> 0 = Unknown 1 = Minimal B&W lossless, S 2 = Extended B&W lossless, F 3 = Lossless JBIG B&W, J 4 = Lossy color and grayscale, C 5 = Lossless color and grayscale, L 6 = Mixed raster content, M 7 = Profile T 255 = Multi Profiles |
> 0x0193 | CodingMethods | N | - |
> Bit 0 = Unspecified compression Bit 1 = Modified Huffman Bit 2 = Modified Read Bit 3 = Modified MR Bit 4 = JBIG Bit 5 = Baseline JPEG Bit 6 = JBIG color |
> 0x0194 | VersionYear | N | - |
> 0x0195 | ModeNumber | N | - |
> 0x01b1 | Decode | N | - |
> 0x01b2 | DefaultImageColor | N | - |
> 0x01b3 | T82Options | N | - |
> 0x01b5 | JPEGTables | N | - |
> 0x0200 | JPEGProc | N | - | 1 = Baseline 14 = Lossless
> 0x0201 | ThumbnailOffset ThumbnailOffset ThumbnailOffset PreviewImageStart PreviewImageStart JpgFromRawStart JpgFromRawStart OtherImageStart OtherImageStart OtherImageStart | int32u* int32u* int32u* int32u* int32u* int32u* int32u* int32u* int32u* N | IFD1 IFD0 SubIFD MakerNotes IFD0 SubIFD IFD2 SubIFD1 SubIFD2 - | (ThumbnailOffset in IFD1 of JPEG and some TIFF-based images, IFD0 of MRW images and AVI and MOV videos, and the SubIFD in IFD1 of SRW images; PreviewImageStart in MakerNotes and IFD0 of ARW and SR2 images; JpgFromRawStart in SubIFD of NEF images and IFD2 of PEF images; and OtherImageStart in everything else)
> 0x0202 | ThumbnailLength ThumbnailLength ThumbnailLength PreviewImageLength PreviewImageLength JpgFromRawLength JpgFromRawLength OtherImageLength OtherImageLength OtherImageLength | int32u* int32u* int32u* int32u* int32u* int32u* int32u* int32u* int32u* N | IFD1 IFD0 SubIFD MakerNotes IFD0 SubIFD IFD2 SubIFD1 SubIFD2 - | (ThumbnailLength in IFD1 of JPEG and some TIFF-based images, IFD0 of MRW images and AVI and MOV videos, and the SubIFD in IFD1 of SRW images; PreviewImageLength in MakerNotes and IFD0 of ARW and SR2 images; JpgFromRawLength in SubIFD of NEF images, and IFD2 of PEF images; and OtherImageLength in everything else)
> 0x0203 | JPEGRestartInterval | N | - |
> 0x0205 | JPEGLosslessPredictors | N | - |
> 0x0206 | JPEGPointTransforms | N | - |
> 0x0207 | JPEGQTables | N | - |
> 0x0208 | JPEGDCTables | N | - |
> 0x0209 | JPEGACTables | N | - |
> 0x0211 | YCbCrCoefficients | rational64u[3]! | IFD0 |
> 0x0212 | YCbCrSubSampling | int16u[2]! | IFD0 |
> '1 1' = YCbCr4:4:4 (1 1) '1 2' = YCbCr4:4:0 (1 2) '1 4' = YCbCr4:4:1 (1 4) '2 1' = YCbCr4:2:2 (2 1) |  | '2 2' = YCbCr4:2:0 (2 2) '2 4' = YCbCr4:2:1 (2 4) '4 1' = YCbCr4:1:1 (4 1) '4 2' = YCbCr4:1:0 (4 2) |
> 0x0213 | YCbCrPositioning | int16u!: | IFD0 | 1 = Centered 2 = Co-sited
> 0x0214 | ReferenceBlackWhite | rational64u[6] | IFD0 |
> 0x022f | StripRowCounts | N | - |
> 0x02bc | ApplicationNotes | int8u! | ExifIFD | --> XMP Tags
> 0x03e7 | USPTOMiscellaneous | N | - |
> 0x1000 | RelatedImageFileFormat | string! | InteropIFD |
> 0x1001 | RelatedImageWidth | int16u! | InteropIFD |
> 0x1002 | RelatedImageHeight | int16u! | InteropIFD | (called RelatedImageLength by the DCF spec.)
> 0x4746 | Rating | int16u/ | IFD0 |
> 0x4747 | XP_DIP_XML | N | - |
> 0x4748 | StitchInfo | - | - | --> Microsoft Stitch Tags
> 0x4749 | RatingPercent | int16u/ | IFD0 |
> 0x800d | ImageID | N | - |
> 0x80a3 | WangTag1 | N | - |
> 0x80a4 | WangAnnotation | N | - |
> 0x80a5 | WangTag3 | N | - |
> 0x80a6 | WangTag4 | N | - |
> 0x80b8 | ImageReferencePoints | N | - |
> 0x80b9 | RegionXformTackPoint | N | - |
> 0x80ba | WarpQuadrilateral | N | - |
> 0x80bb | AffineTransformMat | N | - |
> 0x80e3 | Matteing | N | - |
> 0x80e4 | DataType | N | - |
> 0x80e5 | ImageDepth | N | - |
> 0x80e6 | TileDepth | N | - |
> 0x8214 | ImageFullWidth | N | - |
> 0x8215 | ImageFullHeight | N | - |
> 0x8216 | TextureFormat | N | - |
> 0x8217 | WrapModes | N | - |
> 0x8218 | FovCot | N | - |
> 0x8219 | MatrixWorldToScreen | N | - |
> 0x821a | MatrixWorldToCamera | N | - |
> 0x827d | Model2 | N | - |
> 0x828d | CFARepeatPatternDim | int16u[2]! | SubIFD |
> 0x828e | CFAPattern2 | int8u[n]! | SubIFD |
> 0x828f | BatteryLevel | N | - |
> 0x8290 | KodakIFD | - | - | --> Kodak IFD Tags (used in various types of Kodak images)
> 0x8298 | Copyright | string | IFD0 | (may contain copyright notices for photographer and editor, separated by a newline. As per the EXIF specification, the newline is replaced by a null byte when writing to file, but this may be avoided by disabling the print conversion)
> 0x829a | ExposureTime | rational64u | ExifIFD |
> 0x829d | FNumber | rational64u | ExifIFD |
> 0x82a5 | MDFileTag | N | - | (tags 0x82a5-0x82ac are used in Molecular Dynamics GEL files)
> 0x82a6 | MDScalePixel | N | - |
> 0x82a7 | MDColorTable | N | - |
> 0x82a8 | MDLabName | N | - |
> 0x82a9 | MDSampleInfo | N | - |
> 0x82aa | MDPrepDate | N | - |
> 0x82ab | MDPrepTime | N | - |
> 0x82ac | MDFileUnits | N | - |
> 0x830e | PixelScale | N | - |
> 0x8335 | AdventScale | N | - |
> 0x8336 | AdventRevision | N | - |
> 0x835c | UIC1Tag | N | - |
> 0x835d | UIC2Tag | N | - |
> 0x835e | UIC3Tag | N | - |
> 0x835f | UIC4Tag | N | - |
> 0x83bb | IPTC-NAA | int32u! | IFD0 | --> IPTC Tags
> 0x847e | IntergraphPacketData | N | - |
> 0x847f | IntergraphFlagRegisters | N | - |
> 0x8480 | IntergraphMatrix | N | - |
> 0x8481 | INGRReserved | N | - |
> 0x8482 | ModelTiePoint | N | - |
> 0x84e0 | Site | N | - |
> 0x84e1 | ColorSequence | N | - |
> 0x84e2 | IT8Header | N | - |
> 0x84e3 | RasterPadding | N | - | 0 = Byte 1 = Word 2 = Long Word 9 = Sector 10 = Long Sector
> 0x84e4 | BitsPerRunLength | N | - |
> 0x84e5 | BitsPerExtendedRunLength | N | - |
> 0x84e6 | ColorTable | N | - |
> 0x84e7 | ImageColorIndicator | N | - | 0 = Unspecified Image Color 1 = Specified Image Color
> 0x84e8 | BackgroundColorIndicator | N | - | 0 = Unspecified Background Color 1 = Specified Background Color
> 0x84e9 | ImageColorValue | N | - |
> 0x84ea | BackgroundColorValue | N | - |
> 0x84eb | PixelIntensityRange | N | - |
> 0x84ec | TransparencyIndicator | N | - |
> 0x84ed | ColorCharacterization | N | - |
> 0x84ee | HCUsage | N | - | 0 = CT 1 = Line Art 2 = Trap
> 0x84ef | TrapIndicator | N | - |
> 0x84f0 | CMYKEquivalent | N | - |
> 0x8546 | SEMInfo | string | IFD0 | (found in some scanning electron microscope images)
> 0x8568 | AFCP_IPTC | - | - | --> IPTC Tags
> 0x85b8 | PixelMagicJBIGOptions | N | - |
> 0x85d7 | JPLCartoIFD | N | - |
> 0x85d8 | ModelTransform | N | - |
> 0x8602 | WB_GRGBLevels | N | - | (found in IFD0 of Leaf MOS images)
> 0x8606 | LeafData | - | - | --> Leaf Tags
> 0x8649 | PhotoshopSettings | - | - | --> Photoshop Tags
> 0x8769 | ExifOffset | - | - | --> EXIF Tags
> 0x8773 | ICC_Profile | - | - | --> ICC_Profile Tags
> 0x877f | TIFF_FXExtensions | N | - | Bit 0 = Resolution/Image Width Bit 1 = N Layer Profile M Bit 2 = Shared Data Bit 3 = B&W JBIG2 Bit 4 = JBIG2 Profile M
> 0x8780 | MultiProfiles | N | - |
> Bit 0 = Profile S Bit 1 = Profile F Bit 2 = Profile J Bit 3 = Profile C Bit 4 = Profile L Bit 5 = Profile M Bit 6 = Profile T Bit 7 = Resolution/Image Width Bit 8 = N Layer Profile M Bit 9 = Shared Data Bit 10 = JBIG2 Profile M |
> 0x8781 | SharedData | N | - |
> 0x8782 | T88Options | N | - |
> 0x87ac | ImageLayer | N | - |
> 0x87af | GeoTiffDirectory | undef | IFD0 | (these "GeoTiff" tags may read and written as a block, but they aren't extracted unless specifically requested. Byte order changes are handled automatically when copying between TIFF images with different byte order)
> 0x87b0 | GeoTiffDoubleParams | undef | IFD0 |
> 0x87b1 | GeoTiffAsciiParams | string | IFD0 |
> 0x87be | JBIGOptions | N | - |
> 0x8822 | ExposureProgram | int16u | ExifIFD | (the value of 9 is not standard EXIF, but is used by the Canon EOS 7D)
> 0 = Not Defined 1 = Manual 2 = Program AE 3 = Aperture-priority AE 4 = Shutter speed priority AE 5 = Creative (Slow speed) 6 = Action (High speed) 7 = Portrait 8 = Landscape 9 = Bulb |
> 0x8824 | SpectralSensitivity | string | ExifIFD |
> 0x8825 | GPSInfo | - | - | --> GPS Tags
> 0x8827 | ISO | int16u[n] | ExifIFD | (called ISOSpeedRatings by EXIF 2.2, then PhotographicSensitivity by the EXIF 2.3 spec.)
> 0x8828 | Opto-ElectricConvFactor | N | - | (called OECF by the EXIF spec.)
> 0x8829 | Interlace | N | - |
> 0x882a | TimeZoneOffset | int16s[n] | ExifIFD | (1 or 2 values: 1. The time zone offset of DateTimeOriginal from GMT in hours, 2. If present, the time zone offset of ModifyDate)
> 0x882b | SelfTimerMode | int16u | ExifIFD |
> 0x8830 | SensitivityType | int16u | ExifIFD | (applies to EXIF:ISO tag) 0 = Unknown 1 = Standard Output Sensitivity 2 = Recommended Exposure Index 3 = ISO Speed 4 = Standard Output Sensitivity and Recommended Exposure Index 5 = Standard Output Sensitivity and ISO Speed 6 = Recommended Exposure Index and ISO Speed 7 = Standard Output Sensitivity, Recommended Exposure Index and ISO Speed
> 0x8831 | StandardOutputSensitivity | int32u | ExifIFD |
> 0x8832 | RecommendedExposureIndex | int32u | ExifIFD |
> 0x8833 | ISOSpeed | int32u | ExifIFD |
> 0x8834 | ISOSpeedLatitudeyyy | int32u | ExifIFD |
> 0x8835 | ISOSpeedLatitudezzz | int32u | ExifIFD |
> 0x885c | FaxRecvParams | N | - |
> 0x885d | FaxSubAddress | N | - |
> 0x885e | FaxRecvTime | N | - |
> 0x8871 | FedexEDR | N | - |
> 0x888a | LeafSubIFD | - | - | --> Leaf SubIFD Tags
> 0x9000 | ExifVersion | undef: | ExifIFD |
> 0x9003 | DateTimeOriginal | string | ExifIFD | (date/time when original image was taken)
> 0x9004 | CreateDate | string | ExifIFD | (called DateTimeDigitized by the EXIF spec.)
> 0x9009 | GooglePlusUploadCode | undef[n] | ExifIFD |
> 0x9101 | ComponentsConfiguration | undef[4]!: | ExifIFD |
> 0 = - 1 = Y 2 = Cb 3 = Cr |  | 4 = R 5 = G 6 = B |
> 0x9102 | CompressedBitsPerPixel | rational64u! | ExifIFD |
> 0x9201 | ShutterSpeedValue | rational64s | ExifIFD | (displayed in seconds, but stored as an APEX value)
> 0x9202 | ApertureValue | rational64u | ExifIFD | (displayed as an F number, but stored as an APEX value)
> 0x9203 | BrightnessValue | rational64s | ExifIFD |
> 0x9204 | ExposureCompensation | rational64s | ExifIFD | (called ExposureBiasValue by the EXIF spec.)
> 0x9205 | MaxApertureValue | rational64u | ExifIFD | (displayed as an F number, but stored as an APEX value)
> 0x9206 | SubjectDistance | rational64u | ExifIFD |
> 0x9207 | MeteringMode | int16u | ExifIFD |
> 0 = Unknown 1 = Average 2 = Center-weighted average 3 = Spot 4 = Multi-spot 5 = Multi-segment 6 = Partial 255 = Other |
> 0x9208 | LightSource | int16u | ExifIFD | --> EXIF LightSource Values
> 0x9209 | Flash | int16u | ExifIFD | --> EXIF Flash Values
> 0x920a | FocalLength | rational64u | ExifIFD |
> 0x920b | FlashEnergy | N | - |
> 0x920c | SpatialFrequencyResponse | N | - |
> 0x920d | Noise | N | - |
> 0x920e | FocalPlaneXResolution | N | - |
> 0x920f | FocalPlaneYResolution | N | - |
> 0x9210 | FocalPlaneResolutionUnit | N | - | 1 = None 2 = inches 3 = cm 4 = mm 5 = um
> 0x9211 | ImageNumber | int32u | ExifIFD |
> 0x9212 | SecurityClassification | string | ExifIFD | 'C' = Confidential 'R' = Restricted 'S' = Secret 'T' = Top Secret 'U' = Unclassified
> 0x9213 | ImageHistory | string | ExifIFD |
> 0x9214 | SubjectArea | int16u[n] | ExifIFD |
> 0x9215 | ExposureIndex | N | - |
> 0x9216 | TIFF-EPStandardID | N | - |
> 0x9217 | SensingMethod | N | - | (values 1 and 6 are not standard EXIF)
> 1 = Monochrome area 2 = One-chip color area 3 = Two-chip color area 4 = Three-chip color area 5 = Color sequential area 6 = Monochrome linear 7 = Trilinear 8 = Color sequential linear |
> 0x923a | CIP3DataFile | N | - |
> 0x923b | CIP3Sheet | N | - |
> 0x923c | CIP3Side | N | - |
> 0x923f | StoNits | N | - |
> 0x927c | MakerNoteApple MakerNoteNikon MakerNoteCanon MakerNoteCasio MakerNoteCasio2 MakerNoteFLIR MakerNoteFujiFilm MakerNoteGE MakerNoteGE2 MakerNoteHasselblad MakerNoteHP MakerNoteHP2 MakerNoteHP4 MakerNoteHP6 MakerNoteISL MakerNoteJVC MakerNoteJVCText MakerNoteKodak1a MakerNoteKodak1b MakerNoteKodak2 MakerNoteKodak3 MakerNoteKodak4 MakerNoteKodak5 MakerNoteKodak6a MakerNoteKodak6b MakerNoteKodak7 MakerNoteKodak8a MakerNoteKodak8b MakerNoteKodak8c MakerNoteKodak9 MakerNoteKodak10 MakerNoteKodak11 MakerNoteKodakUnknown MakerNoteKyocera MakerNoteMinolta MakerNoteMinolta2 MakerNoteMinolta3 MakerNoteNikon2 MakerNoteNikon3 MakerNoteNintendo MakerNoteOlympus MakerNoteOlympus2 MakerNoteLeica MakerNoteLeica2 MakerNoteLeica3 MakerNoteLeica4 MakerNoteLeica5 MakerNoteLeica6 MakerNotePanasonic MakerNotePanasonic2 MakerNotePentax MakerNotePentax2 MakerNotePentax3 MakerNotePentax4 MakerNotePentax5 MakerNotePentax6 MakerNotePhaseOne MakerNoteReconyx MakerNoteRicoh MakerNoteRicoh2 MakerNoteRicohText MakerNoteSamsung1a MakerNoteSamsung1b MakerNoteSamsung2 MakerNoteSanyo MakerNoteSanyoC4 MakerNoteSanyoPatch MakerNoteSigma MakerNoteSony MakerNoteSony2 MakerNoteSony3 MakerNoteSony4 MakerNoteSony5 MakerNoteSonyEricsson MakerNoteSonySRF MakerNoteUnknownText MakerNoteUnknownBinary MakerNoteUnknown | undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef undef | ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD ExifIFD | --> Apple Tags --> Nikon Tags --> Canon Tags --> Casio Tags --> Casio Type2 Tags --> FLIR Tags --> FujiFilm Tags --> GE Tags --> FujiFilm Tags --> Unknown Tags --> HP Tags --> HP Type2 Tags --> HP Type4 Tags --> HP Type6 Tags --> Unknown Tags --> JVC Tags --> JVC Text Tags --> Kodak Tags --> Kodak Tags --> Kodak Type2 Tags --> Kodak Type3 Tags --> Kodak Type4 Tags --> Kodak Type5 Tags --> Kodak Type6 Tags --> Kodak Type6 Tags --> Kodak Type7 Tags --> Kodak Type8 Tags --> Kodak Type8 Tags --> Kodak Type8 Tags --> Kodak Type9 Tags --> Kodak Type10 Tags --> Kodak Type11 Tags --> Kodak Unknown Tags --> Unknown Tags --> Minolta Tags --> Olympus Tags (not EXIF-based) --> Nikon Type2 Tags --> Nikon Tags --> Nintendo Tags --> Olympus Tags --> Olympus Tags --> Panasonic Tags --> Panasonic Leica2 Tags --> Panasonic Leica3 Tags --> Panasonic Leica4 Tags --> Panasonic Leica5 Tags --> Panasonic Leica6 Tags --> Panasonic Tags --> Panasonic Type2 Tags --> Pentax Tags --> Pentax Type2 Tags --> Casio Type2 Tags --> Pentax Type4 Tags --> Pentax Tags --> Pentax S1 Tags --> PhaseOne Tags --> Reconyx Tags --> Ricoh Tags --> Ricoh Type2 Tags --> Ricoh Text Tags (Samsung "STMN" maker notes without PreviewImage) --> Samsung Tags --> Samsung Type2 Tags --> Sanyo Tags --> Sanyo Tags --> Sanyo Tags --> Sigma Tags --> Sony Tags --> Olympus Tags --> Olympus Tags --> Sony PIC Tags --> Sony Tags --> Sony Ericsson Tags --> Sony SRF Tags (unknown text-based maker notes) (unknown binary maker notes) --> Unknown Tags
> 0x9286 | UserComment | undef | ExifIFD |
> 0x9290 | SubSecTime | string | ExifIFD |
> 0x9291 | SubSecTimeOriginal | string | ExifIFD |
> 0x9292 | SubSecTimeDigitized | string | ExifIFD |
> 0x932f | MSDocumentText | N | - |
> 0x9330 | MSPropertySetStorage | N | - |
> 0x9331 | MSDocumentTextPosition | N | - |
> 0x935c | ImageSourceData | undef! | IFD0 |
> 0x9c9b | XPTitle | int8u | IFD0 | (tags 0x9c9b-0x9c9f are used by Windows Explorer; special characters in these values are converted to UTF-8 by default, or Windows Latin1 with the -L option. XPTitle is ignored by Windows Explorer if ImageDescription exists)
> 0x9c9c | XPComment | int8u | IFD0 |
> 0x9c9d | XPAuthor | int8u | IFD0 | (ignored by Windows Explorer if Artist exists)
> 0x9c9e | XPKeywords | int8u | IFD0 |
> 0x9c9f | XPSubject | int8u | IFD0 |
> 0xa000 | FlashpixVersion | undef: | ExifIFD |
> 0xa001 | ColorSpace | int16u: | ExifIFD | (the value of 0x2 is not standard EXIF. Instead, an Adobe RGB image is indicated by "Uncalibrated" with an InteropIndex of "R03". The values 0xfffd and 0xfffe are also non-standard, and are used by some Sony cameras) 0x1 = sRGB 0x2 = Adobe RGB 0xfffd = Wide Gamut RGB 0xfffe = ICC Profile 0xffff = Uncalibrated
> 0xa002 | ExifImageWidth | int16u: | ExifIFD | (called PixelXDimension by the EXIF spec.)
> 0xa003 | ExifImageHeight | int16u: | ExifIFD | (called PixelYDimension by the EXIF spec.)
> 0xa004 | RelatedSoundFile | string | ExifIFD |
> 0xa005 | InteropOffset | - | - | --> EXIF Tags
> 0xa20b | FlashEnergy | rational64u[n] | ExifIFD |
> 0xa20c | SpatialFrequencyResponse | N | - |
> 0xa20d | Noise | N | - |
> 0xa20e | FocalPlaneXResolution | rational64u | ExifIFD |
> 0xa20f | FocalPlaneYResolution | rational64u | ExifIFD |
> 0xa210 | FocalPlaneResolutionUnit | int16u | ExifIFD | (values 1, 4 and 5 are not standard EXIF) 1 = None 2 = inches 3 = cm 4 = mm 5 = um
> 0xa211 | ImageNumber | N | - |
> 0xa212 | SecurityClassification | N | - |
> 0xa213 | ImageHistory | N | - |
> 0xa214 | SubjectLocation | int16u[2] | ExifIFD |
> 0xa215 | ExposureIndex | rational64u | ExifIFD |
> 0xa216 | TIFF-EPStandardID | N | - |
> 0xa217 | SensingMethod | int16u | ExifIFD |
> 1 = Not defined 2 = One-chip color area 3 = Two-chip color area 4 = Three-chip color area 5 = Color sequential area 7 = Trilinear 8 = Color sequential linear |
> 0xa300 | FileSource | undef | ExifIFD | 1 = Film Scanner 2 = Reflection Print Scanner 3 = Digital Camera "\x03\x00\x00\x00" = Sigma Digital Camera
> 0xa301 | SceneType | undef | ExifIFD | 1 = Directly photographed
> 0xa302 | CFAPattern | undef | ExifIFD |
> 0xa401 | CustomRendered | int16u | ExifIFD | 0 = Normal 1 = Custom
> 0xa402 | ExposureMode | int16u | ExifIFD | 0 = Auto 1 = Manual 2 = Auto bracket
> 0xa403 | WhiteBalance | int16u | ExifIFD | 0 = Auto 1 = Manual
> 0xa404 | DigitalZoomRatio | rational64u | ExifIFD |
> 0xa405 | FocalLengthIn35mmFormat | int16u | ExifIFD | (called FocalLengthIn35mmFilm by the EXIF spec.)
> 0xa406 | SceneCaptureType | int16u | ExifIFD | 0 = Standard 1 = Landscape 2 = Portrait 3 = Night
> 0xa407 | GainControl | int16u | ExifIFD | 0 = None 1 = Low gain up 2 = High gain up 3 = Low gain down 4 = High gain down
> 0xa408 | Contrast | int16u | ExifIFD | 0 = Normal 1 = Low 2 = High
> 0xa409 | Saturation | int16u | ExifIFD | 0 = Normal 1 = Low 2 = High
> 0xa40a | Sharpness | int16u | ExifIFD | 0 = Normal 1 = Soft 2 = Hard
> 0xa40b | DeviceSettingDescription | N | - |
> 0xa40c | SubjectDistanceRange | int16u | ExifIFD | 0 = Unknown 1 = Macro 2 = Close 3 = Distant
> 0xa420 | ImageUniqueID | string | ExifIFD |
> 0xa430 | OwnerName | string | ExifIFD | (called CameraOwnerName by the EXIF spec.)
> 0xa431 | SerialNumber | string | ExifIFD | (called BodySerialNumber by the EXIF spec.)
> 0xa432 | LensInfo | rational64u[4] | ExifIFD | (4 rational values giving focal and aperture ranges, called LensSpecification by the EXIF spec.)
> 0xa433 | LensMake | string | ExifIFD |
> 0xa434 | LensModel | string | ExifIFD |
> 0xa435 | LensSerialNumber | string | ExifIFD |
> 0xa480 | GDALMetadata | N | - |
> 0xa481 | GDALNoData | N | - |
> 0xa500 | Gamma | rational64u | ExifIFD |
> 0xafc0 | ExpandSoftware | N | - |
> 0xafc1 | ExpandLens | N | - |
> 0xafc2 | ExpandFilm | N | - |
> 0xafc3 | ExpandFilterLens | N | - |
> 0xafc4 | ExpandScanner | N | - |
> 0xafc5 | ExpandFlashLamp | N | - |
> 0xbc01 | PixelFormat | N | - | (tags 0xbc** are used in Windows HD Photo (HDP and WDP) images. The actual PixelFormat values are 16-byte GUID's but the leading 15 bytes, '6fddc324-4e03-4bfe-b1853-d77768dc9', have been removed below to avoid unnecessary clutter)
> 0x5 = Black & White 0x8 = 8-bit Gray 0x9 = 16-bit BGR555 0xa = 16-bit BGR565 0xb = 16-bit Gray 0xc = 24-bit BGR 0xd = 24-bit RGB 0xe = 32-bit BGR 0xf = 32-bit BGRA 0x10 = 32-bit PBGRA 0x11 = 32-bit Gray Float 0x12 = 48-bit RGB Fixed Point 0x13 = 32-bit BGR101010 0x15 = 48-bit RGB 0x16 = 64-bit RGBA 0x17 = 64-bit PRGBA 0x18 = 96-bit RGB Fixed Point 0x19 = 128-bit RGBA Float 0x1a = 128-bit PRGBA Float 0x1b = 128-bit RGB Float 0x1c = 32-bit CMYK 0x1d = 64-bit RGBA Fixed Point 0x1e = 128-bit RGBA Fixed Point 0x1f = 64-bit CMYK 0x20 = 24-bit 3 Channels 0x21 = 32-bit 4 Channels 0x22 = 40-bit 5 Channels 0x23 = 48-bit 6 Channels 0x24 = 56-bit 7 Channels 0x25 = 64-bit 8 Channels 0x26 = 48-bit 3 Channels 0x27 = 64-bit 4 Channels 0x28 = 80-bit 5 Channels 0x29 = 96-bit 6 Channels 0x2a = 112-bit 7 Channels 0x2b = 128-bit 8 Channels 0x2c = 40-bit CMYK Alpha 0x2d = 80-bit CMYK Alpha 0x2e = 32-bit 3 Channels Alpha 0x2f = 40-bit 4 Channels Alpha 0x30 = 48-bit 5 Channels Alpha 0x31 = 56-bit 6 Channels Alpha 0x32 = 64-bit 7 Channels Alpha 0x33 = 72-bit 8 Channels Alpha 0x34 = 64-bit 3 Channels Alpha 0x35 = 80-bit 4 Channels Alpha 0x36 = 96-bit 5 Channels Alpha 0x37 = 112-bit 6 Channels Alpha 0x38 = 128-bit 7 Channels Alpha 0x39 = 144-bit 8 Channels Alpha 0x3a = 64-bit RGBA Half 0x3b = 48-bit RGB Half 0x3d = 32-bit RGBE 0x3e = 16-bit Gray Half 0x3f = 32-bit Gray Fixed Point |
> 0xbc02 | Transformation | N | - |
> 0 = Horizontal (normal) 1 = Mirror vertical 2 = Mirror horizontal 3 = Rotate 180 4 = Rotate 90 CW 5 = Mirror horizontal and rotate 90 CW 6 = Mirror horizontal and rotate 270 CW 7 = Rotate 270 CW |
> 0xbc03 | Uncompressed | N | - | 0 = No 1 = Yes
> 0xbc04 | ImageType | N | - | Bit 0 = Preview Bit 1 = Page
> 0xbc80 | ImageWidth | N | - |
> 0xbc81 | ImageHeight | N | - |
> 0xbc82 | WidthResolution | N | - |
> 0xbc83 | HeightResolution | N | - |
> 0xbcc0 | ImageOffset | N | - |
> 0xbcc1 | ImageByteCount | N | - |
> 0xbcc2 | AlphaOffset | N | - |
> 0xbcc3 | AlphaByteCount | N | - |
> 0xbcc4 | ImageDataDiscard | N | - | 0 = Full Resolution 1 = Flexbits Discarded 2 = HighPass Frequency Data Discarded 3 = Highpass and LowPass Frequency Data Discarded
> 0xbcc5 | AlphaDataDiscard | N | - | 0 = Full Resolution 1 = Flexbits Discarded 2 = HighPass Frequency Data Discarded 3 = Highpass and LowPass Frequency Data Discarded
> 0xc427 | OceScanjobDesc | N | - |
> 0xc428 | OceApplicationSelector | N | - |
> 0xc429 | OceIDNumber | N | - |
> 0xc42a | OceImageLogic | N | - |
> 0xc44f | Annotations | N | - |
> 0xc4a5 | PrintIM | undef | IFD0 | --> PrintIM Tags
> 0xc573 | OriginalFileName | N | - | (used by some obscure software)
> 0xc580 | USPTOOriginalContentType | N | - | 0 = Text or Drawing 1 = Grayscale 2 = Color
> 0xc612 | DNGVersion | int8u[4]! | IFD0 | (tags 0xc612-0xc7b5 are used in DNG images unless otherwise noted)
> 0xc613 | DNGBackwardVersion | int8u[4]! | IFD0 |
> 0xc614 | UniqueCameraModel | string | IFD0 |
> 0xc615 | LocalizedCameraModel | string | IFD0 |
> 0xc616 | CFAPlaneColor | N | - |
> 0xc617 | CFALayout | N | - | 1 = Rectangular 2 = Even columns offset down 1/2 row 3 = Even columns offset up 1/2 row 4 = Even rows offset right 1/2 column 5 = Even rows offset left 1/2 column 6 = Even rows offset up by 1/2 row, even columns offset left by 1/2 column 7 = Even rows offset up by 1/2 row, even columns offset right by 1/2 column 8 = Even rows offset down by 1/2 row, even columns offset left by 1/2 column 9 = Even rows offset down by 1/2 row, even columns offset right by 1/2 column
> 0xc618 | LinearizationTable | int16u[n]! | SubIFD |
> 0xc619 | BlackLevelRepeatDim | int16u[2]! | SubIFD |
> 0xc61a | BlackLevel | rational64u[n]! | SubIFD |
> 0xc61b | BlackLevelDeltaH | rational64s[n]! | SubIFD |
> 0xc61c | BlackLevelDeltaV | rational64s[n]! | SubIFD |
> 0xc61d | WhiteLevel | int32u[n]! | SubIFD |
> 0xc61e | DefaultScale | rational64u[2]! | SubIFD |
> 0xc61f | DefaultCropOrigin | int32u[2]! | SubIFD |
> 0xc620 | DefaultCropSize | int32u[2]! | SubIFD |
> 0xc621 | ColorMatrix1 | rational64s[n]! | IFD0 |
> 0xc622 | ColorMatrix2 | rational64s[n]! | IFD0 |
> 0xc623 | CameraCalibration1 | rational64s[n]! | IFD0 |
> 0xc624 | CameraCalibration2 | rational64s[n]! | IFD0 |
> 0xc625 | ReductionMatrix1 | rational64s[n]! | IFD0 |
> 0xc626 | ReductionMatrix2 | rational64s[n]! | IFD0 |
> 0xc627 | AnalogBalance | rational64u[n]! | IFD0 |
> 0xc628 | AsShotNeutral | rational64u[n]! | IFD0 |
> 0xc629 | AsShotWhiteXY | rational64u[2]! | IFD0 |
> 0xc62a | BaselineExposure | rational64s! | IFD0 |
> 0xc62b | BaselineNoise | rational64u! | IFD0 |
> 0xc62c | BaselineSharpness | rational64u! | IFD0 |
> 0xc62d | BayerGreenSplit | int32u! | SubIFD |
> 0xc62e | LinearResponseLimit | rational64u! | IFD0 |
> 0xc62f | CameraSerialNumber | string | IFD0 |
> 0xc630 | DNGLensInfo | rational64u[4] | IFD0 |
> 0xc631 | ChromaBlurRadius | rational64u! | SubIFD |
> 0xc632 | AntiAliasStrength | rational64u! | SubIFD |
> 0xc633 | ShadowScale | rational64u! | IFD0 |
> 0xc634 | SR2Private DNGAdobeData MakerNotePentax MakerNotePentax5 DNGPrivateData | - undef! - - undef! | - IFD0 - - IFD0 | --> Sony SR2Private Tags --> DNG AdobeData Tags --> Pentax Tags --> Pentax Tags
> 0xc635 | MakerNoteSafety | int16u | IFD0 | 0 = Unsafe 1 = Safe
> 0xc640 | RawImageSegmentation | N | - | (used in segmented Canon CR2 images. 3 numbers: 1. Number of segments minus one; 2. Pixel width of segments except last; 3. Pixel width of last segment)
> 0xc65a | CalibrationIlluminant1 | int16u! | IFD0 | --> EXIF LightSource Values
> 0xc65b | CalibrationIlluminant2 | int16u! | IFD0 | --> EXIF LightSource Values
> 0xc65c | BestQualityScale | rational64u! | SubIFD |
> 0xc65d | RawDataUniqueID | int8u[16]! | IFD0 |
> 0xc660 | AliasLayerMetadata | N | - | (used by Alias Sketchbook Pro)
> 0xc68b | OriginalRawFileName | string! | IFD0 |
> 0xc68c | OriginalRawFileData | undef! | IFD0 | --> DNG OriginalRaw Tags
> 0xc68d | ActiveArea | int32u[4]! | SubIFD |
> 0xc68e | MaskedAreas | int32u[4]! | SubIFD |
> 0xc68f | AsShotICCProfile | undef! | IFD0 | --> ICC_Profile Tags
> 0xc690 | AsShotPreProfileMatrix | rational64s[n]! | IFD0 |
> 0xc691 | CurrentICCProfile | undef! | IFD0 | --> ICC_Profile Tags
> 0xc692 | CurrentPreProfileMatrix | rational64s[n]! | IFD0 |
> 0xc6bf | ColorimetricReference | int16u! | IFD0 |
> 0xc6c5 | SRawType | N | - |
> 0xc6d2 | PanasonicTitle | undef | IFD0 | (proprietary Panasonic tag used for baby/pet name, etc)
> 0xc6d3 | PanasonicTitle2 | undef | IFD0 | (proprietary Panasonic tag used for baby/pet name with age)
> 0xc6f3 | CameraCalibrationSig | string! | IFD0 |
> 0xc6f4 | ProfileCalibrationSig | string! | IFD0 |
> 0xc6f5 | ProfileIFD | - | - | --> EXIF Tags
> 0xc6f6 | AsShotProfileName | string! | IFD0 |
> 0xc6f7 | NoiseReductionApplied | rational64u! | SubIFD |
> 0xc6f8 | ProfileName | string! | IFD0 |
> 0xc6f9 | ProfileHueSatMapDims | int32u[3]! | IFD0 |
> 0xc6fa | ProfileHueSatMapData1 | float[n]! | IFD0 |
> 0xc6fb | ProfileHueSatMapData2 | float[n]! | IFD0 |
> 0xc6fc | ProfileToneCurve | float[n]! | IFD0 |
> 0xc6fd | ProfileEmbedPolicy | int32u! | IFD0 | 0 = Allow Copying 1 = Embed if Used 2 = Never Embed 3 = No Restrictions
> 0xc6fe | ProfileCopyright | string! | IFD0 |
> 0xc714 | ForwardMatrix1 | rational64s[n]! | IFD0 |
> 0xc715 | ForwardMatrix2 | rational64s[n]! | IFD0 |
> 0xc716 | PreviewApplicationName | string! | IFD0 |
> 0xc717 | PreviewApplicationVersion | string! | IFD0 |
> 0xc718 | PreviewSettingsName | string! | IFD0 |
> 0xc719 | PreviewSettingsDigest | int8u! | IFD0 |
> 0xc71a | PreviewColorSpace | int32u! | IFD0 | 0 = Unknown 1 = Gray Gamma 2.2 2 = sRGB 3 = Adobe RGB 4 = ProPhoto RGB
> 0xc71b | PreviewDateTime | string! | IFD0 |
> 0xc71c | RawImageDigest | int8u[16]! | IFD0 |
> 0xc71d | OriginalRawFileDigest | int8u[16]! | IFD0 |
> 0xc71e | SubTileBlockSize | N | - |
> 0xc71f | RowInterleaveFactor | N | - |
> 0xc725 | ProfileLookTableDims | int32u[3]! | IFD0 |
> 0xc726 | ProfileLookTableData | float[n]! | IFD0 |
> 0xc740 | OpcodeList1 | N | - |
> 0xc741 | OpcodeList2 | N | - |
> 0xc74e | OpcodeList3 | N | - |
> 0xc761 | NoiseProfile | double[n]! | SubIFD |
> 0xc763 | TimeCodes | int8u[n] | IFD0 |
> 0xc764 | FrameRate | rational64s | IFD0 |
> 0xc772 | TStop | rational64u[n] | IFD0 |
> 0xc789 | ReelName | string | IFD0 |
> 0xc791 | OriginalDefaultFinalSize | int32u[2]! | IFD0 |
> 0xc792 | OriginalBestQualitySize | int32u[2]! | IFD0 | (called OriginalBestQualityFinalSize by the DNG spec)
> 0xc793 | OriginalDefaultCropSize | rational64u[2]! | IFD0 |
> 0xc7a1 | CameraLabel | string | IFD0 |
> 0xc7a3 | ProfileHueSatMapEncoding | int32u! | IFD0 | 0 = Linear 1 = sRGB
> 0xc7a4 | ProfileLookTableEncoding | int32u! | IFD0 | 0 = Linear 1 = sRGB
> 0xc7a5 | BaselineExposureOffset | rational64s! | IFD0 |
> 0xc7a6 | DefaultBlackRender | int32u! | IFD0 | 0 = Auto 1 = None
> 0xc7a7 | NewRawImageDigest | int8u[16]! | IFD0 |
> 0xc7a8 | RawToPreviewGain | double! | IFD0 |
> 0xc7b5 | DefaultUserCrop | rational64u[4]! | SubIFD |
> 0xea1c | Padding | undef | ExifIFD |
> 0xea1d | OffsetSchema | int32s | ExifIFD | (Microsoft's ill-conceived maker note offset difference)
> 0xfde8 | OwnerName | string/ | ExifIFD | (tags 0xfde8-0xfdea and 0xfe4c-0xfe58 are generated by Photoshop Camera RAW. Some names are the same as other EXIF tags, but ExifTool will avoid writing these unless they already exist in the file)
> 0xfde9 | SerialNumber | string/ | ExifIFD |
> 0xfdea | Lens | string/ | ExifIFD |
> 0xfe00 | KDC_IFD | - | - | --> Kodak KDC_IFD Tags (used in some Kodak KDC images)
> 0xfe4c | RawFile | string/ | ExifIFD |
> 0xfe4d | Converter | string/ | ExifIFD |
> 0xfe4e | WhiteBalance | string/ | ExifIFD |
> 0xfe51 | Exposure | string/ | ExifIFD |
> 0xfe52 | Shadows | string/ | ExifIFD |
> 0xfe53 | Brightness | string/ | ExifIFD |
> 0xfe54 | Contrast | string/ | ExifIFD |
> 0xfe55 | Saturation | string/ | ExifIFD |
> 0xfe56 | Sharpness | string/ | ExifIFD |
> 0xfe57 | Smoothness | string/ | ExifIFD |
> 0xfe58 | MoireFilter | string/ | ExifIFD |

## EXIF Compression Values

> Value | Compression
> --- | ---
> 1 | = Uncompressed
> 2 | = CCITT 1D
> 3 | = T4/Group 3 Fax
> 4 | = T6/Group 4 Fax
> 5 | = LZW
> 6 | = JPEG (old-style)
> 7 | = JPEG
> 8 | = Adobe Deflate
> 9 | = JBIG B&W
> 10 | = JBIG Color
> 99 | = JPEG
> 262 | = Kodak 262
> 32766 | = Next
> 32767 | = Sony ARW Compressed
> 32769 | = Packed RAW
> 32770 | = Samsung SRW Compressed
> 32771 | = CCIRLEW
> 32772 | = Samsung SRW Compressed 2
> 32773 | = PackBits
> 32809 | = Thunderscan
> 32867 | = Kodak KDC Compressed
> 32895 | = IT8CTPAD
> 32896 | = IT8LW
> 32897 | = IT8MP
> 32898 | = IT8BL
> 32908 | = PixarFilm
> 32909 | = PixarLog
> 32946 | = Deflate
> 32947 | = DCS
> 34661 | = JBIG
> 34676 | = SGILog
> 34677 | = SGILog24
> 34712 | = JPEG 2000
> 34713 | = Nikon NEF Compressed
> 34715 | = JBIG2 TIFF FX
> 34718 | = Microsoft Document Imaging (MDI) Binary Level Codec
> 34719 | = Microsoft Document Imaging (MDI) Progressive Transform Codec
> 34720 | = Microsoft Document Imaging (MDI) Vector
> 34892 | = Lossy JPEG
> 65000 | = Kodak DCR Compressed
> 65535 | = Pentax PEF Compressed

## EXIF LightSource Values

> Value | LightSource | Value | LightSource | Value | LightSource
> --- | --- | --- | --- | --- | ---
> 0 | = Unknown | 12 | = Daylight Fluorescent | 20 | = D55
> 1 | = Daylight | 13 | = Day White Fluorescent | 21 | = D65
> 2 | = Fluorescent | 14 | = Cool White Fluorescent | 22 | = D75
> 3 | = Tungsten (Incandescent) | 15 | = White Fluorescent | 23 | = D50
> 4 | = Flash | 16 | = Warm White Fluorescent | 24 | = ISO Studio Tungsten
> 9 | = Fine Weather | 17 | = Standard Light A | 255 | = Other
> 10 | = Cloudy | 18 | = Standard Light B |  |
> 11 | = Shade | 19 | = Standard Light C |  |

## EXIF Flash Values

> Value | Flash
> --- | ---
> 0x0 | = No Flash
> 0x1 | = Fired
> 0x5 | = Fired, Return not detected
> 0x7 | = Fired, Return detected
> 0x8 | = On, Did not fire
> 0x9 | = On, Fired
> 0xd | = On, Return not detected
> 0xf | = On, Return detected
> 0x10 | = Off, Did not fire
> 0x14 | = Off, Did not fire, Return not detected
> 0x18 | = Auto, Did not fire
> 0x19 | = Auto, Fired
> 0x1d | = Auto, Fired, Return not detected
> 0x1f | = Auto, Fired, Return detected
> 0x20 | = No flash function
> 0x30 | = Off, No flash function
> 0x41 | = Fired, Red-eye reduction
> 0x45 | = Fired, Red-eye reduction, Return not detected
> 0x47 | = Fired, Red-eye reduction, Return detected
> 0x49 | = On, Red-eye reduction
> 0x4d | = On, Red-eye reduction, Return not detected
> 0x4f | = On, Red-eye reduction, Return detected
> 0x50 | = Off, Red-eye reduction
> 0x58 | = Auto, Did not fire, Red-eye reduction
> 0x59 | = Auto, Fired, Red-eye reduction
> 0x5d | = Auto, Fired, Red-eye reduction, Return not detected
> 0x5f | = Auto, Fired, Red-eye reduction, Return detected

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Dec 9, 2014

<-- ExifTool Tag Names