3563696286
5769027229
M
TITLE
ID,Sub Cat,Flr,Size,Item,Count,Extra,Un,Quantity,Price,Tot. Cost,Supplier,Def.,Code,Comment,Manufacturer

TITLEWIDTH
5,3,12,14,6,6,4,10,8,11,10,5,8,10,

MANUFACTURER
21,0,0,0
Stone Products Corp.,www.culturedstone.com,(800) 255-1727,(707) 254-5572
Avonite inc.,www.avonite.com,(505) 864-3800,(505) 864-7790,
Aqua Glass Corp.,www.aquaglass.com,(800) 632-0911,Please Call,
Arcways,www.arcways.com,(800) 558-5096,(920) 725-2053,
CertainTeed Corp.,www.certainteed.com,(800) 233-8990,Please Call,
Dal-Tile,www.daltile.com,(800) 933-8453,Please Call,
Formica Corp.,www.formica.com,(513) 786-3400,(513) 786-3024,
Jeld-Wen,www.jeld-wen.com,Visit our Web site,Visit our Web site,
Morgan,www.jeld-wen.com,Visit our Web site,Visit our Web site,
Caradco,www.jeld-wen.com,Visit our Web site,Visit our Web site,
Nord Doors,www.jeld-wen.com,Visit our Web site,Visit our Web site,
Pozzi,www.jeld-wen.com,Visit our Web site,Visit our Web site,
New England Classic Interiors,www.homefittings.com,(888) 880-6324,(207) 774-1685,
Owens Corning,www.owenscorning.com,(800) GET-PINK,Please Call,
Simpson Strong-Tie,www.strongtie.com,(800) 999-5099,(510) 632-8925,
Superior Fireplaces,www.superiorfireplace.com,(800) 731-8101,(901) 885-7880,
Therma Tru Doors,www.thermatru.com,(800) 366-7799,Please Call,
Warner Wallpaper,www.thewarnerco.com/warner.htm,(800) 685-8822,(312) 372-9584,
Window Products,www.windowproducts.com,(800) 442-8544,(509) 924-9473,
A-19,www.A-19.com,(800) 664-4204,(800) 329-9899,
Maytag,www.maytag.com,(800) 688-9900,Please Call,

SCHEDULEHEADING
WINDOW,DOOR,CABINET,FIXTURE,FURNITURE,ELECTRICAL,SCHEDULE

SCHEDULETITLES
NUMBER,QTY,FLOOR,SIZE,R/O,DIMENSIONS,HEADER,THICKNESS,MATERIAL,DESCRIPTION,EXTRA2,EXTRA3,CODE,MANUFACTURER,REMARKS

DOORTYPE
doorway,hinged,slider,pocket,bifold,garage,

DOORSTYLE
default,slab,glass,panel,louvered,library

WINDOWTYPE
plan default,fixed glass,single hung,double hung,sngl casement,dbl casement,triple casemnt
left sliding,right sliding,triple sliding,awning,double awning,triple awning
hopper,double hopper,triple hopper,louvered,mulled unit

SWINDOWTYPE
XX,FX,SH,DH,SC,DC,TC
LS,RS,TS,AW,FA,TA
HO,FH,TH,LV,MU

WINDOWSTYLE
-eg,-ct,-at,-mu,-hl,-hr,lhl,lhr,rhl,rhr,chl,chr,t,b,c

CABSTRINGS
,kit. ,bath ,,gar. ,
base,util,wall,shelf & rod,partition
crnr ,pen ,end ,rad end ,pen rad ,ang front , cab

SERVICE1
wall mount, floor mount, ceiling mount
SERVICE2
110V duplex outlet,220V outlet,std light,wall switch

UNITTEXT
,16th,in,ft,yd,sqft,sqyd,cuft,cuyd
UNITTEXTM
,mm,cm,m,m,sq m,sq m,cu m,cu m

WALLLAYERS
fir stud 16" OC,fir stud 24" OC,steel stud 16" OC,steel stud 24" OC,air gap,
sheet insulation,foam insulation,sheathing,OSB,sheetrock,
plaster,marble,corian,ceramic tile,ceramic tile 2,
wood panel,wood panel 2,wood siding,wood siding 2,wood siding 3,
vinyl siding,alum. siding,stucco,brick,brick 2,
brick 3,concrete block,concrete block 2,concrete block 3,glass block,
stone,concrete,laminate,laminate 2,carpet,
carpet 2,vinyl floor,vinyl floor 2,parquet hdwd,tile floor,
2x4 deck plank,2x6 deck plank,asphalt shingles,wood shingles,wood shakes,
roofing tiles,
Standing Seam Roofing,Corrugated Metal Roofing,Asphalt Membrane Roofing,Steel,Copper,
Brass,Aluminum,Iron,Sheet Metal,Vinyl,
Polyethylene Plastic,Fiberglass,Glass,Tempered Glass,Laminated Glass,
Vertical Siding,Vertical Siding 2,Granite,Gravel

WALLLAYERSM
fir stud 450 OC,fir stud 600 OC,steel stud 450 OC,steel stud 600 OC,air gap,
sheet insulation,foam insulation,sheathing,OSB,sheetrock,
plaster,marble,corian,ceramic tile,ceramic tile 2,
wood panel,wood panel 2,wood siding,wood siding 2,wood siding 3,
vinyl siding,alum. siding,stucco,brick,brick 2,
brick 3,concrete block,concrete block 2,concrete block 3,glass block,
stone,concrete,laminate,laminate 2,carpet,
carpet 2,vinyl floor,vinyl floor 2,parquet hdwd,tile floor,
100x35 deck plank,150x35 deck plank,asphalt shingles,wood shingles,wood shakes,
roofing tiles,
Standing Seam Roofing,Corrugated Metal Roofing,Asphalt Membrane Roofing,Steel,Copper,
Brass,Aluminum,Iron,Sheet Metal,Vinyl,
Polyethylene Plastic,Fiberglass,Glass,Tempered Glass,Laminated Glass,
Vertical Siding,Vertical Siding 2,Granite,Gravel

WALLDXFCODE
FS,FS,SS,SS,AG,IS,IF,SG,OB,SR
PL,MB,CO,CT,CT,WP,WP,WS,WS,WS
VS,AS,SC,BK,BK,BK,CB,CB,CB,GB
ST,CN,LA,LA,CP,CP,VF,VF,HF,TF
DP,DP,SA,SN,SH,RT
SSR,CMR,AMR,CRS,CU,BR,AL,FE,GSM,VI
PPS,PGS,GL,TGL,LGL,VS1,VS2,GRAN,GRAV

WALLDIMEN
%dx%d-%s",%sx%sx%s,%s" wide,%dx%dx%s,gap,
%s" thick,%s" thick,%s" thick,%sx%sx%s,%sx%sx%s,
%s" thick,%sx%sx%s,%sx%sx%s,%s side x%s thk,%s side x%s thk,
%s side x%s thk,%s" thick,%s" thick,%s" thick

WALLDIMENM
%dx%d-%s,%sx%sx%s,%smm wide,%dx%dx%s,gap,
%smm thick,%smm thick,%smm thick,%sx%sx%s,%sx%sx%s,
%smm thick,%sx%sx%s,%sx%sx%s,%s side x%s thk,%s side x%s thk,
%s side x%s thk,%smm thick,%smm thick,%smm thick

ITEM
GN     General
5
140   heated wall area
340   heated glass area
440   heated door area
540   heated ceiling area
640   heated roof area

ITEM
FO     Foundation
19
10    concrete found. wall,^%sx%d"h,^%sx%dmm h
20    concrete grade beam,^%sx%d"h,^%sx%dmm h
30    foundation girder,%dx8"
40    concrete footing,^%sx%s"h,^%sx%smm h
50    treated mud sill,2x6",150x38mm
60    foam sill seal,1/2x6",150x12mm
70    foundation bolts
80    concrete slab,^%s sq ft,%s sq m
90    termite flashing
120   drilled pier hole,^%d"diam x %d",^%ddiam x %dmm
140   concrete for piers
150   post support concrete
170   slab for fireplace,^%dx%dx%d",^%dx%dx%dmm
200   steel mesh for slab,%s sq ft,%s sq m
220   rebar (slab),no. %d
230   rebar (footing),no. %d
240   horiz. rebar (wall),no. %d
250   vert. rebar (wall),no. %d
260   rebar (piers),no. %d

ITEM
M     Masonry
1
8     masonry fireplace


ITEM
SF    Subfloor
18
1     floor joists,%dx%d"-%d',%dx%d-%dmm
2     floor joists,%dx%d"-16'+,%dx%d-4800mm+
3     rim joists,%dx%d"-%d',%dx%d-%dmm
4     rim joists,%dx%d"-16'+,%dx%d-4800mm+
5     ceiling joists,%dx%d"-%d',%dx%d-%dmm
6     ceiling joists,%dx%d"-16'+,%dx%d-4800mm+
7     joists,%dx%d"-%d',%dx%d-%dmm
8     joist,%dx%d"-16'+,%dx%d-4800mm+
21    framing nails
22    nails
23    screws
24    adhesive
25    subfloor nails
26    subfloor nails
27    adhesive
70    floor joists,2x%d" 16" OC,%dx38mm 450 OC
71    ceiling joists,2x%d" 16" OC,%dx38mm 450 OC
80    floor sheathing,4x8'x%s" sheets,1200x2400x%s sheets

ITEM
F     Framing
22
7     door/window header,4x12",300x100mm
8     fir stud,2x%d-%s",%dx35-%s
9     fir stud,2x%d-16ft+,%dx35-4800mm+
1     fir stud,%dx%d"-%s",%dx%dmm-%smm
2     fir stud stock,%dx%d-16ft+,%dx%d-4800mm+
3     fir plate,%dx%d-16ft+,%dx%d-4800mm+
4     curved plate,%dx%d-16ft+,%dx%d-4800mm+
10    header,%dx%d"-%s",%dx%dmm-%smm
11    header,%dx%d-16ft+,%dx%d-4800mm+
21    framing nails
22    nails
23    screws
24    adhesive
26    corner window support
41    steel stud,%dx%d"-%d",%dx%dmm-%dmm
42    steel stud stock,%dx%d,%dx%dmm
43    steel plate,%dx%d,%dx%dmm
44    curved plate,%dx%d,%dx%d
50    steel header,%dx%d"-%d",%dx%dmm-%dmm
51    steel header,%dx%d",%dx%dmm
90    framing,%dx%d"-%d',%dx%d-%dmm
92    framing,%dx%d"-16'+,%dx%d-4800mm+


ITEM
R     Roofing
26
1     rafters,%dx%d"-%d',%dx%d-%dmm
2     rafters,%dx%d"-16'+,%dx%d-4800mm+
3     ridge board,%dx%d"-%d',%dx%d-%dmm
4     ridge board,%dx%d"-16'+,%dx%d-4800mm+
8     roof truss, %s", %smm
21    framing nails
22    framing nails
24    adhesive
25    sheathing nails
26    sheathing nails
27    adhesive
28    roofing nails
41    gutter
42    downspout
45    metal drip edge
47    valley flashing
48    roof/wall flashing,90 deg. bend
49    roof/wall flashing,bend to slope
54    ridge vent
55    ridge cap
56    hip ridge cap
70    rect. skylight,%sx%s",%sx%smm
71    non rect. skylight,%sx%s",%sx%smm
100   roofing material
120   roof sheathing,4x8' sheets,1200x2400 sheets
160   rafters - fir,2x%d" 16" OC,%dx38mm 450 OC
190   gable fascia,2x%d",%dx35mm
200   eave fascia,2x%d",%dx35mm

ITEM
S     Siding
6
10    sheathing,4x8' sheets,1200x2400 sheets
25    sheathing nails
26    sheathing nails
27    adhesive
40    exterior siding
80    house wrap

ITEM
EX    Ext. Trim
30
40    exterior sill,1x%d-16ft+,%dx18-4800mm+
45    vertical mull trim,%d" wide,%dmm wide
46    horiz. mull trim,%d" wide,%dmm wide
60    between window trim,%d" wide,%dmm wide
62    corner window trim
70    door threshold,1x%d-%d",%dx18-%dmm
80    shutter,%sx%s in,%sx%s mm
82    rnd top shutter,%sx%s in,%sx%s mm
84    arch top shutter,%sx%s in,%sx%s mm
160   ext. window casing,1x%d-16ft+,%dx18-4800mm+
161   ext. window casing,1x%d ir=%s,%dx18 ir=%s
163   ext. window lintel,1x%d-16ft+,%dx18-4800mm+
164   ext. window lintel,1x%d ir=%s,%dx18 ir=%s
166   exterior plinth,%s" w,%smm w
167   exterior base plinth,%s" w,%smm w
170   ext. door casing,1x%d-16ft+,%dx18-4800mm+
171   ext. door casing,1x%d ir=%s,%dx18 ir=%s
173   ext. door lintel,1x%d-16ft+,%dx18-4800mm+
174   ext. door lintel,1x%d ir=%s,%dx18 ir=%s
176   ext. door plinth,%s" w,%smm w
177   ext. door base plinth,%s" w,%smm w
180   garage door casing,1x%d-16ft+,%dx18-4800mm+
181   garage door casing,1x%d ir=%s,%dx18 ir=%s
183   garage door lintel,1x%d-16ft+,%dx18-4800mm+
184   garage door lintel,1x%d ir=%s,%dx18 ir=%s
190   ext. door jamb,%d in,%d mm
191   ext. door jamb,%d in ir=%s,%d mm ir=%s
200   garage door jamb,%d in,%d mm
201   garage door jamb,%d in ir=%s,%d mm ir=%s
260   corner board,%sx%s in (2),%sx%s mm (2)

ITEM
FL   Flooring
5
5     carpet pad
7     underlayment,4x8' sheets,1200x2400mm sheets
9     mortar (tile)
10    tile underlayment
21    wire mesh (tile)

ITEM
WB   Wall Board
3
10   wall board,4x8'-1/2",1200x2400x12mm
30   1hr wall board,4x8'-5/8",1200x2400x16mm
50   wp wall board,4x8'-1/2",1200x2400x12mm

ITEM
IN    Insulation
6
10   wall insulation,4x%sx93" batts,100x%sx2400 batts
20   wall insulation,6x%sx93" batts,150x%sx2400 batts
80   wall insulation,4x16" roll,100x450mm roll
90   wall insulation,6x16" roll,150x450mm roll
140  ceiling insulation,%sx48" batts,%sx1200mm batts
160  roof insulation,%sx48" batts,%smmx1200 batts

ITEM
T     Int. Trim
36
20   interior jamb,%d in,%d mm
25   interior jamb,%d in ir=%s,%d mm ir=%s
30   interior casing,1x%d-16ft+,%dx18-4800mm+
31   interior casing,1x%d ir=%s,%dx18 ir=%s
33   interior lintel,1x%d-16ft+,%dx18-4800mm+
34   interior lintel,1x%d ir=%s,%dx18 ir=%s
36   interior plinth,%s" w,%smm w
37   interior base plinth,%s" w,%smm w
40   sill,1x%d-16ft+,%dx18-4800mm+
45   vertical mull trim,"1x%d-16ft+",%dx18-4800mm+
46   horiz. mull trim,"1x%d-16ft+",%dx18-4800mm+
50   window apron,1x%d-16ft+,%dx18-4800mm+
60   between window trim,"1x%d-16ft+",%dx18-4800mm+
110  base moulding,1x%d-16ft+,%dx18-4800mm+
120  chair rail,1x%d-16ft+,%dx18-4800mm+
130  crown moulding,1x%d-16ft+,%dx18-4800mm+
41   int. railing,%s" wide,%smm wide
42   int. rail cap,%s" wide,%smm wide
51   middle rail
61   railing shoe
71   beam over rail,4x8 in,100x200mm
121  support post,%s" square,%smm square
122  support post,%s" diam.,%smm diam.
131  newel post,%s" square,%smm square
132  newel post,%s" diam.,%smm diam.
141  half support post,%s" square,%smm square
142  half support post,%s" diam.,%smm diam.
151  half newel post,%s" square,%smm square
152  half newel post,%s" diam.,%smm diam.
181  baluster,%s" diam.,%smm diam.
206  stair tread,%sx%s-%s",%sx%s-%smm
216  riser,%sx%s",%sx%smm
226  landing joists - fir,2x10",150x38mm
236  landing rim trim,1x8",200x19mm
246  landing floor
266  stair stringer,%d treads

ITEM
H    Hardware
16
200   cab drawer handle
201   kit. cab drawer handle
202   bath cab drawer handle
204   utility cab drawer handle
210   cab door handle
211   kit. cab door handle
212   bath cab door handle
214   utility cab door handle
220   cab drawer glide
221   kit. cab drawer glide
222   bath cab drawer glide
224   utility cab drawer glide
230   cab door hinge
231   kit. cab door hinge
232   bath cab door hinge
234   utility cab door hinge

ITEM
C     Cabinets
28
100   cab. drawer,%sx%s",%sx%smm
101   kit. cab. drawer,%sx%s",%sx%smm
102   bath cab. drawer,%sx%s",%sx%smm
104   utility cab. drawer,%sx%s",%sx%smm
120   cab. door,%sx%s",%sx%smm
121   kit. cab. door,%sx%s",%sx%smm
122   bath cab. door,%sx%s",%sx%smm
124   utility cab. door,%sx%s",%sx%smm
130   %s door,%sx%s",%sx%smm
131   %s door (kit),%sx%s",%sx%smm
132   %s door (bath),%sx%s",%sx%smm
134   %s door (utility),%sx%s",%sx%smm
140   counter top
150   counter top front cap
151   front cap (kit.)
152   front cap (bath)
154   front cap (utility)
160   backsplash
161   backsplash (kit.)
162   backsplash (bath)
164   backsplash (utility)
166   backsplash
167   backsplash (kit.)
168   backsplash (bath)
169   backsplash (utility)
170   full backsplash 
171   full backsplash (kit.)
172   full backsplash (bath)
174   full backsplash (utility)


ITEM
DW    Decks-Walks
23
210   deck joists - fir,2x8",200x38mm UNUSED
110   redwood deck planks,2x4-16ft+,100x35-4800mm+
120   redwood deck planks,2x6-16ft+,150x35-4800mm+
41    ext. railing,%s" wide,%smm wide
42    ext. rail cap,%s" wide,%smm wide
51    middle rail
61    railing shoe
71    beam over rail,4x8 in,100x200mm
121   support post,%s" square,%smm square
122   support post,%s" diam.,%smm diam.
131   rail post,%s" square,%smm square
132   rail post,%s" diam.,%smm diam.
141   half support post,%s" square,%smm square
142   half support post,%s" diam.,%smm diam.
151   half rail post,%s" square,%smm square
152   half rail post,%s" diam.,%smm diam.
181   baluster,%s" diam.,%smm diam.
206   ext. stair tread,%sx%s-%s",%sx%s-%smm
216   ext. riser,%sx%s",%sx%s-%smm
226   landing joists - fir,2x8",150x38mm
236   rdwd deck rim,2x10",250x19mm
246   landing flooring
266   stair stringer,%d treads


