First enter the line a, by clicking on the control panel of the IBIS on the "line / course" button. To enter the line 5 digits are reserved.

The first three digits correspond to the known line number, for example 076 for line 76. In buses with matrix display the last two digits of the code number match a line-additive, for example, N for night - or X for express lines. If 00 is set, there is no addition.

Please set line 76 by ​​typing 07600.

Confirm your input by pressing the appropriate button on the control panel.