;; aaaPci.inf
;; Copyright (C) ShareBit 2008-2011, all rights are reserved

;--------- Version Section ---------------------------------------------------

[Version]
Signature="$CHICAGO$"

Class=LonSe
ClassGUID={F27B103F-1F86-4548-9F98-39D43472A655}
Provider=%ProviderName%
DriverVer= 12/12/2011,3.0.0.0

;--------- SourceDiskNames and SourceDiskFiles Section -----------------------

[SourceDisksNames]
1 = "ShareBit PCI device driver Disk",,,

[SourceDisksFiles]
aaaPci.sys = 1

;--------- ClassInstall/ClassInstall32 Section -------------------------------

; Not necessary if using a standard class

; 9X Style
[ClassInstall]
Addreg=Class_AddReg

; NT Style
[ClassInstall32]
Addreg=Class_AddReg

[Class_AddReg]
HKR,,,,%DeviceClassName%
HKR,,Icon,,"-1"

;--------- DestinationDirs Section -------------------------------------------

[DestinationDirs]
CaaaPci_Files_Driver = 10,System32\Drivers

;--------- Manufacturer and Models Sections ----------------------------------

[Manufacturer]
%MfgName%=Mfg0

[Mfg0]

; PCI hardware IDs use the form
;
%Device6801Desc%=CaaaPci_DDI, PCI\VEN_1797&DEV_6801
%Device6802Desc%=CaaaPci_DDI, PCI\VEN_1797&DEV_6802
%Device6804Desc%=CaaaPci_DDI, PCI\VEN_1797&DEV_6804
%Device6805Desc%=CaaaPci_DDI, PCI\VEN_1797&DEV_6805
%Device6810Desc%=CaaaPci_DDI, PCI\VEN_1797&DEV_6810
%Device6811Desc%=CaaaPci_DDI, PCI\VEN_1797&DEV_6811
%Device6812Desc%=CaaaPci_DDI, PCI\VEN_1797&DEV_6812
%Device6813Desc%=CaaaPci_DDI, PCI\VEN_1797&DEV_6813
%Device6814Desc%=CaaaPci_DDI, PCI\VEN_1797&DEV_6814
%Device6815Desc%=CaaaPci_DDI, PCI\VEN_1797&DEV_6815
%Device6816Desc%=CaaaPci_DDI, PCI\VEN_1797&DEV_6816
%Device6817Desc%=CaaaPci_DDI, PCI\VEN_1797&DEV_6817
%Device6864Desc%=CaaaPci_DDI, PCI\VEN_1797&DEV_6864
%Device6869Desc%=CaaaPci_DDI, PCI\VEN_1797&DEV_6869
%Device7130Desc%=CaaaPci_DDI, PCI\VEN_1131&DEV_7130
%Device7134Desc%=CaaaPci_DDI, PCI\VEN_1131&DEV_7134

;---------- DDInstall Sections -----------------------------------------------
; --------- Windows 9X -----------------

; Experimentation has shown that DDInstall root names greater than 19 characters
; cause problems in Windows 98

[CaaaPci_DDI]
CopyFiles=CaaaPci_Files_Driver
AddReg=CaaaPci_9X_AddReg

[CaaaPci_9X_AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,aaaPci.sys
; --------- Windows NT -----------------

[CaaaPci_DDI.NT]
CopyFiles=CaaaPci_Files_Driver

[CaaaPci_DDI.NT.Services]
Addservice = CaaaPci, 0x00000002, CaaaPci_AddService

[CaaaPci_AddService]
DisplayName    = %SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\aaaPci.sys



; --------- Files (common) -------------

[CaaaPci_Files_Driver]
aaaPci.sys

;--------- Strings Section ---------------------------------------------------

[Strings]
ProviderName="LonSe"
MfgName="LonSe"
Device6801Desc="LonSe-6802 Video"
Device6802Desc="LonSe-6802 Audio"
Device6804Desc="LonSe-6805 Video"
Device6805Desc="LonSe-6805 Audio"
Device6810Desc="LonSe-6816 Video"
Device6811Desc="LonSe-6816 Video"
Device6812Desc="LonSe-6816 Video"
Device6813Desc="LonSe-6816 Video"
Device6814Desc="LonSe-6816 Audio"
Device6815Desc="LonSe-6816 Audio"
Device6816Desc="LonSe-6816 Audio"
Device6817Desc="LonSe-6816 Audio"
Device6864Desc="LonSe-6864 Capture"
Device6869Desc="LonSe-6869 Capture"
Device7130Desc="LonSe-7130 Video"
Device7134Desc="LonSe-7134 Capture"
DeviceClassName="LonSe"
SvcDesc="LonSe PCI device"
